SGI Digital Video Specification

October 1, 1993

Copyright 1993 Silicon Graphics, Inc. All Rights Reserved This document contains proprietary and confidential information of Silicon Graphics, Inc., and is protected by Federal copyright law.

The contents of this document may not be copied nor duplicated in any form, in whole or in part, without the express written consent of Silicon Graphics, Inc. U.S. Government Limited Rights Use, duplication, or disclosure of the technical data contained in this document is subject to restrictions as set forth by the Government in subdivision (b)(2) of the Rights in Technical Data and Computer Software clause at 52.227-7013. Contractor/manufacturer is Silicon Graphics, Inc., 2011 North Shoreline Road, Mountain View, CA 94039-7311.

Send corrections to this document via FAX to: (415) 967-6239

SGI Digital Video Specification October 1, 1993 1

SGI Digital Video

Specification

This document defines the electrical specifications of the SGI Digital Video standard and the mechanical interface to the digital video port. This interface is used for transporting digital video information either into or out of Silicon Graphics machines. There are currently two implementations of this interface - an input only implementation as used by the IndyCam digital camera on the Indy workstation, and an input/output implementation as found on the Galileo, Indy Video, Indigo^2 video add-in products and the upcoming Cosmo Compress Motion JPEG compression card. This specification covers both of these variations.

General Description

SGI Digital Video provides an interface for moving digital video information into and/or out of a Silicon Graphics workstation. The full implementation provides two digital ports - one, an input only port, and the other capable of either input or output (but not simultaneously). The interface also provides an I^2C interface for controlling external devices. The IndyCam port on the Indy workstation only provides the ability to input digital video data. Figure 1 shows a diagram of the interface.

Figure 1 SGI Digital Video Interface

2 October 1, 1993 SGI Digital Video Specification

SGI Digital Video Signals CONFIDENTIAL

The SGI Digital Video interface is nearly identical to that specified in the definition of the CCIR 601 Digital Video Specification. There are two differences between the CCIR 601 interface and the Digital Video Port. The first exception is that the data lines in the SGI Digital Video interface are implemented as single-ended TTL level signals rather than differential ECL signals. The second exception is that not all of the systems or products with SGI Digital Video connections support pixel sampling at 13.5 MHz as specified by CCIR 601. These systems may only be capable of supporting square pixel sampling. This is discussed more completely in Digital Video Sampling on page 6. Mechanically the connection to SGI Digital Video port is made via a 60 pin high density connector. This connector may be included as part of the workstation system (Indy, for example) or may be included as part of an add-in option board (Galileo, for example).

SGI Digital Video Signals

The SGI Digital Video interface consists of two 8 bit (per component) video ports and associated clocks, a signal that defines the direction of data for the bidirectional port, trigger in and trigger out signals, and data and clock signals for the I^2C interface bus. Table 1 shows a listing of these signal groups. A definition of each of the signals follows.

XDATAIO.[0-7]: These 8 data lines contain the video data that is either going into, or coming out of the Silicon Graphics Video port. For each of the signals there is a corresponding return line with the suffix “_RET”. The signal and it’s return line should be implemented as coax pairs to minimize interference. Data on these lines are at TTL levels. Signal XDATAIO.7 is the Most Significant Bit.

SPARE[AB]IO: These two signals are intended for future expansion. They are currently unused. They should not be used for the present time, but for forward compatibility, cables should include these connections. Each of the signals has a corresponding return line with the suffix “_RET”. SeeDigital Video Port Cable Connections for more information on the cable connections.

Table 1 SGI Digital Video Signals Signal(s) Description XDATAIO.[0-7] Bidirectional Port Video Data Lines SPARE[AB]IO Additional I/O Data Lines (reserved)

XCLKIO Bidirectional Port Clock DIR_SEND/_REC Bidirectional Port Direction

XDATAIN.[0-7] Input Port Video Data Lines SPARE[AB]IN Additional Input Data Lines (reserved)

XCLKIN Input Port Clock TRIGIN Trigger Input TRIGOUT Trigger Output SDA_SEND/_REC I^2C Data SCL_SEND/_REC I^2C Clock +12V_SEND/_REC + 12 Volt output/input +5V_SEND/_REC + 5 Volt output/input -12V_SEND/_REC - 12 Volt output/input

SGI Digital Video Specification October 1, 1993 3

CONFIDENTIAL SGI Digital Video Signals

XCLKIO: This signal is used to clock in (or out) the data on the bidirectional port. Depending on the state of the DIR signal, the clock should be provided by the external device in the case of input, or is provided by the system in the case of output. This clock signal has it’s own return line, XCLKIO_RET.

DIR_SEND/_REC: DIR_SEND is an output signal from the port defining the direction of data for the bidirectional port. When this signal is 0 the port is an input port. When it is 1, the port is configured as an output port. DIR_REC is the signal connection used to receive the DIR_SEND signal at an external device. This signal default state is “0”, or input. XDATAIN.[0-7]: These 8 data lines contain the video data that is going into the input port. This port does not support data output. As with the XDATAIO signals, each of these signals has its corresponding return line, denoted by the “_RET” suffix. Signal XDATAIN.7 is the Most Significant Bit.

SPARE[AB]IN: These two signals are intended for future expansion. They are currently unused. They should not be used for the present time, but for forward compatibility, cables should include these connections. Each of the signals has a corresponding return line with the suffix “_RET”. SeeDigital Video Port Cable Connections for more information on the cable connections.

XCLKIN: This signal is used to clock data into the input port. This clock signal has it’s own return line, XCLKIN_RET. TRIGIN: This input signal is polled by the CPU and can be used to signal an event or trigger some action on the part of the system. The signal is a TTL signal and is active low.

TRIGOUT: This output signal can be used to trigger an external device to take some action. It is a TTL level signal and is active low.

SDA_SEND/_REC: This is the data for the I^2C bus. The SDA_REC connection should be used at the external device for connecting to the SDA_SEND signal. See Digital Video Port Cable Connections for more information. SCL_SEND/_REC: This is the clock for the I^2C bus. The SCL_REC connection should be used at the external device for connecting to the SCL_SEND signal. See Digital Video Port Cable Connections for more information. +12V_SEND/_REC: This is a +12 Volt supply used for the IndyCam. Output capacity is limited to 100 mA. This signal (and the other two supply signals) support the power requirements of the IndyCam only. This signal is not for use by any other external device.

+5V_SEND/_REC: This is a + 5 Volt supply used for the IndyCam. Output capacity is limited to 100 mA. This signal (and the other two supply signals) support the power requirements of the IndyCam only. This signal is not for use by any other external device.

-12V_SEND/_REC: This is a - 12 Volt supply used for the IndyCam. Output capacity is limited to 100 mA. This signal (and the other two supply signals) support the power requirements of the IndyCam only. This signal is not for use by any other external device.

4 October 1, 1993 SGI Digital Video Specification

SGI Digital Video - Electrical CONFIDENTIAL

SGI Digital Video - Electrical

The electrical characteristics of the SGI Digital Video signals are shown in Table 2.

Timing The XDATAIO, XCLKIO, XDATAIN and XCLKIN signals conform to the timing requirements as stated in the SMPTE Recommended Practice 125-1984. The SDA and SCL signals conform to the timing requirements as set out in the I^2C Interface specification (see the Phillips Semiconductors Desktop Video Data Handbook for this specification). The TRIGIN and TRIGOUT signals are asynchronous with respect to the other signals on this interface. The DIR signal is not meant to be a dynamic signal. It is meant purely as an indication of the direction of signal flow. This signal defaults to an input status.

Terminations The IndyCam port found on Indy and the SGI Digital Video port found on Indigo and Indigo^2 differ slightly in their termination schemes. The IndyCam port is a high impedance input suitable for a series termination of 33 Ω at the source. The SGI Digital Video port lines are terminated with a series R-C network from the line to ground. The values of the R and C are 120 Ω and 0.001 μF. If a device will only drive the IndyCam input port and not be expected to receive any data, the signals can be source-terminated by using a series resistor with a value of 33 Ω. This style of termination is designed specifically for IndyCam and is not intended for long (> 4 feet) cables. However, if the device is expected to both send and receive data, then the lines should use the series R-C termination scheme as mentioned above.

Table 2 SGI Digital Video Signal Electrical Characteristics

Signal(s)

Interface Characteristics Levels Timing XDATIO.[0-9]

TTL

See SMPTE RP 125-1984 XCLKIO

DIR Static XDATIN.[0-9] See SMPTE RP 125-1984 XCLKIN TRIGIN Asynchronous TRIGOUT

SDA See the I^2C Interface Specification SCL

SGI Digital Video Specification October 1, 1993 5

CONFIDENTIAL SGI Digital Video - Electrical

Pin # Signal Name I/O

1 XDATAIO.0 I/O 2 XDATAIO.0_RET I/O 3 XDATAIO.1 I/O 4 XDATAIO.1_RET I/O 5 XDATAIO.2 I/O 6 XDATAIO.2_RET I/O 7 SDA_SEND O 8 DIR_SEND O 9 SCL_SEND O 10 TRIGIN_RET I 11 TRIGIN I 12 XCLKIN_RET I 13 XCLKIN I 14 SPAREBIN_RET I 15 SPAREBIN I 16 XDATAIO.3 I/O 17 XDATAIO.3_RET I/O 18 XDATAIO.4 I/O 19 XDATAIO.4_RET I/O 20 XDATAIO.5 I/O 21 XDATAIO.5_RET I/O 22 +12V_SEND O 23 +5V_SEND O 24 -12V_SEND O 25 SPAREAIN_RET I 26 SPAREAIN I 27 XDATAIN.7_RET I 28 XDATAIN.7 I 29 XDATAIN.6_RET I 30 XDATAIN.6 I

31 XDATAIN.3 I 32 XDATAIN.3_RET I 33 XDATAIN.4 I 34 XDATAIN.4_RET I 35 XDATAIN.5 I 36 XDATAIN.5_RET I 37 +12V_REC I 38 +5V_REC I 39 -12V_REC I 40 SPAREAIO_RET I/O 41 SPAREAIO I/O 42 XDATAIO.7_RET I/O 43 XDATAIO.7 I/O 44 XDATAIO.6_RET I/O 45 XDATAIO.6 I/O 46 XDATAIN.0 I 47 XDATAIN.0_RET I 48 XDATAIN.1 I 49 XDATAIN.1_RET I 50 XDATAIN.2 I 51 XDATAIN.2_RET I 52 SDA_REC I 53 DIR_REC I 54 SCL_REC I 55 TRIGOUT_RET O 56 TRIGOUT O 57 XCLKIO_RET I/O 58 XCLKIO I/O 59 SPAREBIO_RET I/O 60 SPAREBIO I/O

Pin # Signal Name I/O

Table 3 SGI Digital Video Connector Pin Assignments

6 October 1, 1993 SGI Digital Video Specification

SGI Digital Video Connector Pin Assignment CONFIDENTIAL

SGI Digital Video Connector Pin Assignment

Table 3 defines the pinout used for the SGI Digital Video connector. This connector is a 60 pin high density connector. It has four rows of 15 contacts each. Figure 2 shows this connector and its numbering scheme. Only those signals that are shown shaded are available at the IndyCam port. While the ninth and tenth data bits are currently not used, their pins are assigned. These signal names are shown in italics. The connector is a female Molex LFH type (Molex P/N 70928-2002) or equivalent.

Figure 2 SGI Digital Video Connector Numbering

Digital Video Sampling

CCIR Recommendation 601 regarding Digital Video states that pixel sampling will be done at 13.5 MHz. Not all the Silicon Graphics systems or options support this capability. For example, the IndyCam port on the Indy workstation supports only square pixel sampling at either 12.2727 MHz for NTSC, or 14.750 MHz for PAL. Other products, such as the Galileo product for Indigo^2, support both square pixel sampling and fully compliant 601 sampling at 13.50 MHz. In the case of products that support both sampling methods, the sampling method is determined by a software call. The table below shows the sampling method supported by each Silicon Graphics product with an SGI Digital Video port.

Table 4 Video Sampling Support CCIR 601 Sampling

Square Pixel IndyCam Input X Indy Video X Galileo for Indigo X X Galileo for Indigo^2 X X

SGI Digital Video Specification October 1, 1993 7

CONFIDENTIAL Digital Video Format Overview

Digital Video Format Overview

From a format point of view, the SGI Digital Video format is identical to CCIR 601. The data coming out or going into the SGI Digital Video port is a stream of multiplexed luminance and chrominance values plus timing information. This video is of the 4:2:2 format. Video data for any active video line follows the form:

U0Y0V0 Y1 U2Y2V2 Y3 U4Y4V4 Y5 U6Y6V6 Y7 ......UnYnVn where U0Y0V0 are co-sited spatially.

CCIR Recommendation 601 specifies that each active line of video contains 1440 samples - 720 luminance samples and 360 samples of each color-difference signal. As mentioned above, the sample rate for this method is 13.5 MHz. The number of samples per line is the same for both NTSC and PAL type systems. The difference between the two is the number of samples that are outside the active line (i.e. in the blanking area).

In systems that sample at a rate other than the 13.5 MHz required by CCIR 601, the number of total samples and the number of samples in the active and blanking periods is different. The table below shows these values.

Valid values for the luminance component are 16_{10} (black) through 235_{10} (peak white). During the blanking period the luminance values transmitted are black (16_{10}). Luminance values received during the blanking period are ignored. Valid values for the chrominance components are 16_{10} through 240_{10}. During the blanking period the chrominance values transmitted are 128_{10}. Chrominance values received during the blanking period are ignored. The beginning and end of active video information is indicated by a three byte preamble and a byte containing field, horizontal and vertical timing information. The three-byte preamble is defined as FF 00 00 (in hex). The fourth byte contains timing information. This byte can be decoded as follows:

Table 5 Sampling Rates and Samples

Sampling Method Sample Frequency

Samples (per line) Lines Total Active line Blanking Total Active CCIR 601 - NTSC 13.5 MHz 1716 1440 276 525 487 CCIR 601 - PAL 13.5 MHz 1728 1440 288 625 576 Square Pixel - NTSC 12.27 MHz 1560 1280 280 525 487 Square Pixel - PAL 14.75 MHz 1888 1536 352 625 576

Table 6 Timing Byte Definition Bit Name Meaning 7 - Always set to 1 6 F Field type - 0 = odd, 1 = even 5 V V=1 during vertical blanking, changes when H=1 (EAV) 4 H H=1 at end of active video (EAV), h=0 at beginning of video 3 P3 Hamming code error protection 2 P2 Hamming code error protection 1 P1 Hamming code error protection 0 P0 parity

8 October 1, 1993 SGI Digital Video Specification

SGI Digital Video Cable Connections CONFIDENTIAL

The following table shows the values for the Hamming Code bits and parity bit for values of F, V, and H.

This scheme protects the F, V and H bits and can correct a one bit error or detect a two bit error.

SGI Digital Video Cable Connections

Since the frequency of the multiplexed luminance and chrominance samples is 20 to 30 MHz and the density of pins on the connector is high, care needs to be taken in creating cables for connecting the SGI Digital Video port with other devices. Through our experiments, we have found that best results are obtained when using cables of 8 feet or less, with multiple 75Ω coax cables (minimum 34 AWG) bundled together surrounded by a braided shield. Twisted pair and flat ribbon cable do not work properly. For this reason, we recommend that the cable type specified in Table 8 be used. No currently available cable exists with the right combination of coaxes, braided shield and cover so custom cables are required. The cable specified in the table below is the individual coax that has been used for each signal in the prototypes we have had made. The connectors and backshells used for the cable and the connector for PCB mounting are also defined in this table.

Table 7 Hamming Code and Parity Bits Signal (Bit #) Signal (Bit #) F (6) V (5) H (4) P3 (3) P2 (2) P1 (1) P0 (0) 0 0 0 0 0 0 0 0 0 1 1 1 0 1 0 1 0 1 0 1 1 0 1 1 0 1 1 0 1 0 0 0 1 1 1 1 0 1 1 0 1 0 1 1 0 1 1 0 0 1 1 1 0 0 0 1

Table 8: Digital Video Cable Components Manufacturer Description Part Number Tensolite Coax Cable, 75Ω 32453/50275X-1(LD) Molex Connector, Male, Straight, 60 pin 70929-1001 Molex Backshell 82007-0131 Molex Connector, Female, Right Angle, 60 pin 70928-2002

SGI Digital Video Specification October 1, 1993 9

CONFIDENTIAL SGI Digital Video Cable Connections

Also important to the quality of the cable is the quality of the cable shields and their connection to the backshells. The shields should be connected to the backshell at both ends of the cable such that the connector housing of the SGI Digital Video port on the platform and the connector housing at the external device are connected by a low impedance path. This will result in lower EMI emissions and less probability that the signals in the cable will be efected by external equipment. The SGI Digital Video port pinout has been defined so that cables for connecting the port with external devices can be made where there is no difference between the pin configuration at each end. This could be considered a “Null Modem” style cable. In other words, the cable ends can be swapped with no effect on function. An example of this kind of cable is shown in Figure 3. The wiring list for the cable shown in Figure 3 is shown in Table 9.

Figure 3 SGI Digital Video Cable

10 October 1, 1993 SGI Digital Video Specification

SGI Digital Video Cable Connections CONFIDENTIAL

From To Pin Signal Pin Signal 1 XDATAIO.0 46 XDATAIN.0 2 XDATAIO.0_RET 47 XDATAIN.0_RET 3 XDATAIO.1 48 XDATAIN.1 4 XDATAIO.1_RET 49 XDATAIN.1_RET 5 XDATAIO.2 50 XDATAIN.2 6 XDATAIO.2_RET 51 XDATAIN.2_RET 7 SDA_SEND 52 SDA_REC 8 DIR_SEND 53 DIR_REC 9 SCL_SEND 54 SCL_REC 10 TRIGIN_RET 55 TRIGOUT_RET 11 TRIGIN 56 TRIGOUT 12 XCLKIN_RET 57 XCLKIO_RET 13 XCLKIN 58 XCLKIO 14 SPAREBIN_RET 59 SPAREBIO_RET 15 SPAREBIN 60 SPAREBIO 16 XDATAIO.3 31 XDATAIN.3 17 XDATAIO.3_RET 32 XDATAIN.3_RET 18 XDATAIO.4 33 XDATAIN.4 19 XDATAIO.4_RET 34 XDATAIN.4_RET 20 XDATAIO.5 35 XDATAIN.5 21 XDATAIO.5_RET 36 XDATAIN.5_RET 22 +12V_SEND - NC 23 +5V_SEND - NC 24 -12V_SEND - NC 25 SPAREAIN_RET 40 SPAREAIO_RET 26 SPAREAIN 41 SPAREAIO 27 XDATAIN.7_RET 42 XDATAIO.7_RET 28 XDATAIN.7 43 XDATAIO.7 29 XDATAIN.6_RET 44 XDATAIO.6_RET 30 XDATAIN.6 45 XDATAIO.6

31 XDATAIN.3 16 XDATAIO.3 32 XDATAIN.3_RET 17 XDATAIO.3_RET 33 XDATAIN.4 18 XDATAIO.4 34 XDATAIN.4_RET 19 XDATAIO.4_RET 35 XDATAIN.5 20 XDATAIO.5 36 XDATAIN.5_RET 21 XDATAIO.5_RET 37 +12V_REC - NC 38 +5V_REC - NC 39 -12V_REC - NC 40 SPAREAIO_RET 25 SPAREAIN_RET 41 SPAREAIO 26 SPAREAIN 42 XDATAIO.7_RET 27 XDATAIN.7_RET 43 XDATAIO.7 28 XDATAIN.7 44 XDATAIO.6_RET 29 XDATAIN.6_RET 45 XDATAIO.6 30 XDATAIN.6 46 XDATAIN.0 1 XDATAIO.0 47 XDATAIN.0_RET 2 XDATAIO.0_RET 48 XDATAIN.1 3 XDATAIO.1 49 XDATAIN.1_RET 4 XDATAIO.1_RET 50 XDATAIN.2 5 XDATAIO.2 51 XDATAIN.2_RET 6 XDATAIO.2_RET 52 SDA_REC 7 SDA_SEND 53 DIR_REC 8 DIR_SEND 54 SCL_REC 9 SCL_SEND 55 TRIGOUT_RET 10 TRIGIN_RET 56 TRIGOUT 11 TRIGIN 57 XCLKIO_RET 12 XCLKIN_RET 58 XCLKIO 13 XCLKIN 59 SPAREBIO_RET 14 SPAREBIN_RET 60 SPAREBIO 15 SPAREBIN

From To Pin Signal Pin Signal

Table 9: SGI Digital Video Cable Wiring List

SGI Digital Video Specification October 1, 1993 11

CONFIDENTIAL I2C Interface

I2C Interface

I^2C is a very simple serial control protocol, developed by Phillips, that has found application in the SGI digital video standard. It is composed of two wires, a data line and a clock line.

A number of devices can share the bus typically with one master and a number of slaves. The protocol is described in detail in Phillips Semiconductors Desktop Video Data Handbook, but here are the basics of a simple interaction:

• When inactive, both the clock and data lines are pulled high by pull-up resistors in the system. • An interaction is initiated by the master by transmitting a one byte word representing a slave station address. The LSB of this station address indicates if this device is to be written to or read from (0 for write, 1 for read) • A start condition, at the beginning of a transaction, is indicated by the data line being pulled low before the clock goes low.

• Conversely, a stop condition is indicated by the data line being released high by the master after the clock is already high.

• A slave device acknowledges its own address by pulling the data bus low. At this point the master transmits a station sub-address, also a byte long, indicating which register in the device is to be accessed. Once again the slave pulls the bus low in acknowledgment.

• Finally the last 1 byte long word is the data that is being either received or transmitted. It is imperative for there to be no duplicate station addresses for this scheme to work. Table10 is a listing of I^2C devices and their station addresses to preclude this possibility. Addresses used in SGI products are noted in the table. An SGI workstation may internally have a SAA7191 decoder, an SAA7199 encoder or a SAA7192 colorspace converter. Which parts are present depend on the product. These addresses should NOT be used. The IndyCam has a station address of 0x56. This address should also be avoided.

12 October 1, 1993 SGI Digital Video Specification

I2C Interface CONFIDENTIAL

Table 10: Assigned I^2C Bus Addresses

Manufacturer Part Number Description I^2C Address(es)*

Signetics

PCD3311/12 Tone generator DTMF/modem/musical 0x40 & 0x4A PCF8200 Voice synthesizer (male or female) 0x20 PCF8566 96-segment LCD driver 1:1 - 1:4 Mux 0x7C & 0x7D PCF8568 LCD row driver for dot matrix displays 0x78 & 0x7A PCF8569 Column driver for dot matrix displays 0x78 & 0x7A PCF8570/71 256 x 8, 128 x 8 static RAM 0xA0 - 0xAE PCF8570C 256 x 8 static RAM 0xB0 - 0xBE PCF8573 Clock/calendar 0xD0 - 0xD6

Phillips

PCF8574 I^2C bus to 8-bit bus converter 0x40^† - 0x4E PCF8574A I^2C bus to 8-bit bus converter 0x70 - 0x7E

Signetics

PCF8576 160-segment LCD driver 1:1 - 1:4 Mux 0x70 & 0x72 PCF8577 64-segment LCD driver 1:1 - 1:2 Mux 0x74 PCF8577A 64-segment LCD driver 1:1 - 1:2 Mux 0x76 PCF8578 Row/column LCD dot-matrix driver 0x78 & 0x7A PCF8579 Row/column LCD dot-matrix driver 0x78 & 0x7A PCF8581 128-byte EEPROM 0xA0 - 0xAE PCF8582 256 x 8 EEPROM 0xA0 - 0xAE PCF8583 256 x 8 RAM with clock/calendar 0xA0 & 0xA2 PCF8591 4-channel, 8-bit A/D plus 8-bit D/A 0x90 - 0x9E PCF8594 512-byte EEPROM 0xA0 - 0xAE SAA1064 4-digit LED driver 0x70 - 0x76 SAA1136 PCM-audio indent-word interface 0x3C SAA1300 5-bit high current driver 0x40 - 0x46 SAA5243/45 Enhanced teletext circuit 0x22

Phillips

SAA5252 Closed caption decoder 0x28 & 0x29 SAA7151B Digital multi-standard color decoder with SCART interface

0x8A & 0x8E^†

SAA7152 Digital combination filter 0xB2 SAA7194(7196) Digital video decoder and scaler circuit (DESC) 0x40 & 0x42 SAA7191B S-VHS digital multi-standard decoder “square pixel” 0x8A^† & 0x8E SAA7192A Digital color space converter 0xE0^† & 0xE2 SAA7199 Digital encoder 0xB0^† Signetics SAA9020 Field memory controller 0x28 - 0x2E Phillips SAA9051 DIgital multi-standard TV decoder 0x8A

Signetics

SAA9068 (PIPCO) Picture-in-picture controller 0x24 & 0x26 SAB3035/36/37 (CITAC) CPU interface for tuning and control 0xC0 - 0xC6 SAF1135 Data line decoder 0x20 - 0x26

SGI Digital Video Specification October 1, 1993 13

CONFIDENTIAL Bibliography

* Addresses specified are in the write mode. † This is address used in Silicon Graphics video products

Bibliography

International Telecommunications Union, CCIR Recommendation 601-2 - Encoding Parameters of Digital Television for Studios [Contained in: Recommendations of the CCIR, 1990 Volume XI-Part 1 Broadcasting Service (Television) (page 95)], 1990, International Telecommunications Union

Available from: National Technical Information Service 5285 Port Royal Road Springfield, Virginia 22161 (703) 487-4600 Also found in: Desktop Video Data Handbook (pages 2-29 through 2-38) [see below] North American Phillips Corporation, I^2C-bus Specification [Contained in: Desktop Video Data Handbook (pages 2-185 through 2-204)], 1993, North American Phillips Corporation Society of Motion Picture and Television Engineers, SMPTE 125M - Television - Component Video Signal 4:2:2 - Bit Parallel Digital Interface

Available from: Society of Motion Picture and Television Engineers 595 W. Hartsdale Avenue White Plains, New York 10607 (914) 761-1100

Phillips

TDA4670 Picture signal improvement circuit 0x88 TDA4680/4686 Video processor 0x88 Signetics TDA8421 Phillips TDA8440 Switch for CTV receivers 0x90 - 0x9E TDA8442 Interface for color decoders 0x88 TDA8443 YUV/RGB interface circuit 0xD0 - 0xDE TDA8444 Octuple 6-bit DAC 0x40 - 0x4E (0x48^†) Signetics TDA8461 PAL/NTSC color decoder 0x80 & 0x8A Phillips TDA9141 PAL/NTSC/SECAM decoder/sync processor 0x8A & 0x8E Signetics TEA6100 FM/IF and tuning interface 0xC2 TEA6300/6310T Sound fader control circuit 0x80 TSA5511/12/14 PLL frequency synthesizer for TV 0xC0 - 0xC6 TSA6057 Radio tuning PLL frequency synthesizer 0xC4 - 0xC6 UMF1009 Frequency synthesizer 0xC0 - oxC6 SGI - IndyCam 0x56^†

Table 10: Assigned I^2C Bus Addresses

Manufacturer Part Number Description I^2C Address(es)*

14 October 1, 1993 SGI Digital Video Specification

Bibliography CONFIDENTIAL