UPDATING.

Automatically,
Pull down the "Update," menu and select "ON," or
"OFF." Also in this menu is the time interval between
updates. You can change the time delay simply by
selecting the new time period you require. While
auto-updating is turned on you should see the
"CAT system," light on your rig flash on and off.

Manually,
Chose the update level you require by selecting the
new level from the menu, either FULL update, the
current Display or both VFOs. Then just click on the
word "UPDATE," bottom  lefthand corner of the main
display. This will force the transceiver to  send
it's data block to the stack.

METER,
Selecting "ON," will display the current meter
setting. When receiving this will be the receive
signal level while in transmit this will depend on
the setting of the METER switch on the front of your
rig.

Display Brightness,
Selecting one of the settings will change the
brightness of the rig's display, Bright, Medium
or Dim.