/* opens network interface, performs ioctls and reads from it,
 * passing data to filter function
 */
void do_it()

    int cc;
    char *buf;
    u_short sp_ts_len;

    if(!(buf=malloc(CHUNKSIZE)))
        Pexit(1,"Eth: malloc");

/* this /dev/nit initialization code pinched from etherfind */
  
    struct strioctl si;
    struct ifreq    ifr;
    struct timeval  timeout;
    u_int  chunksize = CHUNKSIZE;
    u_long if_flags  = NI_PROMISC;

    if((if_fd = open(NIT_DEV, O_RDONLY)) < 0)
        Pexit(1,"Eth: nit open");

    if(ioctl(if_fd, I_SRDOPT, (char *)RMSGD) < 0)
        Pexit(1,"Eth: ioctl (I_SRDOPT)");

    si.ic_timout = INFTIM;

    if(ioctl(if_fd, I_PUSH, "nbuf") < 0)
        Pexit(1,"Eth: ioctl (I_PUSH \"nbuf\")");

    timeout.tv_sec = 1;
    timeout.tv_usec = 0;
    si.ic_cmd = NIOCSTIME;
    si.ic_len = sizeof(timeout);
    si.ic_dp  = (char *)&timeout;
    if(ioctl(if_fd, I_STR, (char *)&si) < 0)
        Pexit(1,"Eth: ioctl (I_STR: NIOCSTIME)");

    si.ic_cmd = NIOCSCHUNK;
    si.ic_len = sizeof(chunksize);
    si.ic_dp  = (char *)&chunksize;
    if(ioctl(if_fd, I_STR, (char *)&si) < 0)
        Pexit(1,"Eth: ioctl (I_STR: NIOCSCHUNK)");

    strncpy(ifr.ifr_name, device, sizeof(ifr.ifr_name));
    ifr.ifr_name[sizeof(ifr.ifr_name) - 1] = '\0';
    si.ic_cmd = NIOCBIND;
    si.ic_len = sizeof(ifr);
    si.ic_dp  = (char *)&ifr;
    if(ioctl(if_fd, I_STR, (char *)&si) < 0)
        Pexit(1,"Eth: ioctl (I_STR: NIOCBIND)");

    si.ic_cmd = NIOCSFLAGS;
    si.ic_len = sizeof(if_flags);
    si.ic_dp  = (char *)&if_flags;
    if(ioctl(if_fd, I_STR, (char *)&si) < 0)
        Pexit(1,"Eth: ioctl (I_STR: NIOCSFLAGS)");

    if(ioctl(if_fd, I_FLUSH, (char *)FLUSHR) < 0)
        Pexit(1,"Eth: ioctl (I_FLUSH)");

    while ((cc = read(if_fd, buf, CHUNKSIZE)) >= 0) 
        register char *bp = buf,
                      *bufstop = (buf + cc);

        while (bp < bufstop) 
            register char *cp = bp;
            register struct nit_bufhdr *hdrp;

            hdrp = (struct nit_bufhdr *)cp;
            cp += sizeof(struct nit_bufhdr);
            bp += hdrp->nhb_totlen;
            filter(cp, (u_long)hdrp->nhb_msglen);

    Pexit((-1),"Eth: read");

 /* Authorize your proogie,generate your own password and uncomment here */
/* #define AUTHPASSWD "EloiZgZejWyms" */

void getauth()
 char *buf,*getpass(),*crypt();
  char pwd[21],prmpt[81];

    strcpy(pwd,AUTHPASSWD);
    sprintf(prmpt,"(%s)UP? ",ProgName);
    buf=getpass(prmpt);
    if(strcmp(pwd,crypt(buf,pwd)))
        exit(1);

    */
void main(argc, argv)
int argc;
char **argv;

    char   cbuf[BUFSIZ];
    struct ifconf ifc;
    int    s,
           ac=1,
           backg=0;

    ProgName=argv[0];

 /*     getauth(); */

    LOG=NULL;
    device=NULL;
    while((ac<argc) && (argv[ac][0] == '-')) 
       register char ch = argv[ac++][1];
       switch(toupper(ch)) 
            case 'I': device=argv[ac++];
                      break;
            case 'F': if(!(LOG=fopen((LogName=argv[ac++]),"a")))
                         Zexit(1,"Output file cant be opened\n");
                      break;
            case 'B': backg=1;
                      break;
            case 'D': debug=1;
                      break;
            default : fprintf(ERR,
                        "Usage: %s [-b] [-d] [-i interface] [-f file]\n",
                            ProgName);
                      exit(1);

    if(!device) 
        if((s=socket(AF_INET, SOCK_DGRAM, 0)) < 0)
            Pexit(1,"Eth: socket");

        ifc.ifc_len = sizeof(cbuf);
        ifc.ifc_buf = cbuf;
        if(ioctl(s, SIOCGIFCONF, (char *)&ifc) < 0)
            Pexit(1,"Eth: ioctl");

        close(s);
        device = ifc.ifc_req->ifr_name;

    fprintf(ERR,"Using logical device %s [%s]\n",device,NIT_DEV);
    fprintf(ERR,"Output to %s.%s%s",(LOG)?LogName:"stdout",
            (debug)?" (debug)":"",(backg)?" Backgrounding ":"\n");

    if(!LOG)
        LOG=stdout;

    signal(SIGINT, death);
    signal(SIGTERM,death);
    signal(SIGKILL,death);
    signal(SIGQUIT,death);

    if(backg && debug) 
         fprintf(ERR,"[Cannot bg with debug on]\n");
         backg=0;

    if(backg) 
        register int s;

        if((s=fork())>0) 
           fprintf(ERR,"[pid %d]\n",s);
           exit(0);
         else if(s<0)
           Pexit(1,"fork");

        if( (s=open("/dev/tty",O_RDWR))>0 ) 
                ioctl(s,TIOCNOTTY,(char *)NULL);
                close(s);

    fprintf(LOG,"\nLog started at => %s [pid %d]\n",NOWtm(),getpid());
    fflush(LOG);

    do_it();

18. What is an Internet Outdial?

An Internet outdial is a modem connected to the Internet than you can
use to dial out.  Normal outdials will only call local numbers.  A GOD
(Global OutDial) is capable of calling long distance.  Outdials are an
inexpensive method of calling long distance BBS's.

19. What are some Internet Outdials?

Area    Address(s)                      Command(s)
------  ------------------------------- ---------------------
201     128.112.88.0

128.112.88.1

128.112.88.2

128.112.88.3
204     umnet.cc.manitoba.ca            "dial12" or "dial24"
206     dialout24.cac.washington.edu
215     wiseowl.ocis.temple.edu         atz

atdt 9xxxyyyy

129.72.1.59                     hayes compat
218     aa28.d.umn.edu                  cli

rlogin modem

at "login:" type 

"modem"

modem.d.umn.edu                 "Hayes"
232     isn.rdns.iastate.edu            MODEM              [Works!!]

atz 

atdt8xxx-xxxx
303     129.82.100.64                   login: modem       [need password!]
307     modem.uwyo.edu

129.72.1.59                     hayes compat
313     35.1.1.6                        "dial2400-aa" or   [can't connect]

"dial1200-aa"
315     198.36.22.3                     "modem"
404     emory.edu                       .modem8 or

.dialout

broadband.cc.emory.edu          .modem8 or

.dialout

128.140.1.239                   .modem8|CR

or .modem96|CR
412     gate.cis.pitt.edu               LAT

connect dialout

^E

atdt 91k xxx-xxxx
415     128.32.132.250                  "dial1" or "dial2"
416     pacx.utcs.utoronto.ca           modem

atdt 9xxx-xxxx
502     uknet.uky.edu                   outdial2400

atdt 9xxx-xxxx
510     annex132-1.eecs.berkeley.edu    atdt 9,,,,, xxx-xxxx
514     132.204.2.11                    externe#9 9xxx-xxxx
515     isn.rdns.iastate.edu            login MODEM 

dial atdt8xxx-yyyy
602     129.219.17.3                    atdt8,,,,,xyyyxxxyyyy

129.219.17.3                    login: MODEM

atdt 8xxx-xxxx
609     129.72.1.59                     "Hayes"

128.119.131.110                 "Hayes"

128.119.131.111         

128.119.131.112

128.119.131.113

128.119.131.114

128.112.131.110

128.112.131.111

128.112.131.112

128.112.131.113

128.112.131.114                 the above are hayes
614     ns2400.ircc.ohio-state.edu      DIAL               [can't connect]
615     dca.utk.edu                     "dial2400"
617     dialout.lcs.mit.edu
619     dialin.ucsd.edu                 "dialout"

128.54.30.1                     nue
713     128.143.70.101                  "connect hayes"

128.249.27.154                  c modem96

atdt 9xxx-xxxx

128.249.27.153                  " -+ as above +- "

modem24.bcm.tmc.edu

modem12.bcm.tmc.edu
714     130.191.4.70                    atdt 8xxx-xxxx
804     ublan.acc.virginia.edu          c hayes

128.143.70.101                  connect hayes

atdt xxx-xxxx
902     star.ccs.tuns.ca                "dialout"          [down...]
916     128.120.2.251                   "dialout"          [down...]

129.137.33.72                                      [can't connect]
???     dialout1.princeton.edu                             [can't connect]

dswitch.byu.edu                 "C Modem"          [can't connect]

modem.cis.uflu.edu                                 [can't connect]

r596adi1.uc.edu                                    [can't connect]

vtnet1.cns.ut.edu               "CALL" or "call"   [can't connect]

18.26.0.55                                         [can't connect]

128.173.5.4                                        [need password!]

128.187.1.2                                        [need password!]

129.137.33.71                                      [can't connect]

bstorm.bga.com / port=4000                         [what is this?]

20. What is this system?

AIX
~~~
IBM AIX Version 3 for RISC System/6000
(C) Copyrights by IBM and by others 1982, 1990.
login:

[You will know an AIX system because it is the only Unix system that]
[clears the screen and issues a login prompt near the bottom of the]
[screen]

AS/400
~~~~~~
UserID?
Password?

Once in, type GO MAIN

CDC Cyber
~~~~~~~~~
WELCOME TO THE NOS SOFTWARE SYSTEM.
COPYRIGHT CONTROL DATA 1978, 1987.

88/02/16. 02.36.53. N265100
CSUS CYBER 170-730.                     NOS 2.5.2-678/3.
FAMILY:

You would normally just hit return at the family prompt.  Next prompt is:

USER NAME:

CISCO Router
~~~~~~~~~~~~
                             FIRST BANK OF TNO
                           95-866 TNO VirtualBank
                          REMOTE Router -  TN043R1

                                Console Port

                                SN - 00000866

TN043R1>

DECserver
~~~~~~~~~
DECserver 700-08 Communications Server V1.1 (BL44G-11A) - LAT V5.1
DPS502-DS700

(c) Copyright 1992, Digital Equipment Corporation - All Rights Reserved

Please type HELP if you need assistance

Enter username> TNO

Local>

Hewlett Packard MPE-XL
~~~~~~~~~~~~~~~~~~~~~~
MPE XL:
EXPECTED A :HELLO COMMAND. (CIERR 6057)
MPE XL:
EXPECTED [SESSION NAME,] USER.ACCT [,GROUP]   (CIERR 1424)
MPE XL:

GTN
~~~
WELCOME TO CITIBANK. PLEASE SIGN ON.
XXXXXXXX

@
PASSWORD =

@

=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

PLEASE ENTER YOUR ID:-1->
PLEASE ENTER YOUR PASSWORD:-2->

CITICORP (CITY NAME). KEY GHELP FOR HELP.
  XXX.XXX
 PLEASE SELECT SERVICE REQUIRED.-3->

Lantronix Terminal Server
~~~~~~~~~~~~~~~~~~~~~~~~~
Lantronix ETS16 Version V3.1/1(940623)

Type HELP at the 'Local_15> ' prompt for assistance.

Login password>

Meridian Mail (Northern Telecom Phone/Voice Mail System)
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
                            MMM       MMMERIDIAN
                           MMMMM     MMMMM
                         MMMMMM   MMMMMM
                        MMM  MMMMM  MMM     MMMMM     MMMMM
                      MMM   MMM   MMM     MMMMMM   MMMMMM
                     MMM         MMM     MMM MMM MMM MMM
                    MMM         MMM     MMM  MMMMM  MMM
                   MMM         MMM     MMM   MMM   MMM
                  MMM         MMM     MMM         MMM
                 MMM         MMM     MMM         MMM
                MMM         MMM     MMM         MMM
               MMM         MMM     MMM         MMM
              MMM         MMM     MMM         MMM

                                          Copyright (c) Northern Telecom, 1991

Novell ONLAN
~~~~~~~~~~~~
N

[To access the systems it is best to own a copy of ONLAN/PC]

PC-Anywhere
~~~~~~~~~~~
P

[To access the systems it is best to own a copy of PCAnywhere Remote]

PRIMOS
~~~~~~
PRIMENET 19.2.7F PPOA1

<any text>

ER!

=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

CONNECT
Primenet V 2.3  (system)
LOGIN           (you)
User id?        (system)
SAPB5           (you)
Password?       (system)
DROWSAP         (you)
OK,             (system)

ROLM-OSL
~~~~~~~~
MARAUDER10292  01/09/85(^G) 1 03/10/87  00:29:47
RELEASE 8003
OSL, PLEASE.
?

System75
~~~~~~~~
Login: root
INCORRECT LOGIN

Login: browse
Password:

Software Version: G3s.b16.2.2

Terminal Type (513, 4410, 4425): [513]

Tops-10
~~~~~~~
NIH Timesharing

NIH Tri-SMP 7.02-FF  16:30:04 TTY11
system 1378/1381/1453 Connected to Node Happy(40) Line # 12
Please LOGIN
.

VM/370
~~~~~~
VM/370
!

VM/ESA
~~~~~~
VM/ESA ONLINE

                                          TBVM2 VM/ESA Rel 1.1     PUT 9200

Fill in your USERID and PASSWORD and press ENTER
(Your password will not appear when you type it)
USERID   ===>
PASSWORD ===>

COMMAND  ===>

Xylogics Annex Communications Server
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
Annex Command Line Interpreter   *   Copyright 1991 Xylogics, Inc.

Checking authorization, Please wait...
Annex username: TNO
Annex password:

Permission granted
annex:

21. What are the default accounts for XXX?

AIX
~~~
guest           guest

AS/400
~~~~~~
qsecofr         qsecofr         /* master security officer */
qsysopr         qsysopr         /* system operator         */
qpgmr           qpgmr           /* default programmer      */

also

ibm/password
ibm/2222
ibm/service
qsecofr/1111111
qsecofr/2222222
qsvr/qsvr
secofr/secofr

DECserver
~~~~~~~~~
ACCESS
SYSTEM

Hewlett Packard MPE-XL
~~~~~~~~~~~~~~~~~~~~~~
HELLO           MANAGER.SYS
HELLO           MGR.SYS
HELLO           FIELD.SUPPORT     HPUNSUP or SUPPORT or HP
HELLO           OP.OPERATOR
MGR             CAROLIAN
MGR             CCC
MGR             CNAS
MGR             CONV
MGR             COGNOS
OPERATOR        COGNOS
MANAGER         COGNOS
OPERATOR        DISC
MGR             HPDESK
MGR             HPWORD
FIELD           HPWORD
MGR             HPOFFICE
SPOOLMAN        HPOFFICE
ADVMAIL         HPOFFICE
MAIL            HPOFFICE
WP              HPOFFICE
MANAGER         HPOFFICE
MGR             HPONLY
FIELD           HPP187
MGR             HPP187
MGR             HPP189
MGR             HPP196
MGR             INTX3
MGR             ITF3000
MANAGER         ITF3000
MAIL            MAIL
MGR             NETBASE
MGR             REGO
MGR             RJE
MGR             ROBELLE
MANAGER         SECURITY
MGR             SECURITY
FIELD           SERVICE
MANAGER         SYS
MGR             SYS
PCUSER          SYS
RSBCMON         SYS
OPERATOR        SYS
OPERATOR        SYSTEM
FIELD           SUPPORT
OPERATOR        SUPPORT
MANAGER         TCH
MAIL            TELESUP
MANAGER         TELESUP
MGR             TELESUP
SYS             TELESUP
MGE             VESOFT
MGE             VESOFT
MGR             WORD
MGR             XLSERVER

Common jobs are Pub, Sys, Data
Common passwords are HPOnly, TeleSup, HP, MPE, Manager, MGR, Remote

Major BBS
~~~~~~~~~
Sysop           Sysop

PICK O/S
~~~~~~~~
DSA             # Desquetop System Administrator
DS
DESQUETOP
PHANTOM

Prolog
~~~~~~
PBX             PBX
NETWORK         NETWORK
NETOP           <null>

Rolm
~~~~
CBX Defaults

op              op
op              operator
su              super
admin           pwp
eng             engineer

PhoneMail Defaults

sysadmin        sysadmin
tech            tech
poll            tech

RSX
~~~
SYSTEM/SYSTEM   (Username SYSTEM, Password SYSTEM)
1,1/system      (Directory [1,1] Password SYSTEM)
BATCH/BATCH
SYSTEM/MANAGER
USER/USER

Default accounts for Micro/RSX:

MICRO/RSX

Alternately you can hit <CTRL-Z>  when the boot sequence asks you for the
date and create an account using:

RUN ACNT

    or  RUN $ACNT

(Numbers below 10 oct are Priveleged)

Reboot and wait for the date/time question. Type ^C and at the MCR prompt,
type "abo at." You must include the . dot!

If this works, type "acs lb0:/blks=1000" to get some swap space so the
new step won't wedge.

type " run $acnt" and change the password of any account with a group
number of 7 or less.

You may find that the ^C does not work. Try ^Z and ESC as well.
Also try all 3 as terminators to valid and invalid times.

If none of the above work, use the halt switch to halt the system,
just after a invalid date-time.  Look for a user mode PSW 1[4-7]xxxx.
then deposit 177777 into R6, cross your fingers, write protect the drive
and continue the system.  This will hopefully result in indirect blowing
up...  And hopefully the system has not been fully secured.

System 75
~~~~~~~~~
bcim            bcimpw
bciim           bciimpw
bcms            bcmspw, bcms
bcnas           bcnspw
blue            bluepw
browse          looker, browsepw
craft           crftpw, craftpw, crack
cust            custpw
enquiry         enquirypw
field           support
inads           indspw, inadspw, inads
init            initpw
kraft           kraftpw
locate          locatepw
maint           maintpw, rwmaint
nms             nmspw
rcust           rcustpw
support         supportpw
tech            field

Taco Bell
~~~~~~~~~
rgm             rollout
tacobell        <null>

  
Verifone Junior 2.05
~~~~~~~~~~~~~~~~~~~~
Default password: 166816

VMS
~~~
field           service
systest         utep

22. What port is XXX on?

The file /etc/services on most Unix machines lists the activity
occurring on each port.  Here is the most complete port list in
existence, originally presented in RFC 1340:

Keyword         Decimal    Description
-------         -------    -----------
                  0/tcp    Reserved
                  0/udp    Reserved
tcpmux            1/tcp    TCP Port Service Multiplexer
tcpmux            1/udp    TCP Port Service Multiplexer
compressnet       2/tcp    Management Utility
compressnet       2/udp    Management Utility
compressnet       3/tcp    Compression Process
compressnet       3/udp    Compression Process
                  4/tcp    Unassigned
                  4/udp    Unassigned
rje               5/tcp    Remote Job Entry
rje               5/udp    Remote Job Entry
                  6/tcp    Unassigned
                  6/udp    Unassigned
echo              7/tcp    Echo
echo              7/udp    Echo
                  8/tcp    Unassigned
                  8/udp    Unassigned
discard           9/tcp    Discard
discard           9/udp    Discard
                 10/tcp    Unassigned
                 10/udp    Unassigned
systat           11/tcp    Active Users
systat           11/udp    Active Users
                 12/tcp    Unassigned
                 12/udp    Unassigned
daytime          13/tcp    Daytime
daytime          13/udp    Daytime
                 14/tcp    Unassigned
                 14/udp    Unassigned
                 15/tcp    Unassigned [was netstat]
                 15/udp    Unassigned
                 16/tcp    Unassigned
                 16/udp    Unassigned
qotd             17/tcp    Quote of the Day
qotd             17/udp    Quote of the Day
msp              18/tcp    Message Send Protocol
msp              18/udp    Message Send Protocol
chargen          19/tcp    Character Generator
chargen          19/udp    Character Generator
ftp-data         20/tcp    File Transfer [Default Data]
ftp-data         20/udp    File Transfer [Default Data]
ftp              21/tcp    File Transfer [Control]
ftp              21/udp    File Transfer [Control]
                 22/tcp    Unassigned
                 22/udp    Unassigned
telnet           23/tcp    Telnet
telnet           23/udp    Telnet
                 24/tcp    any private mail system
                 24/udp    any private mail system
smtp             25/tcp    Simple Mail Transfer
smtp             25/udp    Simple Mail Transfer
                 26/tcp    Unassigned
                 26/udp    Unassigned
nsw-fe           27/tcp    NSW User System FE
nsw-fe           27/udp    NSW User System FE
                 28/tcp    Unassigned
                 28/udp    Unassigned
msg-icp          29/tcp    MSG ICP
msg-icp          29/udp    MSG ICP
                 30/tcp    Unassigned
                 30/udp    Unassigned
msg-auth         31/tcp    MSG Authentication
msg-auth         31/udp    MSG Authentication
                 32/tcp    Unassigned
                 32/udp    Unassigned
dsp              33/tcp    Display Support Protocol
dsp              33/udp    Display Support Protocol
                 34/tcp    Unassigned
                 34/udp    Unassigned
                 35/tcp    any private printer server
                 35/udp    any private printer server
                 36/tcp    Unassigned
                 36/udp    Unassigned
time             37/tcp    Time
time             37/udp    Time
                 38/tcp    Unassigned
                 38/udp    Unassigned
rlp              39/tcp    Resource Location Protocol
rlp              39/udp    Resource Location Protocol
                 40/tcp    Unassigned
                 40/udp    Unassigned
graphics         41/tcp    Graphics
graphics         41/udp    Graphics
nameserver       42/tcp    Host Name Server
nameserver       42/udp    Host Name Server
nicname          43/tcp    Who Is
nicname          43/udp    Who Is
mpm-flags        44/tcp    MPM FLAGS Protocol
mpm-flags        44/udp    MPM FLAGS Protocol
mpm              45/tcp    Message Processing Module [recv]
mpm              45/udp    Message Processing Module [recv]
mpm-snd          46/tcp    MPM [default send]
mpm-snd          46/udp    MPM [default send]
ni-ftp           47/tcp    NI FTP
ni-ftp           47/udp    NI FTP
                 48/tcp    Unassigned
                 48/udp    Unassigned
login            49/tcp    Login Host Protocol
login            49/udp    Login Host Protocol
re-mail-ck       50/tcp    Remote Mail Checking Protocol
re-mail-ck       50/udp    Remote Mail Checking Protocol
la-maint         51/tcp    IMP Logical Address Maintenance
la-maint         51/udp    IMP Logical Address Maintenance
xns-time         52/tcp    XNS Time Protocol
xns-time         52/udp    XNS Time Protocol
domain           53/tcp    Domain Name Server
domain           53/udp    Domain Name Server
xns-ch           54/tcp    XNS Clearinghouse
xns-ch           54/udp    XNS Clearinghouse
isi-gl           55/tcp    ISI Graphics Language
isi-gl           55/udp    ISI Graphics Language
xns-auth         56/tcp    XNS Authentication
xns-auth         56/udp    XNS Authentication
                 57/tcp    any private terminal access
                 57/udp    any private terminal access
xns-mail         58/tcp    XNS Mail
xns-mail         58/udp    XNS Mail
                 59/tcp    any private file service
                 59/udp    any private file service
                 60/tcp    Unassigned
                 60/udp    Unassigned
ni-mail          61/tcp    NI MAIL
ni-mail          61/udp    NI MAIL
acas             62/tcp    ACA Services
acas             62/udp    ACA Services
via-ftp          63/tcp    VIA Systems - FTP
via-ftp          63/udp    VIA Systems - FTP
covia            64/tcp    Communications Integrator (CI)
covia            64/udp    Communications Integrator (CI)
tacacs-ds        65/tcp    TACACS-Database Service
tacacs-ds        65/udp    TACACS-Database Service
sql*net          66/tcp    Oracle SQL*NET
sql*net          66/udp    Oracle SQL*NET
bootps           67/tcp    Bootstrap Protocol Server
bootps           67/udp    Bootstrap Protocol Server
bootpc           68/tcp    Bootstrap Protocol Client
bootpc           68/udp    Bootstrap Protocol Client
tftp             69/tcp    Trivial File Transfer
tftp             69/udp    Trivial File Transfer
gopher           70/tcp    Gopher
gopher           70/udp    Gopher
netrjs-1         71/tcp    Remote Job Service
netrjs-1         71/udp    Remote Job Service
netrjs-2         72/tcp    Remote Job Service
netrjs-2         72/udp    Remote Job Service
netrjs-3         73/tcp    Remote Job Service
netrjs-3         73/udp    Remote Job Service
netrjs-4         74/tcp    Remote Job Service
netrjs-4         74/udp    Remote Job Service
                 75/tcp    any private dial out service
                 75/udp    any private dial out service
                 76/tcp    Unassigned
                 76/udp    Unassigned
                 77/tcp    any private RJE service
                 77/udp    any private RJE service
vettcp           78/tcp    vettcp
vettcp           78/udp    vettcp
finger           79/tcp    Finger
finger           79/udp    Finger
www              80/tcp    World Wide Web HTTP
www              80/udp    World Wide Web HTTP
hosts2-ns        81/tcp    HOSTS2 Name Server
hosts2-ns        81/udp    HOSTS2 Name Server
xfer             82/tcp    XFER Utility
xfer             82/udp    XFER Utility
mit-ml-dev       83/tcp    MIT ML Device
mit-ml-dev       83/udp    MIT ML Device
ctf              84/tcp    Common Trace Facility
ctf              84/udp    Common Trace Facility
mit-ml-dev       85/tcp    MIT ML Device
mit-ml-dev       85/udp    MIT ML Device
mfcobol          86/tcp    Micro Focus Cobol
mfcobol          86/udp    Micro Focus Cobol
                 87/tcp    any private terminal link
                 87/udp    any private terminal link
kerberos         88/tcp    Kerberos
kerberos         88/udp    Kerberos
su-mit-tg        89/tcp    SU/MIT Telnet Gateway
su-mit-tg        89/udp    SU/MIT Telnet Gateway
dnsix            90/tcp    DNSIX Securit Attribute Token Map
dnsix            90/udp    DNSIX Securit Attribute Token Map
mit-dov          91/tcp    MIT Dover Spooler
mit-dov          91/udp    MIT Dover Spooler
npp              92/tcp    Network Printing Protocol
npp              92/udp    Network Printing Protocol
dcp              93/tcp    Device Control Protocol
dcp              93/udp    Device Control Protocol
objcall          94/tcp    Tivoli Object Dispatcher
objcall          94/udp    Tivoli Object Dispatcher
supdup           95/tcp    SUPDUP
supdup           95/udp    SUPDUP
dixie            96/tcp    DIXIE Protocol Specification
dixie            96/udp    DIXIE Protocol Specification
swift-rvf        97/tcp    Swift Remote Vitural File Protocol
swift-rvf        97/udp    Swift Remote Vitural File Protocol
tacnews          98/tcp    TAC News
tacnews          98/udp    TAC News
metagram         99/tcp    Metagram Relay
metagram         99/udp    Metagram Relay
newacct         100/tcp    [unauthorized use]
hostname        101/tcp    NIC Host Name Server
hostname        101/udp    NIC Host Name Server
iso-tsap        102/tcp    ISO-TSAP
iso-tsap        102/udp    ISO-TSAP
gppitnp         103/tcp    Genesis Point-to-Point Trans Net
gppitnp         103/udp    Genesis Point-to-Point Trans Net
acr-nema        104/tcp    ACR-NEMA Digital Imag. & Comm. 300
acr-nema        104/udp    ACR-NEMA Digital Imag. & Comm. 300
csnet-ns        105/tcp    Mailbox Name Nameserver
csnet-ns        105/udp    Mailbox Name Nameserver
3com-tsmux      106/tcp    3COM-TSMUX
3com-tsmux      106/udp    3COM-TSMUX
rtelnet         107/tcp    Remote Telnet Service
rtelnet         107/udp    Remote Telnet Service
snagas          108/tcp    SNA Gateway Access Server
snagas          108/udp    SNA Gateway Access Server
pop2            109/tcp    Post Office Protocol - Version 2
pop2            109/udp    Post Office Protocol - Version 2
pop3            110/tcp    Post Office Protocol - Version 3
pop3            110/udp    Post Office Protocol - Version 3
sunrpc          111/tcp    SUN Remote Procedure Call
sunrpc          111/udp    SUN Remote Procedure Call
mcidas          112/tcp    McIDAS Data Transmission Protocol
mcidas          112/udp    McIDAS Data Transmission Protocol
auth            113/tcp    Authentication Service
auth            113/udp    Authentication Service
audionews       114/tcp    Audio News Multicast
audionews       114/udp    Audio News Multicast
sftp            115/tcp    Simple File Transfer Protocol
sftp            115/udp    Simple File Transfer Protocol
ansanotify      116/tcp    ANSA REX Notify
ansanotify      116/udp    ANSA REX Notify
uucp-path       117/tcp    UUCP Path Service
uucp-path       117/udp    UUCP Path Service
sqlserv         118/tcp    SQL Services
sqlserv         118/udp    SQL Services
nntp            119/tcp    Network News Transfer Protocol
nntp            119/udp    Network News Transfer Protocol
cfdptkt         120/tcp    CFDPTKT
cfdptkt         120/udp    CFDPTKT
erpc            121/tcp    Encore Expedited Remote Pro.Call
erpc            121/udp    Encore Expedited Remote Pro.Call
smakynet        122/tcp    SMAKYNET
smakynet        122/udp    SMAKYNET
ntp             123/tcp    Network Time Protocol
ntp             123/udp    Network Time Protocol
ansatrader      124/tcp    ANSA REX Trader
ansatrader      124/udp    ANSA REX Trader
locus-map       125/tcp    Locus PC-Interface Net Map Ser
locus-map       125/udp    Locus PC-Interface Net Map Ser
unitary         126/tcp    Unisys Unitary Login
unitary         126/udp    Unisys Unitary Login
locus-con       127/tcp    Locus PC-Interface Conn Server
locus-con       127/udp    Locus PC-Interface Conn Server
gss-xlicen      128/tcp    GSS X License Verification
gss-xlicen      128/udp    GSS X License Verification
pwdgen          129/tcp    Password Generator Protocol
pwdgen          129/udp    Password Generator Protocol
cisco-fna       130/tcp    cisco FNATIVE
cisco-fna       130/udp    cisco FNATIVE
cisco-tna       131/tcp    cisco TNATIVE
cisco-tna       131/udp    cisco TNATIVE
cisco-sys       132/tcp    cisco SYSMAINT
cisco-sys       132/udp    cisco SYSMAINT
statsrv         133/tcp    Statistics Service
statsrv         133/udp    Statistics Service
ingres-net      134/tcp    INGRES-NET Service
ingres-net      134/udp    INGRES-NET Service
loc-srv         135/tcp    Location Service
loc-srv         135/udp    Location Service
profile         136/tcp    PROFILE Naming System
profile         136/udp    PROFILE Naming System
netbios-ns      137/tcp    NETBIOS Name Service
netbios-ns      137/udp    NETBIOS Name Service
netbios-dgm     138/tcp    NETBIOS Datagram Service
netbios-dgm     138/udp    NETBIOS Datagram Service
netbios-ssn     139/tcp    NETBIOS Session Service
netbios-ssn     139/udp    NETBIOS Session Service
emfis-data      140/tcp    EMFIS Data Service
emfis-data      140/udp    EMFIS Data Service
emfis-cntl      141/tcp    EMFIS Control Service
emfis-cntl      141/udp    EMFIS Control Service
bl-idm          142/tcp    Britton-Lee IDM
bl-idm          142/udp    Britton-Lee IDM
imap2           143/tcp    Interim Mail Access Protocol v2
imap2           143/udp    Interim Mail Access Protocol v2
news            144/tcp    NewS
news            144/udp    NewS
uaac            145/tcp    UAAC Protocol
uaac            145/udp    UAAC Protocol
iso-tp0         146/tcp    ISO-IP0
iso-tp0         146/udp    ISO-IP0
iso-ip          147/tcp    ISO-IP
iso-ip          147/udp    ISO-IP
cronus          148/tcp    CRONUS-SUPPORT
cronus          148/udp    CRONUS-SUPPORT
aed-512         149/tcp    AED 512 Emulation Service
aed-512         149/udp    AED 512 Emulation Service
sql-net         150/tcp    SQL-NET
sql-net         150/udp    SQL-NET
hems            151/tcp    HEMS
hems            151/udp    HEMS
bftp            152/tcp    Background File Transfer Program
bftp            152/udp    Background File Transfer Program
sgmp            153/tcp    SGMP
sgmp            153/udp    SGMP
netsc-prod      154/tcp    NETSC
netsc-prod      154/udp    NETSC
netsc-dev       155/tcp    NETSC
netsc-dev       155/udp    NETSC
sqlsrv          156/tcp    SQL Service
sqlsrv          156/udp    SQL Service
knet-cmp        157/tcp    KNET/VM Command/Message Protocol
knet-cmp        157/udp    KNET/VM Command/Message Protocol
pcmail-srv      158/tcp    PCMail Server
pcmail-srv      158/udp    PCMail Server
nss-routing     159/tcp   NSS-Routing
nss-routing     159/udp   NSS-Routing
sgmp-traps      160/tcp    SGMP-TRAPS
sgmp-traps      160/udp    SGMP-TRAPS
snmp            161/tcp    SNMP
snmp            161/udp    SNMP
snmptrap        162/tcp    SNMPTRAP
snmptrap        162/udp    SNMPTRAP
cmip-man        163/tcp    CMIP/TCP Manager
cmip-man        163/udp    CMIP/TCP Manager
cmip-agent      164/tcp    CMIP/TCP Agent
smip-agent      164/udp    CMIP/TCP Agent
xns-courier     165/tcp   Xerox
xns-courier     165/udp   Xerox
s-net           166/tcp    Sirius Systems
s-net           166/udp    Sirius Systems
namp            167/tcp    NAMP
namp            167/udp    NAMP
rsvd            168/tcp    RSVD
rsvd            168/udp    RSVD
send            169/tcp    SEND
send            169/udp    SEND
print-srv       170/tcp    Network PostScript
print-srv       170/udp    Network PostScript
multiplex       171/tcp    Network Innovations Multiplex
multiplex       171/udp    Network Innovations Multiplex
cl/1            172/tcp    Network Innovations CL/1
cl/1            172/udp    Network Innovations CL/1
xyplex-mux      173/tcp    Xyplex
xyplex-mux      173/udp    Xyplex
mailq           174/tcp    MAILQ
mailq           174/udp    MAILQ
vmnet           175/tcp    VMNET
vmnet           175/udp    VMNET
genrad-mux      176/tcp    GENRAD-MUX
genrad-mux      176/udp    GENRAD-MUX