InS_StArT
3C507.COM
1.0
^3Com 3C507 Etherlink 16,3C507.COM,0E0,RII0101
?The driver is self-configuring.
$O0E0(NODE ADDRESS)
0
7FFFFFFFFFFF
*O0E0(FRAME)
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD
