
                    SAA v1.2 to v1.3 Upgrade

Things to Note:

1.   The product is now installed using the standard
     INSTALL.NLM instead of the CSINSTAL.NLM

2.   You can not upgrade from v1.1 to v1.3. Must use CSINTAL
     from v1.1 to remove the product, then install v1.3 using
     INSTALL

3.   VERY IMPORTANT to read the various README files on the
     disks. Especially the README file on Disk #1


The installation can be done from one of the following sources:

          .    Diskettes
          .    DOS partition of the server
          .    NetWare partition of the server
          .    Remote from another server ... apparently there are
                    problems with this method at this time??

Best to install from a NetWare partition since it does not require
you to first down the server.

Step 1:

     .    Create a directory for COMMEXEC files
     .    Create a directory for SAA v1.3 files
     .    xCOPY the contents of all the disks into their
          respective directories

     e.g.

               F:\> md commexec
               F:\> md saa13
               F:\> xcopy a:\*.* commexec /s
                         ...
               F:\> xcopy a:\*.* saa13 /s


Step 2:

     .    All the files on diskette #7 and #8 MUST be
          copied over to the SYS:SYSTEM directory of
          your server. And the server need to be
          restarted before installing and loading SAA
          v1.3

     .    Before rebooting the server, modify the
          AUTOEXEC.NCF file to include the following
          statement before loading the LAN drivers:

               LOAD LSLENH
               LOAD SPXFIX1

     .    Also, make sure you assign a logical board
          name to your adapter card that is your host
          link, eg

               LOAD TOKEN node=xxxx ... name=SNA

          You need this name for the CSCON later.


     .    Down the server


Side note: with the new ODI Token Ring driver, specifing a node
address in the LOAD statement will cause the following to be
displayed at load time:

               WARNING: Token-NU-127: The local bit
               in the node address override was set

This is an informational message to let you know that you have
specified a Locally Administrated Address (LAA) for this Token Ring
adapter.
Step 3:


In order to use the new Token Ring and Ethernet drivers provided
with SAA v1.3, SERVER.EXE must be patched using the following
procedure (no need for the SDLC drivers):

     .    Copy XLOAD.EXE and LDR001.PTF from Diskette #7
          to the directory where SERVER.EXE resides on
          your server's DOS partition

     .    Ensure there is sufficient disk space for a
          second copy of SERVER.EXE

     .    At the DOS prompt, type:

               XLOAD LDR001.PTF SERVER.EXE

          The old copy of SERVER.EXE will be saved as
          SERVER.OLD and the newly patch version will be
          named SERVER.EXE  Make sure you keep the
          SERVER.OLD for future changes.

     .    Reboot the server.


Step 4:

     .    At the server console (or via RCONSOLE) type:

                    LOAD INSTALL

     .    Choose the Products Options screen, then press
          the INSERT key.

               1st time, enter the pathname for the COMMEXEC files
               2nd time, enter the pathname for the SAA v1.3 files


Step 5:

     .    Configure the profiles using CSCON as before.

     .    Make sure you specify a board name in the Host
          Connection section (last entry on the 2-screen
          menu). In our example above, the logical board
          name was SNA.

Step 6:

     .    Modify your AUTOEXEC.NCF file so that you also
          load the following after loading COMMEXEC:

               LOAD DLM
               LOAD SMA

          (DLM = Data Link Manager; SMA = Service Mapping Agent)


Some Changes:

     .    You now do CSLOAD, CSUNLOAD from the console
          prompt (the colon prompt). There is no more
          CS> prompt

     .    You also execute the CSSTATUS command from the
          console prompt.

     .    The name COMMEXEC.CSC has been changed to
          COMMEXEC.NCF


Important Note:

NetWare for SAA creates a SYSTEM.LOG file that will continue to
grow in size. To avoide running of disk space, this file should be
deleted on a periodic basis.

+-----------------------------------+
| Prepared by: Peter Kuo (DreamLAN) |
| Revision   : 1.1                  |
| Date       : April 26, 1993       |
|       All rights reserved         |
+-----------------------------------+
