TCTOKSH
*(INT) Interrupt Request
@2
3
4
5
7
10
11
12
*(PORT) IO Base Address
@1A20
2A20
*(DMA) DMA channel
0
@5
6
7
