9553 0B7 0BB 120MB14 ms 250MB14 ms None None $ 795 $ 960 November 1993 November 1993

All: 486SLC2 - 50/25 MHz All: None

All: Open socket for 387SX - 25 MHz

All: 0 KB / 0 KB All:N/A All:N/A

All: 4 / 16 MB All: 70 ns / 72 pin All: 70 ns speed only (supports 2, 4, 8, MB parity SIMMs) All: 3 sockets / 2 available (one 4 MB parity SIMM is standard) All: Parity

All: IDE All: 16 bit controller on planar

All: Micro Channel^® 3 slots / 3 available

3 bays / 1 bay available (diskette, disk use two)

1.44 MB 3.5" diskette drive / None media sense to correctly format, read, write 1 and 2 MB diskettes All: One 25 pin serial port / DMA support / UART 16550A / 57.6 KBps maximum supported speed All: One parallel port / DMA support / bidirectional / 100 KBps maximum supported speed

All: GD5426 SVGA accelerator / Cirrus Logic^® System rated at 13 Graphics WinMarks All: Micro Channel / 16 bit (on planar) SVGA graphics controller meets ISO 9241-3 requirements All: 1 MB / 1 MB (DRAM memory) 70 ns Power managed display support for VESA DPMS compatible displays

All: No All: Yes All: Yes All: Yes All: Yes No 1 of 3 op sys (see below); models prior to Feb 23, 1994 had no op sys included All: 128 KB in Flash memory on the planar board (SurePath™ BIOS) All: Fast startup mode / selectable boot All: Choice of four keyboards Enhanced 101 key and mouse Enhanced 101 key with TrackPoint II; no mouse ($50) Quiet (rubber dome) 101 key and mouse Quiet Touch 84 key with TrackPoint II; no mouse ($50) All: IBM Enhanced mouse (400 dpi) except no mouse if select keyboard with TrackPoint II™ All: 90 watt / universal / manual switch setting /

built in overload, surge protection

9553 LAN Station 1BX 2BX No disk No disk Ethernet 10BaseT 16/4 Token-Ring $ 667 $ 1,033 November 1993 November 1993

3 slots / 2 available (LAN adapter in one slot)

3 bays / 3 available

Type Models Disk - size / speed Standard adapter Price (retail USD) Available date

Processor / MHz Processor upgrade(s)

Math coprocessor

L2 cache - std / max L2 cache - write policy L2 cache - method

Memory - std / max Memory - speed / pins Mem - supported SIMMs Mem - total sockets / avail Memory - type

Disk controller Controller implementation

Architecture MCA slots / available

Bays / available

Diskette drive

Serial port Parallel port

Graphics - controller/vendor Graphics - arch / data path Graphics - memory std/max

Security Tamper evident cover Privileged-access passwd Power-on password Cover key lock U Bolt support

3 MB System Partition Software included

BIOS Other Keyboard

Mouse Power supply

All: Three bays: 3.5", SL1", access, std diskette, (except LS) 3.5", SL1", no access, std disk, (except LS) 5.25", SL1", no access, open

IBM PS/2 Model 53

IBM^® PS/2^® :

IBM only supports a slim line (1" high) 3.5" IDE disk in the open 5.25" bay. IBM does not support diskette drives, CD-ROM, or tape in the open bay. IBM does not support internal SCSI devices.

disk

All: Maximum disk capacity Internal: 1.05 GB with two 527 MB IDE disks Internal/external: 43.05 GB by using three SCSI adapters, three external 3511-0V0 Exernal Enclosures with 21 IBM 2.0 GB SCSI-2 disks (42 GB).

diskette

53 486SLC2 53LS 486SLC2

Privileged-access password: restricts access to system programs; stops system after a POST error also

restricting access to system programs; prohibits unauthorized modifications to hardware

All: Vital Product Data (VPD) enabled for unique ID (model/submodel); Type/model/serial number; Planar serial number; Manufacturing ID; Planar FRU number; Planar part number.

GD5426 VIDEO MODES

Resolution 640 x 480 640 x 480 640 x 480 640 x 480

800 x 600 800 x 600 800 x 600

1024 x 768 1024 x 768

Video Memory (1MB) can not be increased or decreased Note (i)= ISO certified with specific fonts, typeface, and monitors Note (a)= Not supported by OS/2 1.3.x or 2.0 without Service Pack Note (b)= Not supported by OS/2 with Service Pack or 2.1 I = Interlaced

Frame rate Hz (non-interlaced)

60, 72 60, 72 60, 72 60 56, 60, 72 56, 60, 72 56, 60

60, 70, 72, 43.5 (I) 60, 70, 72, 43.5 (I)

Maximum

colors 16 256 65,536 16.7 mil 16 256 65,536 16 256

Device Drivers Support DOS Windows OS/2

Y(i) Y Y Y Y Y(a) � Y � � Y �

Y Y Y(b) Y Y Y(a) � Y �

Y Y Y(b) Y Y Y(i, a)

Ideal LAN client

Entry-level Micro Channel

Lowest PS/2 price

Ethernet (1BX) model has a 10BaseT (twisted pair) connector. Data transfers via 10Base2 (thin coax), 10Base5 (thick coax), or a fiber optic cable can be done via an Attachment Unit Interface (AUI) connection and external transceiver.

All trademarks are the property of their respective owners (listed on Trademark sheet) Price decrease effective October 3, 1994

No warranties are expressed or implied in this summary (53) Compiled by Roger Dodson, IBM. October 1994

3 year warranty On site warranty all 3 years All cities in all states 24 hour / 7 day service coverage 4 hour response time 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM or dealer warranty/service 30 day money back guarantee

PS/2 WARRANTY SERVICE SUPPORT

N/A since no disk None

Choice of operating sys (until 11/21/94):

IBM OS/2^® 2.1 IBM DOS 6.1 / Windows™ 3.1 IBM DOS 5.02 / Windows 3.1 After September 20, 1994:

IBM OS/2 2.11 IBM DOS 6.3 / Windows 3.11 Includes all software pubs and all diskettes (op sys is not preinstalled)