15PT 15" FST 13.7" / 348 mm Touch SVGA .28 Capacitive Anti-glare Polished 9525-T01 9525-T21 Sept 93 Feb 94 $ 1,260 $ 1,260

10.5 x 8.0" 11.0 x 8.3" 266 x 201 280 x 210

Multiscanning 50 to 110 Hz 30 to 64 kHz 90 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60 � � 2, 3, 4, 5

MPR-II ISO 9241-3 Lift option Digital Digital Digital Digital Continual (r,b) Reset button No No No No No No No Microprocessor 15 Automatic 11 26 Yes Reset button No No No 3 year

Name Screen Actual viewable diagonal size Type Dot pitch (mm) Touch technology Screen Type-model Available date Price(retail USD)

Viewing area (inches) Max view area (inches) Viewing area (mm) Max view area (mm)

Frequency Vertical refresh rate range Horizontal line rate range Maximum pel rate

640 x 480 NI (presets) 800 x 600 NI (presets) 1024 x 768 NI (presets) 1024 x 768 I (presets) 1280 x 1024 NI orI (presets) 1360 x 1024 NI orI (presets) 1600 x 1200 NI (presets) 3270 MFI emulation modes

Emission ISO 9241-3 Lift/tilt/swivel option Brightness/contrast control Picture width/height control Horizontal/vertical centering Trapezoidal/pincushion adj Color tint (red, green, blue) Color tint reset button 5 BNC connectors Apple/RS/6000/Sun attach

Horz converg adj button Vert converg adj button Rotation adjustment button Converg/rotation reset button Degauss button

Microprocsor (detects modes) Factory preset modes Ability to save a new setting User modes that can save Total recallable modes Prevent overwriting presets Geometry reset button

Power management Power mgmt flashing LED Power mgmt on/off switch Warranty

(Premium Touch)

TOUCH - SUPER VGA COLOR

IBM Displays (Touch)

21PT 21" Diamondtron™ 19.1" / 485 mm Touch SVGA .31 stripe Capacitive Anti-glare Polished 9521-T01 9521-T21 Nov 93 Feb 94 $ 3,039 $ 3,039

15.0 x 11.2" 15.5 x 11.5 380 x 285 395 x 292

Multiscanning 50 to 152 Hz 30 to 82 kHz 175 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60, 77 NI 77 NI 60 2, 3, 4, 5

MPR-II ISO 9241-3 No (too big) Digital Digital Digital Digital Continual (r,g,b) Reset button 5 BNC Apple attach

Horz converg No Rotation button Reset button Degauss button

Microprocessor 12 Automatic 10 22 Yes Reset button No No Yes 3 year

14PT 14" 13" / 331 mm Touch SVGA .28 Capacitive Anti-glare Polished 9524-T01 9524-T21 Sept 93 Feb 94 $ 1,140 $ 1,140

10.0 x 7.6" 10.6 x 8.0" 256 x 193 270 x 202

Multiscanning 50 to 110 Hz 30 to 64 kHz 90 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60 � � 2, 3, 4, 5

MPR-II ISO 9241-3 Lift option Digital Digital Digital Digital Continual (r,b) Reset button No No No No No No No Microprocessor 15 Automatic 11 26 Yes Reset button No No No 3 year

17PT 17" Trinitron™ 15.4" / 391 mm Touch SVGA .26 stripe Capacitive Anti-glare Polished 9527-T01 9527-T21 Nov 93 Feb 94 $ 2,260 $ 2,034

11.8 x 8.8" 12.4 x 9.3 300 x 225 315 x 235

Multiscanning 50 to 110 Hz 30 to 82 kHz 160 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60, 77 NI 77 Hz � 2, 3, 4, 5

MPR-II ISO 9241-3 No (too big) Digital Digital Digital Digital Continual (r,b) Reset button 5 BNC Apple attach

Horz converg Vert converg No Reset button Degauss button

Microprocessor 14 Automatic 16 30 Yes Reset button No No No 3 year

No warranties are expressed or implied in this summary (DISPT) Compiled by Roger Dodson, IBM. September 1994

All trademarks are the property of their respective owners (listed on Trademark sheet) Price decrease effective September 27, 1994

I =Interlaced; NI = Non-interlaced Withdrawn from marketing

The 14PT, 15PT, 17PT, and 21PT have the same functions and features of the14P, 15P, 17P, and 21P (except no power management).

14PT and 15PT is the successor to the 8516 touch display.

Touch capability on 14PT, 15PT, 17PT, and 21PT is done by a capacitive overlay which reacts to the naturally occuring charge in the body. Although it will not work with a non charged object like a pencil, it will work through thin gloves like surgical ones. The 8516 worked with anything because it detected movement via strain guages. The 8516 required recalibration after relocating, but thePT models do not require this. Touch displays are factory fitted and the display looks just like a non-touch display. 8516 14" .28 Strain guage Etched 9.8 x 7.4"

NI 60 Hz � I 43.5 Hz VLMF Touch 1 year Jun 91 withdrawn

Size Dot pitch Touch technology Screen Viewing area

640 x 480 800 x 600 1024 x 768

Emission Other Warranty Avail date Price

TOUCH - XGA COLOR

STANDARD FEATURES 95xx TOUCH Universal power supply Anti-static screen Tilt/swivel stand Automatic degauss

952x "P" DISPLAYS WARRANTY SERVICE SUPPORT 3 year warranty On-site first year Mail-in repair second and third year (with option of upgrade to on-site) All cities in all states 24 hr/7 day service coverage 1st yr 4 hr average response time (1st yr) Option to upgrade yrs 2 and 3 to: 9-5 Mon-Fri cov, next day resp or 24 hr/7 day coverage, 4 hr response 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM^® or dealer warranty/service 30 day money back guarantee

T0x (1993 models)

Anti-glare (etched screen) Dull glass surface Little glare from lights so

recommend when reflections are a problem Better for darker screen

backgrounds Less screen sharpness Ideal for kiosk use

T2x (1994 models)

Polished (non-etched screen) Shiny glass surface Subject to glare from lights so recommend when reflections are minimal Better for lighter screen backgrounds Enhanced screen sharpness Ideal for desktop use