Name Type-model Screen Actual viewable diagonal size Type Dot pitch (mm) Viewing area (inches) Max view area (inches) Viewing area (mm) Max view area (mm)

Frequency Vertical refresh rate Horizontal line rate Maximum pel rate

640 x 480 NI (presets) 800 x 600 NI (presets) 1024 x 768 NI (presets) 1024 x 768 I (presets) 1280 x 1024NI orI(presets) 3270 MFI emulation modes

Emission ISO 9241-3 Lift/Tilt/Swivel option Brightness/contrast control Picture width/height control Horizontal/vertical centering Trapezoidal/pincushion adj Color tint setting (red/blue) Color tint reset button Type of controls

Rotation adjustment button Degauss button

Microprocsr (detects modes) Factory preset modes Ability to save a new setting User modes that can save Total recallable modes Prevent overwriting presets Geometry reset button Auto-borderless Focus adjustment

DPMS compliant Power management Power mgmt flashing LED Universal power supply Anti-glare screen Anti-static screen Available date Warranty Price (retail USD)

IBM Displays (V series / 63xx)

SUPER VGA COLOR (Value) 14V 6324-001 14" 13.0" / 330 mm SVGA color .28 10.0 x 7.6" 10.6 x 8.0" 256 x 193 270 x 202

Multiscanning 50 to 110 Hz 30 to 64 kHz 90 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60 2, 3, 4, 5

MPR-II ISO 9241-3 Lift option Digital Digital Digital Digital Continual (r, b) Reset button Pushbuttons No No Microprocessor 15 Automatic 11 26 Yes Reset button No Single

DPMS compliant Energy Star 30 watts Flashing LED No Anti-glare Anti-static July 93 1 year onsite $ 450

15V 6325-001 15" FST 13.7" / 348 mm SVGA color .28 10.5 x 8.0" 11.0 x 8.3" 266 x 201 280 x 210

Multiscanning 50 to 110 Hz 30 to 64 kHz 90 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60 2, 3, 4, 5

MPR-II ISO 9241-3 Lift option Digital Digital Digital Digital Continual (r, b) Reset button Pushbuttons No No Microprocessor 15 Automatic 11 26 Yes Reset button No Single

DPMS compliant Energy Star 30 watts Flashing LED No Anti-glare Anti-static July 93 1 year onsite $ 606

6319 6319-001 15" FST 12.7" / 322 mm SVGA color .28 10.2 x 7.4" 11.0 x 8.2" 260 x 190 281 x 209

Multiscanning 50 to 100 Hz 30 to 60 kHz 80 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72 Hz I 43.5 I 50 2, 3, 4, 5

VLMF No No Analog Digital Digital Digital 2 fixed settings N/A Pushbuttons No No Microprocessor 7 Yes 6 13 No No No No No No N/A No Anti-glare No Sept 92 1 year onsite $ 504

17V 6327-001 17" FST 15.6" / 397 mm SVGA color .28 11.8 x 8.8" 12.6 x 9.4" 300 x 225 320 x 239

Multiscanning 50 to 110 Hz 30 to 64 kHz 110 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 75 I 43.5 I 50, NI 60 2, 3, 4, 5

MPR-II ISO 9241-3 No (too big) Digital Digital Digital Pincushion only Continual (r,b) Reset button Pushbuttons No Degauss button

Microprocessor 10 Automatic 6 16 Yes Reset button No No DPMS compliant Energy Star 30 watts Flashing LED Yes Anti-glare Anti-static Oct 93 1 year onsite $ 1,050

No warranties are expressed or implied in this summary (DISPV) Compiled by Roger Dodson, IBM. August 1994

I =Interlaced; NI = Non-interlaced Price decrease effective June 15, 1994

Products announced August 1994 or later All trademarks are the property of their respective owners (listed on Trademark sheet)

17V 6327-023 17" FST 15.6" / 398 mm SVGA color .28 11.8 x 8.8" 12.6 x 9.5" 300 x 225 320 x 244

Multiscanning 50 to 110 Hz 30 to 64 kHz 110 MHz

60, 72, 75 Hz 56, 60, 72 Hz 60, 70, 72, 76 I 43.5 I 50, NI 60 2, 3, 4, 5

MPR-II ISO 9241-3 No (too big) Digital Digital Digital Digital Continual (r,b) Reset button Pushbuttons

Rotation button Degauss button

Microprocessor 15 Automatic 11 26 Yes Reset button Auto-borderless Double

DPMS compliant Energy Star 30 watts Flashing LED Yes Anti-glare Anti-static August 94 1 year onsite $ 1,050

63xx DISPLAYS WARRANTY SERVICE SUPPORT 1 year warranty On site warranty all year All cities in all states 8am-5pm, Monday-Friday coverage Next day response time Option to upgrade to: 24 hr / 7 day coverage, 4 hr response 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM^® or dealer warranty/service 30 day money back guarantee

632x = 14V, 15V, 17V

STANDARD FEATURES 63xx

Tilt / swivel stand Automatic degauss Borderless

6324 (14V) is the successor to the 6312 and 6314. 6325 (15V) is the successor to the 6319. 6327 (17V)is the successor to the 6317. 63xx displays also have 720 x 350 and 720 x 400 text modes at 70 Hz (NI) and 88 Hz (NI). (6318 is only 70 Hz). The 63xx (except 6318, 14L39, and 14L8) displays aremulti-sync (multifrequency, multiscanning, variable frequency, autosyncing) displays and are capable of any modes whose refresh rates fall within the displays range (for example, 50 to 100 Hz). Preset modes (listed in italics) allow the picture on screen to be perfectly positioned without adjustment.

All IBM color displays have automatic degauss at power on.

17" displays provide almost 50% more viewing area than a 14" display.

V series displays work on all IBM system brands and on non-IBM brands.