Pentium ™

Intel^® CISC/RISC P5 Available June 93 PS/2 Model 95 VP P60/D

60, 66 MHz 567 at 66 MHz 64 bit Data Path 32 bit Processor 32 bit Address Path 8 KB instruction cache Write-thru 2 way set; with parity; 8 KB data cache Write-thru or write-back 2 way set; with parity

Pipelined math co std 2 execute units (superscalar) Internal and external parity Dynamic branch prediction Optimized instructions Address pipelining Burst mode bus (to 528 MB/sec) Power management (SMM)

273 pin / 0.8u 5.0 volts

P5T; 273 pin; Available 1996

Vendor Type Code name Avail date IBM models

MHz iCOMP Data bus Processor Address bus Cache

Features

Voltage

OverDrive™ upgrade

PC Processors (Pentium)

Intel CISC/RISC P54C Available March 94

100/66, 90/60, 75/50 MHz 735 at 90/60 MHz Same Same Same Same Same Same Same Same Same

Same Same Same Same Same Same Same Same Dual processing ready via built in APIC (Advanced Programmable Interrupt Controller) 296 pin / 0.6u 3.3 volts

P54CT uniprocessor replacement;

320 pin; Available 1996 P54CM upgrades P54C to

multiprocessing; 100/66, 90/60 MHz; Available mid 1995

Pentium

No warranties are expressed or implied in this summary (3INTEL) Compiled by Roger Dodson, IBM. June 1994

All trademarks are the property of their respective owners (listed on Trademark sheet)