IBM SCSI Controllers (non-Micro Channel)

Controller

Implementation

SCSI type SCSI bus path / speed I/O Architecture I/O bus path / speed I/O features

RAID levels Tagged Command Queuing Processor Size Channels Connectors

Devices supported Cache std / max Cache method Cache configurations Cache write policy Available date Warranty Price (retail USD) Part number

SCSI-2 Fast PCI Adapter

Option Adapter in IBM PC Server 0PT SCSI-2 Fast 8 bit / 10 MB/sec PCI 32 bit / 66 MB/sec

None (use software) Yes None (intelligent SCSI processor) PCI standard One (internal/external) One internal; one external

7 devices per adapter None (32 byte FIFO buffer) N/A N/A N/A May 1994 3 years $ 199 32G3100

16-Bit AT Fast SCSI Adapter

Option (Options by IBM™ )

SCSI-2 Fast 8 bit / 10 MB/sec ISA 16 bit / 3 MB/sec

None (use software) No None (PIO) 4.25"H x .75"W x 7"D One (internal/external) One internal; one external

7 devices per adapter 0 KB / 0 KB (8 KB buffer) N/A N/A N/A January 1993 3 years $ 179 70G8496

SCSI-2 VL-Bus Adapter

Option (Options by IBM™ )

SCSI-2 Fast 8 bit / 10 MB/sec VL-Bus™ 32 bit / up to 40 MB/sec

None (use software) Yes Custom (RISC based) 3.5"H x .8"W x 6.9"D One (internal/external) One internal; one external Includes diskette connector for on-board diskette controller which supports up to two diskette drives including 2.88 MB

7 devices per adapter 0 KB / 0 KB (256 byte FIFO buffer) N/A N/A N/A July 1994 3 years $ 325 70G8482

All trademarks are the property of their respective owners (listed on Trademark sheet) No warranties are expressed or implied in this summary (4SCSI) Compiled by Roger Dodson, IBM. July 1994