14L8 6321-001 14" 12.5" / 318 mm SVGA color .28 9.8 x 7.4" 10.2 x 7.7" 250 x 187 260 x 195

Fixed � � 45 MHz

60, 72 Hz 56, 60 Hz � I 43.5 Hz � � � 2, 3, 4

MPR-II No Yes No Analog Analog Analog

Analog No No No N/A Knobs No 7 Only current Only current 7 N/A No No No No N/A No Anti-static Anti-glare January 94 1 yr onsite 8-5 M-F Next day Yes $8 $ 359

14L39 6321-011 14" 12.5" / 318 mm SVGA color .39 9.8 x 7.4" 10.2 x 7.7" 250 x 187 260 x 195

Fixed � � 45 MHz

60, 72 Hz 56, 60 Hz � I 43.5 Hz � � � 2, 3, 4

MPR-II No Yes No Analog Analog Analog

Analog No No No N/A Knobs No 7 Only current Only current 7 N/A No No No No N/A No Anti-static Anti-glare April 94 1 yr onsite 8-5 M-F Next day Yes $8 $ 324

9507 Color Display 9507-001 10.4" (similar to 12" display) 10.4" / 263 mm VGA color .33 8.3 x 6.2" 9.7 x 7.3" 211 x 158 247 x 185

Fixed � � 28 MHz

60, 70 Hz � � � � � � � MPR-II and TCO-91 Yes (Flat Panel Addendum) Yes Standard Rocker switch No No No No No No N/A Rocker switch

Yes (but not via Many microprocessor) No N/A N/A N/A N/A N/A No Energy Star (17 watts) Yes Yes N/A Anti-glare October 93 1 yr onsite 24 hr 7 days 4 hour N/A $ 3,540

IBM Displays (Low end; active matrix)

SUPER VGA COLOR(Low end) Name Type-model Screen Actual viewable diagonal size Type Dot pitch (mm) Viewing area (inches) Max view area (inches) Viewing area (mm) Max view area (mm)

Frequency Vertical refresh rate Horizontal line rate Maximum pel rate

640 x 480 NI (presets) 800 x 600 NI (presets) 1024 x 768 NI (presets) 1024 x 768 I (presets) 1280 x 1024NI orI (presets) 1360 x 1024NI orI (presets) 1600 x 1200NI 3270 MFI emulation modes

Emission ISO 9241-3 Tilt/swivel standard Lift/Tilt/Swivel option Brightness/contrast control Picture width/height control Horizontal centering control

Vertical centering control Trapezoidal adjustment Pincushion adjustment Color tint setting (r, b, g) Color tint reset button Type of controls

Microprcsor (detects modes) Factory preset modes Ability to save a new setting User modes that can save Total recallable modes Prevent overwriting presets Geometry reset button Auto-borderless

DPMS compliant Power management Power mgmt flashing LED Universal power supply Anti-static screen Anti-glare screen Available date Warranty Warranty coverage Warranty response Wrnty upgrade 24hr/4hr resp Price(retail USD)

ACTIVE MATRIX - FLAT PANEL

10.4" active matrix flat panel color display. Thin film transistor (same screen as ThinkPad^® 720C).

VGA 640 x 480 with 16 simultaneous colors (out of 512).

No flicker. No glare. No black boarder. 50 to 1 contrast ratio. 13.9 lbs. No fan so virtually silent. Virtually no emissions. External power supply to reduce

size/foot print. Low power consumption (37 watts) Low power standby mode (17 watts). ISO 9241-3 conformance. Requires little desk space (48 sq in). Includes lift, tilt, swivel stand. Easily place/remove 9507 from stand. Hang off wall (when remove from stand).

The 9507 operates at only 37 watts and idles at 17 watts. The 9507 powers down to 17 watts independent of any system unit driver. Contrary to other displays (V and P series), the 9507 does not need VESA DPMS drivers for power saving stages.

Price decrease effective June 15, 1994 All trademarks are the property of their respective owners (listed on Trademark sheet)

No warranties are expressed or implied in this summary (DISPL) Compiled by Roger Dodson, IBM. June 1994

Withdrawn from marketing I = Interlaced; NI = Non-interlaced

The 14L39 replaces the 6318 .

6318, 14L39 and 14L8 also have 720 x 350 and 720 x 400 text modes at 70 Hz.

9507 text modes include:

640 x 350 at 60, 70 Hz 640 x 400 at 60, 70 Hz 720 x 400 at 70 Hz