12M 8504-021 12" FST 10.3" / 261 mm Monochrome N/A ^2 8.3 x 6.2" Same 210 x 157.5 Same

Fixed � � 31.5 kHz 28 MHz

NI 60 Hz � � � � � 2, 3, 4

MPR-II No Yes No Analog No No No N/A Knobs No 3 No None N/A N/A No N/A No Anti-static Anti-glare Oct 93 1 year carry in $ 221

Name Type-model Screen Actual viewable diagonal size Type Dot pitch (mm) Viewing area (inches) Max view area (inches) Viewing area (mm) Max view area (mm)

Frequency Vertical refresh rate range Horizontal line rate range Horizontal scan frequency Maximum pel rate

640 x 480 NI (presets) 800 x 600 NI (presets) 1024 x 768 NI or I (presets) 1280 x 1024 NI or I (presets) 1360 x 1024 NI or I (presets) 1600 x 1280 NI (presets) 3270 MFI emulation modes

Emission ISO 9241-3 Tilt/swivel stand standard Lift/tilt/swivel option Brightness/contrast control Picture width/height control Horizontal/vertical centering

Trapezoidal/pincushion adj Color point setting (blue/pink) Type of controls

Microprocsr (detects modes) Factory preset modes Ability to save a new setting User modes that can save Total recallable modes Prevent overwriting presets

Power management Power mgmt flashing LED Universal power supply Anti-static screen Anti-glare screen Available date Warranty Price (retail USD)

IBM Displays (Monochrome and Image)

MONOCHROME 8507 8507-001 19" 17.3" / 439 mm Monochrome N/A ^2 14 x 10.5 Same 350 x 265 Same

Fixed � � 31.5 or 35.5 kHz 45 MHz NI 60 Hz � I 43.5 Hz � � 2, 3, 4 � No Yes No Analog No No No N/A Knobs No 4 No None N/A N/A No N/A No No Anti-glare Sept 88 1 year carry in $ 400

IMAGE 9504 9504-001 21" FST 19.0" / 482 mm Monochrome - Image N/A ^2(110 dots per inch) 14.6 x 11.7" 15.1 x 12.1" 370 x 296 384 x 308

Fixed � � 102 Khz 230 Mhz

NI 77 Hz (emulated by Image-I) � NI 77 Hz (emulated by Image-I) � NI 77 Hz (emulated by Image-I) NI 77 Hz with 16 grey shades None

MPR-II ISO 9241-3 Yes No Analog Analog Analog No N/A Knobs No 1 Only current Only current N/A N/A None No Universal Anti-static Anti-glare Aug 93 1 year on site $ 1,200

Requires IBM^® Image-I Adapter/A

8504 8504-001 12" FST 10.3" / 261 mm Monochrome N/A ^2 8.2 x 6.2 Same 210 x 157.5 Same

Fixed � � 31.5 kHz 28 MHz NI 60Hz � � � � 2, 3, 4

VLMF No Yes No Analog No No No N/A Knobs No 3 No None N/A N/A No N/A No No Anti-glare Jun 91 1 year carry in $ 245

No warranties are expressed or implied in this summary (DISPM) Compiled by Roger Dodson, IBM. June 1994

Product announced October 28, 1993 All trademarks are the property of their respective owners (listed on Trademark sheet)

1 year warranty On-site warranty all year (9504 only) All cities in all states 8am-5pm, Monday-Friday coverage Next day response time Option to upgrade to: 24 hr / 7 day coverage, 4 hr response 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM or dealer warranty / service 30 day money back guarantee

MONOCHROME DISPLAYS WARRANTY SERVICE SUPPORT

The Image-I Adapter/A always fills the screen with 1600 x 1200 pels. The 1360 x 1024 and 1024 x 768 are just windows within this. The 640 x 480 mode is pel doubled to look like 1280 x 960.

Withdrawn from marketing I =Interlaced; NI = Non-interlaced Price decrease effective June 15, 1994

The resolution, vertical refresh rate, and maximum shades of grey are controlled by a combination of the video controller, device driver, and display.

Note 2: Monochrome displays have no shadow mask and therefore no dot pitch. The gun design determines differences in screen quality.

Monochrome displays do not have or need degauss as there is no metal in the tube to become magnetized.

Analog = knobs / thumbwheel; Digital = pushbuttons

85xx also have 720 x 350 and 720 x 400 text modes at 70 Hz (NI).

The 9504 requires the IBM^® Image-I Adapter/A. A special connector is used to make it plug only into this adapter.

The 9504 is specifically designed for the Image Plus market to run at 1600 x 1280 resolution. If used in any other resolution than 1600 x 1280 there will be a reduction in picture size in accordance with the following table:

1600 x 1280 = 370 x 296 mm 1360 x 1024 = 315 x 237 mm 1024 x 768 = 237 x 178 mm 640 x 480 = 296 x 222 mm