8640-0Nx 0N0 0NJ None 728 MB IDE N/A 12 ms $ 2,499 $ 3,099 June 1994 June 1994

486DX2 - 66/33 MHz IntelDX4 at 100/33 MHz P24T (Intel^® Pentium™ OverDrive™ ) Remove standard CPU from 237 pin ZIF socket (Intel^® Socket 3)

256 KB / 256 KB 256 KB / 512 KB Soldered DIP modules All: Write-back (organization: direct mapped; 15 ns)

8 MB / 128 MB 4 sockets / 2 available All: 70 ns / 72 pin All: 70 ns speed only (supports 4, 8, 16, 32 MB parity SIMMs) All: Parity / all memory must be installed in matched pairs / all memory addressable by DMA Matched pairs reqd due to interleaved memory

Enhanced IDE on PCI bus (2 drops)

PIO modes 0, 1, 2, 3 Enhanced IDE on ISA bus

(2 drops) PIO modes 0, 1, 2

All: 11 MB/sec across Enhanced IDE interface (16 bit) if used with Mode 3 disks

Mode 0 = 3.3 MB/sec / Mode 1 = 5.2 MB/sec / Mode 2 = 8.3 MB/sec / Mode 3 = 11.1 MB/sec All: Disks greater than 528 MB only support PIO Mode 0 on ISA based IDE controller All: Maximum 10 MB/sec across Fast SCSI bus (8 bit) All: Maximum 132 MB/sec to PCI (32 bit) for Enhanced IDE and SCSI-2 All: Enhanced IDE controller(s) on planar / SCSI-2 Fast Adapter in PCI slot SCSI model: One (maximum of 7 SCSI devices internal or external) All: IDE has no cache / SCSI-2 Fast PCI has no cache (32 byte FIFO buffer)

All: PCI (2 slots) /PCI/EISA shared slot (1 slot) /EISA(5 slots) All: PCI maximum transfer rate is 132 MB/sec; EISA maximum data transfer rate is 33 MB/sec All: 8 slots (all 32 bit) / 6 or 7 slots available (VGA adapter in one slot; 0PT has SCSI-2 in one slot; see below) All: 9 bays / 7 or 8 available (one used for diskette; one used for disk; see diagram below)

All: 3.5" 1.44 MB diskette drive / dust cover / media sense / supports 3.5" 2.88 MB and 5.25" 1.2 MB (2 diskette max) All: Two 9 pin serial port / DMA support / UART 16550A / 115.2 Kbps maximum supported speed All: One parallel port / DMA support / bidirectional / supports ECP/EPP protocols adhering to IEEE 1284 standard

All: VGA / Cirrus Logic™ (adapter is a dumb frame buffer) All: ISA / 16 bit (in 32 bit EISA adapter slot) / 512 KB DRAM memory

All: Power switch behind door / selectable boot (A: and C: only) / keyboardless and displayless operation All: No (because power switch behind locked door) All: Front door keylock (no keylock to lock system cover) All: Yes

All: None (no operating system ships standard) / fast startup mode All: 128 KB in Flash EEPROM on the planar board (Phoenix™ BIOS) / upgrades free of charge (via diskette) All: IBM Quiet (rubber dome) 101 key / no mouse ships standard All: 300 watt / universal / manual switch setting / built in overload, surge protection All: QAPlus/PRO ships standard / Optional NetFinity™ software

8640-0Px 0P0 0PT None 1 GB SCSI-2 Fast N/A 8.6 ms $ 3,899 $ 4,999 June 1994 June 1994

Pentium - 60 MHz P5T (Pentium OverDrive)

Remove standard CPU from 273 pin ZIF socket

Upgrade to 512 KB via 8 DIP modules

16 MB / 192 MB 6 sockets / 4 available

Matched pairs required due to 64 bit path to memory

SCSI-2 Fast Adapter on PCI bus

Enhanced IDE on ISA Enhanced IDE on ISA (2 drops) (2 drops) PIO modes 0, 1, 2 PIO modes 0, 1, 2

Type Models Disk - individual size Disk - speed Price (retail USD) Available date

Processor / MHz Processor upgrade(s)

Upgrade method

L2 cache - std / max L2 cache - method L2 cache - write policy

Memory - std / max Mem - total sockets / avail Memory - speed / pins Mem - supported SIMMs Memory - type Memory

Disk controllers

Controller transfer rates

Controller implementation SCSI controller channels Cntrllr cache - std / max

Architecture Architecture features 32 bit slots / available Bays / available

Diskette drive Serial port Parallel port

Video - controller / vendor Video - arch / data path

Security Power-on password Cover key lock U Bolt support

Preloaded software BIOS Keyboard / mouse Power supply Systems management

IBM PC Server (PCI/EISA Server)

All trademarks are the property of their respective owners (listed on Trademark sheet) No warranties are expressed or implied in this summary (PCSERV) Compiled by Roger Dodson, IBM. May 1994

IBM^® PC Server: PC Server PC Server

Supports 640 x 480 with 256 colors or 800 x 600 with 16 colors

std disk

(access)

(access)

(access)

(access)

(access)

(access)

(access) for diskette only

(access)

(no access)

PC SERVER BAYS

or Full Height or Full Height

diskette

Optional diskette/tape

HH HH HH HH HH HH SL SL SL

5.25"

5.25"

5.25"

5.25"

5.25"

5.25"

3.5"

3.5"

3.5"

FH: Full Height bay (up to 3.2") HH: Half Height bay (up to 1.6") SL: Slim Line bay (up to 1") or Half Height

Slot 1: fullsize, 32 bit PCI Slot 2: fullsize, 32 bit PCI Slot 3: fullsize, 32 bit PCI or EISA or 16 bit ISA Slot 4: fullsize, 32 bit EISA or 16 bit ISA Slot 5: fullsize, 32 bit EISA or 16 bit ISA Slot 6: fullsize, 32 bit EISA or 16 bit ISA Slot 7: fullsize*,32 bit EISA or 16 bit ISA Slot 8: fullsize*,32 bit EISA or 16 bit ISA

(Slot 3: occupied by PCI SCSI-2 Adapter in model 0PT) (Slot 4: occupied by VGA adapter) (* = Pentium models support halfsize adapters)

FloThru™ air flow design utilizing two fans, a heat sensing speed control, and full length front venting to allow electronics and drive components to run cooler for longer life

EISA Configuration Utility is on the EISA Configuration Diskette

CTRL+ALT+S = Setup Utility at startup or within any application

The IBM PC Server does NOT have: - ECC memory - Plug-n-play support - 3 MB system partition - Vital Product Data - Tamper evident cover - Privileged access psswrd

PC SERVER WARRANTY SERVICE SUPPORT

3 year warranty On site warranty all 3 years All cities in all states 8 am - 5 pm Mon - Fri coverage Next day response time Option to upgrade warranty to:

24 hr / 7 day coverage, 4 hr response for $40 per year 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM or dealer warranty/service 30 day money back guarantee

All: Maximum internal disk capacity: If have SCSI-2 adapter: 14 GB with seven 2 GB SCSI-2 disks;

486DX2 models allow four 1 GB IDE for a max of 4 GB (SCSI optional)

QAPlus/PRO™ is graphical software for diagnostic and testing included with PC Server