53 53 53 LS 53 LS

56 SLC2 56 SLC2

56 SLC3 56 SLC3 56 SLC3 56 LS 56 LS

57 SLC2 57 SLC2 57 SLC2

57 SLC3 57 SLC3 57 SLC3 57 SLC3 M57 M57 M57 M57 76 486 76 486

77 486 77 486

77 486DX2 77 486DX2

90 XP 90 XP

486SLC2 at 50/25 MHz

486SLC2 at 50/25 MHz

486SLC3 at 75/25 MHz " 486SLC2 at 50/25 MHz

486SLC3 at 75/25 MHz

486SLC3 at 75/25 MHz

486SX at 33 MHz

486SX at 33 MHz

486DX2 at 66/33 MHz

486DX2 at 50/25 MHz

9553-0B7

-0BB " -1BX " -2BX

9556-DB6 " -DBA

9556-DE9

-DEB " -DED " -1EX " -2EX

9557-DB6

-DBA " -DBG

9557-DE9

-DEB " -DED " -DEG

9557-6EB

-7EB " -6EG " -7EG

9576-DU6 " -DUA

9577-DUA " -DUG

77-DNA 77-DNG

9590-DLA

-DLG

Type-model

IBM PS/2 Desktop

Diskette Disk: std-max internal ms seek / interface

Available date 93 93 93 93 93 93 94 94 94 94 94 93 93 93 94 94 94 94 94 94 94 94 93 93 93 93 93 93 93 93

CPU / /

Speed MHz Upgrade MHz IBM^® PS/2^® : Nov Nov Nov Nov Aug Aug Feb Feb Feb Feb Feb Aug Aug Aug Feb Feb Feb Feb Mar Jun Mar Jun Aug Aug Aug Aug Aug Aug Aug Aug

SUP^1

Total bays

Slots available 16+32 bit Std features

Video; std/max memory

L2 cache std / max

Memory in MB; std / max

d 120M-1.05G14 IDE d 250M-1.05G14 IDE Opt: 1 diskette, 2 IDE Opt: 1 diskette, 2 IDE

D104M-2.0G 12 scsi D208M-2.0G 12 scsi

D170M-2.0G 13 scsi D245M-2.0G 16 scsi D340M-2.0G 14 scsi Opt: 2 diskette, 2 scsi Opt: 2 diskette, 2 scsi

D104M-6.0G 12 scsi D208M-6.0G 12 scsi D540M-6.0G 10 scsi

D170M-6.0G 13 scsi D245M-6.0G 16 scsi D340M-6.0G 14 scsi D540M-6.0G 10 scsi

D245M-6.0G 16 scsi D245M-6.0G 16 scsi D540M-6.0G 10 scsi D540M-6.0G 10 scsi

D104M-2.0G 12 scsi D208M-2.0G 12 scsi

D208M-6.0G 12 scsi D540M-6.0G 10 scsi

D208M-6.0G 12 scsi D540M-6.0G 10 scsi

D208M-4.54G12 SCSI D540M-4.54G10 SCSI m/k m/k m/k Ethernet m/k Token-Ring m/K m/K m/K m/K m/K m/K Ethernet m/K Token-Ring m/K m/K m/K m/K m/K m/K m/K m/KCD/Audiv/W m/KCD/Audiv/2 m/KCD/Audiv/W m/KCD/Audiv/2 m/K m/K m/K m/K m/K m/K m/K/U m/K/U

0KB/0KB " " " " 0 /0 " " 0 /0 " " " " " " 0 /0 " " 0 /0 " " " " 0 /0 " " " " 0 /0 " " 0 /0 " " 0 /0 " " 0 /0

4 /16 4 /16 4 /16 4 /16

8 /16 8 /16

8 /16 " 4 /16 4 /16

8 /16 8 /16 8 /16

8 /16 8 /16 8 /16 8 /16

8 /16 8 /16 8 /16 8 /16

8 /32 8 /32

8 /32 8 /32

8 /32 8 /32

8 /64 8 /64

SVGA GD5426 1 MB

XGA-2 1 MB

XGA-2 1 / 1 MB " " XGA-2 1 MB " XGA-2 1 MB " XGA-2 1 MB " XGA-2 1 MB

XGA-2 1 MB

XGA-2 1 MB

XGA-2 1 MB

3+0 3+0 2+0 2+0

3+0 3+0

3+0 " 2+0 2+0

5+0 5+0 5+0

5+0 5+0 5+0 5+0

4+0 4+0 4+0 4+0

0+2 0+2

0+4 0+4

0+4 0+4

0+2 0+2

3 3 3 3 3 3 3 " 3 3 4 4 4 4 4 4 4 4 4 4 4 3 3 4 4 4 4 4 4

1460 1625 1335 1700

2065 2335

2300 2435 2535 1865 2200

2200 2465 2865

2465 2600 2700 3065

3465 3465 3935 3935

2435 2700

2835 3435

3365 3965

3535 4135

$

PS/2 FEATURES

Micro Channel^® Architecture 32 bit adapters (Models 76, 77, 90) Performance (20 MB/sec data transfer) Automatic configuration (no switches, jumpers) Multiple busmaster support (high throughput) Parity memory 70 ns memory speed standard All memory on planar; 72 pin SIMMs Extensive embedded diagnostics Selectable boot capability 32 bit XGA-2^® graphics busmaster or SVGA 640x480, 800x600, 1024x768, 1280x1024 ISO 9241-3 compliant Busmaster 16/32 bit SCSI (vs slave 16 bit IDE) Maximum total disk capacity (internal and external) about 54 GB w/ IBM 2.0 GB disks Cover key lock (unique for every PS/2) U-bolt holes to lock to furniture 2.88 MB diskette drive with media sense Choice of 84, 101, or 122 keyboards IBM mouse included Numerous hard copy documentation High parts availability; high resale value 24 hr/day support via fax (1-800-426-3395), bulletin board (1-404-835-6600), and phone (HelpWare at 1-800-772-2227)

MODELS 53, 56, 57, 76, 77and 90

Choice of operating system:

IBM OS/2^® 2.1 IBM OS/2 2.00.1 IBM DOS 6.1 / Windows™ 3.1 IBM DOS 5.02/ Windows 3.1

Includes all software publications and all diskettes (op sys is not preinstalled); 53 LS and 56 LS do not include op sys

3 year warranty On site warranty all 3 years All cities in all states 24 hour / 7 day service coverage 4 hour response time 24 hour / 7 day telephone support 24 hour / 7 day bulletin board 24 hour / 7 day fax support IBM or dealer warranty/service 30 day money back guarantee

PS/2 WARRANTY SERVICE SUPPORT

scsi = 16 bit SCSI-1 busmaster on planar SCSI = 32 bit SCSI-1 busmaster on planar SCSI = 32 bit SCSI-1 busmaster adapter

Note 1: Price (retail USD) Note 2: P24T: Intel Pentium OverDrive (in 1994)

Micro Channel architecture Products announced February 1, 1994 or later Systems withdrawn Price decrease effective February 1, 1994 Price decrease effective February 2, 1994

No warranties are expressed in this summary. (PS2) Compiled by Roger Dodson, IBM

all: none

all: 486SLC3 at 75/25

Current as of February 23, 1994 all:

486SLC3 at 75/25

all: none

all: none

all: 486DX2-66 P24T ^{(2)}

all: 486DX-50 486DX2-66 Pentium-60 all: none

Audiv = 16 bit sound adapter (Audiovation) CD = CD-ROM/XA (double speed) d = 1.44 MB 3.5" diskette drive D= 2.88 MB 3.5" diskette drive with media sense E = 10 Mbps Ethernet adapter 10BaseT K= Choice of 84, 101 or 122 host key keyboard k = Choice of Enhanced or Quiet 101 keyboard K = Choice of Enhanced or Quiet 101 keyboard with mouse or Enhanced 101 key with TrackPoint II or Quiet Touch 84 key with TrackPoint II (TrackPoint II keyboards available 1H94 at additional cost) m= PS/2 mouse T = 16/4 Mbps Token-Ring Adapter U= Upgradeable processor, memory controller, DMA, L2 cache, and Micro Channel (I/O) controller W=DOS 6.1/Windows 3.1 preinstalled 2 = OS/2 2.1 preinstalled 256 = (italics) write-back L2 cache 256 = (no italics) write-through L2 cache