4 /64 4 /64 8 /64 4 /64 8 /64

4 /64 4 /64 8 /64 4 /64 8 /64

4 /64 4 /64 8 /64 8 /64 4 /64 8 /64

4 /64 4 /64 4 /64 8 /64 8 /64

4 /64 4 /64 8 /64 4 /64 8 /64

4 /64 4 /64 8 /64 8 /64

4 /64 4 /64 8 /64 4 /64 8 /64

4 /64 4 /64 8 /64 8 /64

16 /128 8 /128 8 /128 16 /128 16 /128

5/1 " " " 5/1 " " " 5/1 " " " " 8/1 " " " 5/1 " " " 8/1 " " 5/1 " " " 8/1 " " 3/0 3/0 3/0 3/0 3/0 4 total slots: 1 PCI, 1 PCI/ISA, 2 ISA

S/s/P S/s/P /9 S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /1 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /9 S/s/P /1

S/s/P S/s/P /9 S/s/P /9 S/s/P /1

S/S/P S/S/P S/S/P S/S/P S/S/P

4 options for all: 486DX-33 486DX2-50/25 486DX2-66/33 P24T (238 pin)

4 options listed above

3 options for all: 486DX-33 486DX2-66/33 P24T (238 pin)

3 options for all: 486DX-33 486DX2-66/33 P24T (238 pin)

2 options for all: 486DX2-66/33 P24T (238 pin)

2 options for all: 486DX2-66/33 P24T (238 pin)

1 option for all: P24T (238 pin)

1 option for all: P24T (238 pin)

1 option for all: future

OverDrive™ (273 pin)

S3-805 local bus 1 / 2 MB " S3-805 local bus 1 / 2 MB " S3-805 local bus 1 / 2 MB " " S3-805 local bus 1 / 2 MB " S3-805 local bus 1 / 2 MB " S3-805 local bus 1 / 2 MB

S3-805 local bus 1 / 2 MB " S3-805 local bus 1 / 2 MB

68800AX PCI local 1 / 2 MB

�““ �“ �“ �“ �“ �““ �“ �“ �“ �“ �““ �“ �“ �“ �“ �“ �“@“ �@“ �@“ �@“ �@“ �““ �“ �“ �“ �“ �“@“ �@“ �@“ �@“ �““ �“ �“ �“ �“ �“@“ �@“ �@“ �@“ �“ �“ �“ �“ �“

@@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@ @@

0KB256 " " " " " " 0 256 " " " " " " 0 256 " " " " " " " " 0 256 " " " " " " 128 256 " " " " " " 128 256 " " " " 128 256 " " " " " " 128 256 " " " " 256 256 256 256 256 256 256 256 256 256

6384-G00 -G40 " -G41 " -G50 " -G53

6384-L00 -L40 " -L41 " -L50 " -L53

6384-N00 -N50 " -N51 " -N53 " -N70 " -N73

6387-N00 -N50 " -N70 " -N71 " -N73

6384-V00 -V50 " -V51 " -V70 " -V73

6387-V00 -V50 " -V81 " -V83

6384-X00 -X50 " -X51 " -X70 " -X73

6387-X00 -X70 " -X91 " -X93

6384-189 6384-193 6384-1A3 6384-199 6384-1A9

IBM ValuePoint - Fall 1993 models / P60/D

ValuePoint Type-model

Diskette Disk: std-max internal ms seek / interface CPU MHz Upgrade MHz / IBM Direct Price ^1

Available date

Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Oct Feb Jul Oct Jul

93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 93 94 94 94 94

425SX/D 425SX/D 425SX/D 425SX/D 425SX/D

433SX/D 433SX/D 433SX/D 433SX/D 433SX/D

433DX/D 433DX/D 433DX/D 433DX/D 433DX/D 433DX/D

433DX/T 433DX/T 433DX/T 433DX/T 433DX/T

450DX2/D 450DX2/D 450DX2/D 450DX2/D 450DX2/D

450DX2/T 450DX2/T 450DX2/T 450DX2/T

466DX2/D 466DX2/D 466DX2/D 466DX2/D 466DX2/D

466DX2/T 466DX2/T 466DX2/T 466DX2/T

P60/D P60/D P60/D P60/D P60/D

486SX at 25 MHz " 486SX at 33 MHz " 486DX at 33 MHz " " 486DX at 33 MHz " 486DX2 at 50/25 " 486DX2 at 50/25

486DX2 at 66/33 " 486DX2 at 66/33

Pentium at 60 MHz

IBM^® ValuePoint™:

L2 cache std / max

Memory in MB; std / max all 70 ns

SVGA controller; memory std / max

d Opt: up to 2 IDE d 170M-1.05G14 IDE d 170M-1.05G14 IDE d 245M-1.05G14 IDE d 245M-1.05G14 IDE

d Opt: up to 2 IDE d 170M-1.05G14 IDE d 170M-1.05G14 IDE d 245M-1.05G14 IDE d 245M-1.05G14 IDE

d Opt: up to 2 IDE d 212M-1.05G13 IDE d 212M-1.05G13 IDE d 212M-1.05G13 IDE d 340M-1.05G14 IDE d 340M-1.05G14 IDE

d Opt: up to 2 IDE d 212M-1.05G13 IDE d 340M-1.05G14 IDE d 340M-1.05G14 IDE d 340M-1.05G14 IDE

d Opt: up to 2 IDE d 212M-1.05G13 IDE d 212M-1.05G13 IDE d 340M-1.05G14 IDE d 340M-1.05G14 IDE

d Opt: up to 2 IDE d 212M-1.05G13 IDE d 424M-1.05G14 IDE d 424M-1.05G14 IDE

d Opt: up to 2 IDE d 212M-1.05G13 IDE d 212M-1.05G13 IDE d 340M-1.05G14 IDE d 340M-1.05G14 IDE

d Opt: up to 2 IDE d 340M-1.05G14 IDE d 527M-1.05G 9 IDE d 527M-1.05G 9 IDE

d 424M-1.05G13 IDE d 527M-1.05G 9 IDE d 527M-1.05G12 IDE d 527M-1.05G 9 IDE d 527M-1.05G12 IDE

Slots available 16 bit/32 bit VL-Bus

↓^{Total bays}

3.5" | 5.25"

$

Std features

1000 1170 1370 1280 1480

1030 1200 1400 1310 1510

1380 1550 1750 1750 1660 1860

1500 1670 1780 1980 1980

1370 1540 1740 1650 1850

1490 1660 2100 2100

1790 1960 2160 2070 2270

1900 2190 2530 2530

3170 2860 2860 3320 3320

VALUEPOINT FEATURES (FALL 1993 MODELS)

ISA architecture (AT bus) 1 available 32 bit VESA local bus slot 238 pin ZIF socket (upgrades) Write-back L2 cache controller All memory on planar (local bus) Parity memory 4 SIMM sockets - 72 pin SIMMs Standard memory uses only one socket

SVGA video (up to 1280 x 1024) VESA local bus 32 bit graphics accelerator 86C805 allows 2 MB video

memory IBM mouse (except LAN diskless) IBM Enhanced 101 keyboard 128 KB flash mem for BIOS/POST 200 watt power supply Many security features

d =1.44 MB 3.5" diskette drive P =DMA parallel port

P =DMA parallel port ECP 2-5 MB/sec s =Async port (19.2 KBps)UART16450

S =Async port (56 KBps) UART16550A S =DMA async (345 KBps)UART16550A

1 =OS/2^® 2.1 preinstalled 9 =DOS 6.1 & Windows™ 3.1 preinstalled

128 256 = (italics) write-back L2 cache 128 = (not italic) write-thru L2 cache SIMM

Si= SpaceSaver Introductory 3/3; 6381

/S = SpaceSaver (3 slts x 3 bays); 6382 /D= DeskTop (5 slots x 5 bays); 6384

/T = Mini-Tower (8 slots x 6 bays);6387

VALUEPOINT WARRANTY SERVICE SUPPORT

1 year warranty

On site warranty all year

All cities in all states

8 am - 5 pm Mon - Fri coverage

Next day response time

Optional warranty: 4 hour

response, 24 hr / 7 day coverage

Post warranty: 2 options above

24 hour / 7 day telephone support

24 hour / 7 day bulletin board

24 hour / 7 day fax support

IBM or dealer warranty/service

30 day money back guarantee

MULTIMEDIA VALUEPOINT (MVP Series)

The following models are available as preconfigured multimedia units withdouble speed CD-ROM/XAand Creative Labs Sound Blaster ™ 16 audio adapter. Additional peripherals and software are available in three configurations: Office, Reference, or Entertainment.

ValuePoint listed above Office Reference Entertainment

6384-G40 GS1 GS4 GS7 6384-L40 LS1 LS4 LS7 6384-N50 NS2 NS5 NS8 6384-V50 VS2 VS5 VS8 6384-X70 XS3 XS6 XS9

See MVP93F sheet for details on multimedia models.

� bay occupied by standard diskette

or hard disk.

“ open bay with NO front

media access.

@ open bay with front media access.

Multimedia models available.

Price decrease effective July 13, 1994.

Announced July 12, 1994

Systems withdrawn

Note 1: Dealer prices will vary.

No warranties are expressed or implied in this summary.

(VP93F) Compiled by Roger Dodson, IBM Current as of July 14, 1994

Models announced October 18, 1993 or July 5, 1994: