* * * * * * * * * * * * A T T E N T I O N * * * * * * * * * * * *

The memory part numbers which GURU generates for this record are for standard non-parity DIMMs. Standard DIMMs work but run slower than parity DIMMs. If you wish to use parity DIMMs please use the following substitution table:

32MB DIMM      (standard)=7DM32M/64B-60S      (parity)=7DM32P6FX1 
64MB DIMM      (standard)=7DM64M/64B-60S      (parity)=7DM64P6FX1 
128MB DIMM    (standard)=7DM128M/64B-60S    (parity)=7DM128P6FX1 

SCSI: DB-25
Serial Ports: 2
Sound Output: stereo 16 bit.
ADB: 1
Ethernet: AAUI
Machine Gestalt ID: n/a
PRAM Battery: 3.6V lithium (Maxell ER3S, Radio Shack 23-026)

Minutiae:

Upgraded with one DIMM at a time.

Can interleave memory for approximately 10-30% faster RAM access.  For the fastest speed, sockets A1 & B1, A2 & B2...A4 & B4 should contain identical capacity DIMMs.

Serial Port with the phone icon supports synchronous modems, with handshaking on both output and input supported.