There are four 1MB VRAM DIMM sockets configured as two 2MB banks.
-- 1 Bank (2MB)
-- 2 Banks (4MB).

This computer has a built-in Video input capability for display (up to 24 bpp and up to 640 by 480 pixels at 30 frames per second), frame capture, or QuickTime movie capture.

This computer does not support Dual-stream Video output.  Dual-stream Video output enables a computer to display computer graphics and transmit video output at the same time. In this computer the graphics display goes blank when it is transmitting video output.

This computer has a built-in DAV slot for use by an optional digital video processor in a PCI expansion slot.