SCSI: DB-25
Serial Ports: 2
Sound Output: 16-bit stereo 44.1 KHz sample rate
ADB: 1, plus additional port for PS/2 keyboard
Ethernet:  10BaseT
Machine Gestalt ID: ???
PRAM Battery: 4.5V alkaline (Rayovac 840)

Minutiae:

Some low-end models have only 256 KB of level-2 cache.  Improve performance by installing a Newer Technology 512 KB level-2 cache DIMM, part # 7CC512C.

All models are based on the Tanzania logic board, which was co-developed by Apple and Motorola.

Supports only 3.3 volt EDO DIMMs.  It does not support interleaved memory.  The three DIMM sockets are NOT identical.  The first socket can only accept up to 32 MB DIMMs.  The other two sockets can accept up to 64 MB DIMMs.  The maximum memory is therefore 160 MB.

Manufactured by: 

Vertegri Research
a division of Paul Gossen Consulting Inc.
300 - 341 Water Street
Vancouver B.C. V6B 1B9
Canada

Voice: 604-688-6792
Toll Free: 800-622-9611
Fax: 604-687-6577