Supported Systems Software: 7.5.3
SCSI: DB-25
Serial Ports: 2
Sound Output: 16-bit stereo 44.1 KHz sample rate
ADB: 1, plus additional port for PS/2 keyboard
Ethernet:  Add-in card
Machine Gestalt ID: ??

Minutiae:

PowerBase can take only EDO DIMMs.  It does not support interleaved memory.  The three DIMM sockets are NOT identical.  The first socket, which comes stock with a 16 MB DIMM installed, can only accept up to 32 MB DIMMs.  The other two sockets can accept up to 64 MB DIMMs.  The maximum memory is therefore 160 MB.

PowerBase has a socketed CPU daughter card which can be upgraded. No specifics on upgrades or upgradeability for PowerBase are available at this time.

Each PowerBase system comes with 16MB RAM, a 1.2GB IDE hard drive, 8x CD-ROM, 2MB IDO DRAM for graphics, and a 256K Level-2 Cache.

Manufactured by:
Power Computing Corporation
1-800-769-5917
info@powercc.com
http://www.powercc.com