; PSPad clip definition file for Ansys 7.0
; author:  Novotny L. W., www.TOSHULIN.cz
; last revision 31. 12. 2003  21:01
;
[*ABBR | Defines an abbreviation.]
*ABBR,Abbr,String 
[*AFUN | Specifies units for angular functions in parameter expressions.]
*AFUN,Lab 
[*ASK | Prompts the user to input a parameter value.]
*ASK,Par,Query,DVAL 
[*CFCLOS |"Closes the""command""file."]
*CFCLOS 
[*CFOPEN |"Opens a""command""file."]
*CFOPEN,Fname,Ext,--,Loc 
[*CFWRITE |"Writes an ANSYS command (or similar string) to a""command""file."]
*CFWRITE,Command 
[*CREATE | Opens (creates) a macro file.]
*CREATE,Fname,Ext,-- 
[*CYCLE | Bypasses commands within a do loop.]
*CYCLE 
[*DEL | Deletes a parameter or parameters (GUI).]
*DEL,Val1,Val2 
[*DIM | Defines an array parameter and its dimensions.]
*DIM,Par,Type,IMAX,JMAX,KMAX,Var1,Var2,Var3 
[*DO | Defines the beginning of a do loop.]
*DO,Par,IVAL,FVAL,INC 
[*ELSE | Separates the final if then else block.]
*ELSE 
[*ELSEIF | Separates an intermediate if then else block.]
*ELSEIF,VAL1,Oper,VAL2 
[*END | Closes a macro file.]
*END 
[*ENDDO | Ends a do loop and starts the looping action.]
*ENDDO 
[*ENDIF | Ends an if then else.]
*ENDIF 
[*EVAL | Evaluates hyperelastic constants.]
*EVAL,ETYPE,EVPARM,CONST,XMIN,XMAX,XVAL,ECALC 
[*EXIT | Exits a do loop.]
*EXIT 
[*GET | Retrieves a value and stores it as a scalar parameter or part of an array parameter.]
*GET,Par,Entity,ENTNUM,Item1,IT1NUM,Item2,IT2NUM 
[*GO | Causes a specified line on the input file to be read next.]
*GO,Base 
[*IF | Conditionally causes commands to be read.]
*IF,VAL1,Oper1,VAL2,Base1,VAL3,Oper2,VAL4,Base2 
[*LIST | Displays the contents of an external,coded file.]
*LIST,Fname,Ext,-- 
[*MFOURI | Calculates the coefficients for,or evaluates,a Fourier series.]
*MFOURI,Oper,COEFF,MODE,ISYM,THETA,CURVE 
[*MFUN | Copies or transposes an array parameter matrix.]
*MFUN,ParR,Func,Par1 
[*MOONEY | Calculates Mooney Rivlin hyperelastic constants from test data.]
*MOONEY,STRAIN,STRESS,--,CONST,CALC,SORTSN,SORTSS,Fname,Ext 
[*MOPER | Performs matrix operations on array parameter matrices.]
*MOPER,ParR,Par1,Oper,Par2,Par3,kDim,Ratio,kOut 
[*MSG | Writes an output message via the ANSYS message subroutine.]
*MSG,Lab,VAL1,VAL2,VAL3,VAL4,VAL5,VAL6,VAL7,VAL8 
[*MWRITE | Writes a matrix to a file in a formatted sequence.]
*MWRITE,ParR,Fname,Ext,--,Label,n1,n2,n3 
[*REPEAT | Repeats the previous command.]
*REPEAT,NTOT,VINC1,VINC2,VINC3,VINC4,VINC5,VINC6,VINC7,VINC8,VINC9,VINC10,VINC11 
[*SET | Assigns values to user named parameters.]
*SET,Par,VALUE,VAL2,VAL3,VAL4,VAL5,VAL6,VAL7,VAL8,VAL9,VAL10 
[*STATUS | Lists the current parameters and abbreviations.]
*STATUS,Par,IMIN,IMAX,JMIN,JMAX,KMIN,KMAX 
[*TOPER | Operates on table parameters.]
*TOPER,ParR,Par1,Oper,Par2,FACT1,FACT2,CON1 
[*TREAD | Reads data from an external file into a table array parameter.]
*TREAD,Par,Fname,Ext,--,NSKIP 
[*ULIB | Identifies a macro library file.]
*ULIB,Fname,Ext,-- 
[*USE | Executes a macro file.]
*USE,Name,ARG1,ARG2,ARG3,ARG4,ARG5,ARG6,ARG7,ARG8,ARG9,AR10,AR11,AR12,AR13,AR14,AG15,AR16,AR17,AR18
[*VABS | Applies the absolute value function to array parameters.]
*VABS,KABSR,KABS1,KABS2,KABS3 
[*VCOL | Specifies the number of columns in matrix operations.]
*VCOL,NCOL1,NCOL2 
[*VCUM | Allows array parameter results to add to existing results.]
*VCUM,KEY 
[*VEDIT | Allows numerical array parameters to be graphically edited.]
*VEDIT,Par 
[*VFACT | Applies a scale factor to array parameters.]
*VFACT,FACTR,FACT1,FACT2,FACT3 
[*VFILL | Fills an array parameter.]
*VFILL,ParR,Func,CON1,CON2,CON3,CON4,CON5,CON6,CON7,CON8,CON9,CON10
[*VFUN | Performs a function on a single array parameter.]
*VFUN,ParR,Func,Par1,CON1,CON2,CON3 
[*VGET | Retrieves values and stores them into an array parameter.]
*VGET,ParR,Entity,ENTNUM,Item1,IT1NUM,Item2,IT2NUM,KLOOP 
[*VITRP | Forms an array parameter by interpolation of a table.]
*VITRP,ParR,ParT,ParI,ParJ,ParK 
[*VLEN | Specifies the number of rows to be used in array parameter operations.]
*VLEN,NROW,NINC 
[*VMASK | Specifies an array parameter as a masking vector.]
*VMASK,Par 
[*VOPER | Operates on two array parameters.]
*VOPER,ParR,Par1,Oper,Par2,CON1,CON2 
[*VPLOT | Graphs columns (vectors) of array parameters.]
*VPLOT,ParX,ParY,Y2,Y3,Y4,Y5,Y6,Y7,Y8 
[*VPUT | Restores array parameter values into the ANSYS database.]
*VPUT,ParR,Entity,ENTNUM,Item1,IT1NUM,Item2,IT2NUM,KLOOP 
[*VREAD | Reads data and produces an array parameter vector or matrix.]
*VREAD,ParR,Fname,Ext,--,Label,n1,n2,n3,NSKIP 
[*VSCFUN | Determines properties of an array parameter.]
*VSCFUN,ParR,Func,Par1 
[*VSTAT | Lists the current specifications for the array parameters.]
*VSTAT 
[*VWRITE | Writes data to a file in a formatted sequence.]
*VWRITE,Par1,Par2,Par3,Par4,Par5,Par6,Par7,Par8,Par9,Par10,Par11,Par12,Par13,Par14,Par15,Par16,Par17,Par18,Par19
[/AN3D | Specifies 3 D annotation functions]
/AN3D,Kywrd,KEY 
[/ANFILE | Saves or resumes an animation sequence to or from a file.]
/ANFILE,LAB,Fname,Ext,-- 
[/ANGLE | Rotates the display about an axis.]
/ANGLE,WN,THETA,Axis,KINCR 
[/ANNOT | Activates graphics for annotating displays (GUI).]
/ANNOT,Lab,VAL1,VAL2 
[/ANUM | Specifies the annotation number,type,and hot spot (GUI).]
/ANUM,NUM,TYPE,XHOT,YHOT 
[/ASSIGN | Reassigns a file name to an ANSYS file identifier.]
/ASSIGN,Ident,Fname,Ext,-- 
[/AUTO |"Resets the focus and distance specifications to""automatically calculated."""]
/AUTO,WN 
[/AUX12 | Enters the radiation processor.]
/AUX12 
[/AUX15 | Enters the IGES file transfer processor.]
/AUX15 
[/AUX2 | Enters the binary file dumping processor.]
/AUX2 
[/AUX3 | Enters the results file editing processor.]
/AUX3 
[/AXLAB | Labels the X and Y axes on graph displays.]
/AXLAB,Axis,Lab 
[/BATCH |"Sets the program mode to""batch."""]
/BATCH,Lab 
[/CFORMAT | Controls the graphical display of alphanumeric character strings for parameters,components,assemblies,and tables.]
/CFORMAT,NFIRST,NLAST 
[/CLABEL | Specifies contour labeling.]
/CLABEL,WN,KEY 
[/CLEAR | Clears the database.]
/CLEAR,Read 
[/CLOG | Copies the session log file to a named file.]
/CLOG,Fname,Ext,-- 
[/CMAP | Changes an existing or creates a new color mapping table.]
/CMAP,Fname,Ext,--,Kywrd,NCNTR 
[/COLOR | Specifies the color mapping for various items.]
/COLOR,Lab,Clab,N1,N2,NINC 
[/COM | Places a comment in the output.]
/COM,Comment 
[/CONFIG | Assigns values to ANSYS configuration parameters.]
/CONFIG,Lab,VALUE 
[/CONTOUR | Specifies the uniform contour values on stress displays.]
/CONTOUR,WN,NCONT,VMIN,VINC,VMAX 
[/COPY | Copies a file.]
/COPY,Fname1,Ext1,--,Fname2,Ext2,-- 
[/CPLANE | Specifies the cutting plane for section and capped displays.]
/CPLANE,KEY 
[/CTYPE | Specifies the type of contour display.]
/CTYPE,KEY,DOTD,DOTS,DSHP,TLEN 
[/CVAL | Specifies non uniform contour values on stress displays.]
/CVAL,WN,V1,V2,V3,V4,V5,V6,V7,V8 
[/CWD | Changes the current working directory.]
/CWD,DIRPATH 
[/CYCEXPAND | Graphically expands displacements,stresses and strains of a cyclically symmetric model.]
/CYCEXPAND,WN,OPTION,Value1,Value2 
[/DELETE | Deletes a file.]
/DELETE,Fname,Ext,-- 
[/DEVDISP | Controls graphics device options.]
/DEVDISP,Label,KEY 
[/DEVICE | Controls graphics device options.]
/DEVICE,Label,KEY 
[/DIST | Specifies the viewing distance for magnifications and perspective.]
/DIST,WN,DVAL,KFACT 
[/DSCALE | Sets the displacement multiplier for displacement displays.]
/DSCALE,WN,DMULT 
[/DV3D | Sets 3 D device option modes.]
/DV3D,Lab,Key 
[/EDGE |"Displays only the""edges""of an object."]
/EDGE,WN,KEY,ANGLE 
[/EFACET | Specifies the number of facets per element edge for PowerGraphics displays.]
/EFACET,NUM 
[/EOF | Exits the file being read.]
/EOF 
[/ERASE | Specifies that the screen is to be erased before each display.]
/ERASE 
[/ESHAPE | Displays elements with shapes determined from the real constants or section definition.]
/ESHAPE,SCALE 
[/EXIT | Stops the run and returns control to the system.]
/EXIT,Slab,Fname,Ext,-- 
[/EXPAND | Allows the creation of a larger graphic display than represented by the actual finite element analysis model.]
/EXPAND,Nrepeat1,Type1,Method1,DX1,DY1,DZ1,Nrepeat2,Type2,Method2,DX2,DY2,DZ2,Nrepeat3,Type3,Method3,DX3,DY3,DZ3 
[/FACET | Specifies the facet representation used to form solid model displays.]
/FACET,Lab 
[/FDELE | Deletes a binary file after it is used.]
/FDELE,Ident,Stat 
[/FILNAME | Changes the Jobname for the analysis.]
/FILNAME,Fname,Key 
[/FOCUS | Specifies the focus point (center of the window).]
/FOCUS,WN,XF,YF,ZF,KTRANS 
[/FORMAT | Specifies format controls for tables.]
/FORMAT,NDIGIT,Ftype,NWIDTH,DSIGNF,LINE,CHAR 
[/FTYPE | Assigns an external or internal type to a binary file.]
/FTYPE,Ident,Type 
[/GCMD | Controls the type of element or graph display used for the GPLOT command.]
/GCMD,WN,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6,Lab7,Lab8,Lab9,Lab10,Lab11,Lab12 
[/GCOLUMN | Allows the user to apply a label to a specified curve.]
/GCOLUMN,CURVE,STRING 
[/GFILE | Specifies the pixel resolution on Z buffered graphics files.]
/GFILE,SIZE 
[/GFORMAT | Specifies the format for the graphical display of numbers.]
/GFORMAT,Ftype,NWIDTH,DSIGNF 
[/GLINE | Specifies the element outline style.]
/GLINE,WN,STYLE 
[/GMARKER | Specifies the curve marking style.]
/GMARKER,CURVE,KEY,INCR 
[/GO | Reactivates suppressed printout.]
/GO 
[/GOLIST | Reactivates the suppressed data input listing.]
/GOLIST 
[/GOPR | Reactivates suppressed printout.]
/GOPR 
[/GRAPHICS | Defines the type of graphics display.]
/GRAPHICS,Key 
[/GRESUME | Sets graphics settings to the settings on a file.]
/GRESUME,Fname,Ext,-- 
[/GRID | Selects the type of grid on graph displays.]
/GRID,KEY 
[/GROPT | Sets various line graph display options.]
/GROPT,Lab,KEY 
[/GRTYP | Selects single or multiple Y axes graph displays.]
/GRTYP,KAXIS 
[/GSAVE | Saves graphics settings to a file for later use.]
/GSAVE,Fname,Ext,-- 
[/GST | Turns Graphical Solution Tracking (GST) on or off.]
/GST,Lab 
[/GTHK | Sets line thicknesses for graph lines.]
/GTHK,Label,THICK 
[/GTYPE | Controls the entities that the GPLOT command displays.]
/GTYPE,WN,LABEL,KEY 
[/HEADER | Sets page and table heading print controls.]
/HEADER,Header,Stitle,Idstmp,Notes,Colhed,Minmax 
[/ICLWID | Scales the line width of circuit builder icons.]
/ICLWID,FACTOR 
[/ICSCALE | Scales the icon size for elements supported in the circuit builder.]
/ICSCALE,WN,FACTOR 
[/IMAGE | Allows graphics data to be captured and saved.]
/IMAGE,Label,Fname,Ext,-- 
[/INPUT | Switches the input file for the commands that follow.]
/INPUT,Fname,Ext,--,LINE,LOG 
[/INQUIRE | Returns system information to a parameter.]
/INQUIRE,StrArray,FUNC 
[/LARC | Creates annotation arcs (GUI).]
/LARC,XCENTR,YCENTR,XLRAD,ANGLE1,ANGLE2 
[/LIGHT | Specifies the light direction for the display window.]
/LIGHT,WN,NUM,INT,XV,YV,ZV,REFL 
[/LINE | Creates annotation lines (GUI).]
/LINE,X1,Y1,X2,Y2 
[/LSPEC | Specifies annotation line attributes (GUI).]
/LSPEC,LCOLOR,LINSTL,XLNWID 
[/LSYMBOL | Creates annotation symbols (GUI).]
/LSYMBOL,X,Y,SYMANG,SYMTYP,SYMSIZ,KEYBMP 
[/MENU | Activates the Graphical User Interface (GUI).]
/MENU,Key 
[/MPLIB | Sets the default material library read and write paths.]
/MPLIB,R-W_opt,PATH 
[/MREP |"Enables you to reissue the graphics command macro""name""during a replot or zoom operation."]
/MREP,NAME,ARG1,ARG2,ARG3,ARG4,ARG5,ARG6,ARG7,ARG8,ARG9,ARG10,ARG11,ARG12,ARG13,ARG14,ARG15,ARG16,ARG17,ARG18 
[/MSTART | Controls the initial GUI components.]
/MSTART,Label,KEY 
[/NERR | Limits the number of warning and error messages displayed.]
/NERR,NMERR,NMABT,--,IFKEY 
[/NOERASE | Prevents the screen erase between displays.]
/NOERASE 
[/NOLIST | Suppresses the data input listing.]
/NOLIST 
[/NOPR | Suppresses the expanded interpreted input data listing.]
/NOPR 
[/NORMAL | Allows displaying area elements by top or bottom faces.]
/NORMAL,WN,KEY 
[/NUMBER | Specifies whether numbers,colors,or both are used for displays.]
/NUMBER,NKEY 
[/OPT | Enters the design optimizer.]
/OPT 
[/OUTPUT | Redirects text output to a file or to the screen.]
/OUTPUT,Fname,Ext,--,Loc 
[/PAGE | Defines the printout and screen page size.]
/PAGE,ILINE,ICHAR,BLINE,BCHAR 
[/PBC | Shows boundary condition symbols and values on displays.]
/PBC,Item,--,KEY,MIN,MAX,ABS 
[/PBF | Shows magnitude of body force loads on displays.]
/PBF,Item,--,KEY 
[/PCIRCLE | Creates an annotation circle (GUI).]
/PCIRCLE,XCENTR,YCENTR,XLRAD 
[/PCOPY | Automatically generates hard copies for HP Unix work stations.]
/PCOPY,KEY 
[/PDS | Enters the probabilistic design system.]
/PDS 
[/PICE | Shows initial conditions on elements as contours on displays.]
/PICE,Item,--,KEY 
[/PLOPTS | Controls graphics options on subsequent displays.]
/PLOPTS,Label,KEY 
[/PMACRO | Specifies that macro contents be written to the session log file.]
/PMACRO 
[/PMETH | Activates the p method solution options in the Graphical User Interface (GUI).]
/PMETH,Key,OPTION 
[/PMORE | Creates an annotation polygon (GUI).]
/PMORE,--,X5,Y5,X6,Y6,X7,Y7,X8,Y8 
[/PNUM | Controls entity numbering/coloring on plots.]
/PNUM,Label,KEY 
[/POLYGON | Creates annotation polygons (GUI).]
/POLYGON,NVERT,X1,Y1,X2,Y2,X3,Y3,X4,Y4 
[/POST1 | Enters the database results postprocessor.]
/POST1 
[/POST26 | Enters the time history results postprocessor.]
/POST26 
[/PREP7 | Enters the model creation preprocessor.]
/PREP7 
[/PSEARCH |"Specifies a directory to be searched for""unknown command""macro files."]
/PSEARCH,Pname 
[/PSF | Shows surface load symbols on model displays.]
/PSF,Item,Comp,KEY,KSHELL,Color 
[/PSPEC | Creates annotation polygon attributes (GUI).]
/PSPEC,PCOLOR,KFILL,KBORDR 
[/PSTATUS | Displays the global or window display specifications.]
/PSTATUS,WN 
[/PSYMB | Shows various symbols on displays.]
/PSYMB,Label,KEY 
[/PWEDGE | Creates an annotation wedge (GUI).]
/PWEDGE,XCENTR,YCENTR,XLRAD,ANGLE1,ANGLE2 
[/QUIT | Exits a processor.]
/QUIT 
[/RATIO | Distorts the object geometry.]
/RATIO,WN,RATOX,RATOY 
[/RENAME | Renames a file.]
/RENAME,Fname1,Ext1,--,Fname2,Ext2,-- 
[/REPLOT | Automatically reissues the last display command for convenience.]
/REPLOT,Label 
[/RESET | Resets display specifications to their initial defaults.]
/RESET 
[/RGB | Specifies the RGB color values for indices and contours.]
/RGB,Kywrd,PRED,PGRN,PBLU,N1,N2,NINC,NCNTR
[/RUNST | Enters the run statistics processor.]
/RUNST 
[/SECLIB | Library pathsdefining for SECREAD commandSets the default section library path for the SECREAD command.]
/SECLIB,Option,Path 
[/SEG | Allows graphics data to be stored in the local terminal memory.]
/SEG,Label,Aviname,DELAY 
[/SHADE | Defines the type of surface shading used with Z buffering.]
/SHADE,WN,Type 
[/SHOW | Specifies the device and other parameters for graphics displays.]
/SHOW,Fname,Ext,VECT,NCPL 
[/SHOWDISP | Defines the display driver name.]
/SHOWDISP,Dname,--,--,NCPL 
[/SHRINK | Shrinks elements,lines,areas,and volumes for display clarity.]
/SHRINK,RATIO 
[/SMBC | Controls the display of solid model boundary condition symbols and labels.]
/SMBC,Mode 
[/SOLU | Enters the solution processor.]
/SOLU 
[/SSCALE | Sets the contour multiplier for topographic displays.]
/SSCALE,WN,SMULT 
[/STATUS | Lists the status of items for the run.]
/STATUS,Lab 
[/STITLE | Defines subtitles.]
/STITLE,NLINE,Title 
[/SYP | Passes a command string and arguments to the operating system.]
/SYP,String,ARG1,ARG2,ARG3,ARG4,ARG5,ARG6,ARG7,ARG8
[/SYS | Passes a command string to the operating system.]
/SYS,String 
[/TEE | Writes a list of commands to a specified file at the same time that the commands are being executed.]
/TEE,Label,Fname,Ext,-- 
[/TITLE | Defines a main title.]
/TITLE,Title 
[/TLABEL | Creates annotation text (GUI).]
/TLABEL,XLOC,YLOC,Text 
[/TRIAD | Shows the global XYZ coordinate triad on displays.]
/TRIAD,Lab 
[/TRLCY | Specifies the level of translucency.]
/TRLCY,Lab,TLEVEL,N1,N2,NINC
[/TSPEC | Creates annotation text attributes (GUI).]
/TSPEC,TCOLOR,TSIZE,TXTHIC,PANGLE,IANGLE
[/TXTRE | Controls application of texture to selected items.]
/TXTRE,Lab,NUM,N1,N2,NINC
[/TYPE | Defines the type of display.]
/TYPE,WN,Type 
[/UCMD | Assigns a user defined command name.]
/UCMD,Cmd,SRNUM 
[/UDOC | Determines position and content for the multi legend options.]
/UDOC,Wind,Class,Key,
[/UI | Activates specified GUI dialog boxes.]
/UI,Func,Type,Format,Screen,Color,Krev,Orient,Compress,Quality
[/UIS | Controls the GUI behavior.]
/UIS,Label,VALUE 
[/UNITS | Annotates the database with the system of units used.]
/UNITS,Label,LENFACT,MASSFACT,TIMEFACT,TEMPFACT,TOFFSET,CHARGEFACT,FORCEFACT,HEATFACT
[/USER | Conveniently resets /FOCUS and /DIST to USER.]
/USER,WN 
[/VCONE | Defines the view cone angle for perspective displays.]
/VCONE,WN,PHI 
[/VIEW | Defines the viewing direction for the display.]
/VIEW,WN,XV,YV,ZV 
[/VSCALE | Scales the length of displayed vectors.]
/VSCALE,WN,VRATIO,KEY 
[/VUP | Specifies the global Cartesian coordinate system reference orientation.]
/VUP,WN,Label 
[/WAIT | Causes a delay before the reading of the next command.]
/WAIT,DTIME 
[/WINDOW | Defines the window size on the screen.]
/WINDOW,WN,XMIN,XMAX,YMIN,YMAX,NCOPY 
[/XFRM | Controls the centroid or the axis of dynamic rotation.]
/XFRM,LAB,X1,Y1,Z1,X2,Y2,Z2 
[/XRANGE | Specifies a linear abscissa (X) scale range.]
/XRANGE,XMIN,XMAX 
[/YRANGE | Specifies a linear ordinate (Y) scale range.]
/YRANGE,YMIN,YMAX,NUM 
[/ZOOM | Zooms a region of a display window.]
/ZOOM,WN,Lab,X1,Y1,X2,Y2 
[~CAT5IN | Transfers a .CATPart file into the ANSYS program.]
~CAT5IN,Name,Extension,Path,Entity,FMT,NOCL,NOAN 
[~CATIAIN | Transfers a CATIA model into the ANSYS program.]
~CATIAIN,Name,Extension,Path,- -,- -,BLANK,- - 
[~CIFIN | Transfers an electronic layer geometry file in CIF format into the ANSYS program.]
~CIFIN,Filename,Ext,Dir,Scale,Offset 
[~HEAL |"""Heal""a CAD file,then read it into ANSYS."]
~HEAL,Name,Extension,Path,Method,Check 
[~PARAIN | Transfers a Parasolid file into the ANSYS program.]
~PARAIN,Name,Extension,Path,Entity,FMT,Scale 
[~PROEIN | Transfers a Pro/ENGINEER part into the ANSYS program.]
~PROEIN,Name,Extension,Path,Proecomm,FMT 
[~SATIN | Transfers a .SAT file into the ANSYS program.]
~SATIN,Name,Extension,Path,Entity,FMT,NOCL,NOAN 
[~UGIN | Transfers a Unigraphics part into the ANSYS program.]
~UGIN,Name,Extension,Path,Entity,LAYER,FMT 
[A | Defines an area by connecting keypoints.]
A,P1,P2,P3,P4,P5,P6,P7,P8,P9,P10,P11,P12,P13,P14,P15,P16,P17,P18 
[AADD | Adds separate areas to create a single area.]
AADD,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[AATT | Associates element attributes with the selected,unmeshed areas.]
AATT,MAT,REAL,TYPE,ESYS,SECN 
[ABBRES | Reads abbreviations from a coded file.]
ABBRES,Lab,Fname,Ext,-- 
[ABBSAV | Writes the current abbreviation set to a coded file.]
ABBSAV,Lab,Fname,Ext,-- 
[ABS | Forms the absolute value of a variable.]
ABS,IR,IA,--,--,Name,--,--,FACTA 
[ACCAT | Concatenates multiple areas in preparation for mapped meshing.]
ACCAT,NA1,NA2 
[ACEL | Specifies the linear acceleration of the structure.]
ACEL,ACELX,ACELY,ACELZ 
[ACLEAR | Deletes nodes and area elements associated with selected areas.]
ACLEAR,NA1,NA2,NINC 
[ADAMS | Performs solutions and writes flexible body information to a modal neutral file (Jobname.MNF) for use in an ADAMS analysis.]
ADAMS,NMODES,KSTRESS,KSHELL 
[ADAPT | Adaptively meshes and solves a model.]
ADAPT,NSOLN,STARGT,TTARGT,FACMN,FACMX,KYKPS,KYMAC 
[ADD | Adds variables.]
ADD,IR,IA,IB,IC,Name,--,--,FACTA,FACTB,FACTC 
[ADDAM | Specifies the acceleration spectrum computation constants for the analysis of shock resistance of shipboard structures.]
ADDAM,AF,AA,AB,AC,AD,AMIN 
[ADELE | Deletes unmeshed areas.]
ADELE,NA1,NA2,NINC,KSWP 
[ADGL | Lists keypoints of an area that lie on a parametric degeneracy.]
ADGL,NA1,NA2,NINC 
[ADRAG | Generates areas by dragging a line pattern along a path.]
ADRAG,NL1,NL2,NL3,NL4,NL5,NL6,NLP1,NLP2,NLP3,NLP4,NLP5,NLP6
[AESIZE | Specifies the element size to be meshed onto areas.]
AESIZE,ANUM,SIZE,
[AFILLT | Generates a fillet at the intersection of two areas.]
AFILLT,NA1,NA2,RAD 
[AFLIST | Lists the current data in the database.]
AFLIST 
[AFSURF | Generates surface elements overlaid on the surface of existing solid elements and assigns the extra node as the closest fluid element node.]
AFSURF,SAREA,TLINE 
[AGEN | Generates additional areas from a pattern of areas.]
AGEN,ITIME,NA1,NA2,NINC,DX,DY,DZ,KINC,NOELEM,IMOVE 
[AGLUE |"Generates new areas by""gluing""areas."]
AGLUE,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[AINA | Finds the intersection of areas.]
AINA,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[AINP | Finds the pairwise intersection of areas.]
AINP,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[AINV | Finds the intersection of an area with a volume.]
AINV,NA,NV 
[AL | Generates an area bounded by previously defined lines.]
AL,L1,L2,L3,L4,L5,L6,L7,L8,L9,L10 
[ALIST | Lists the defined areas.]
ALIST,NA1,NA2,NINC,Lab 
[ALLSEL | Selects all entities with a single command.]
ALLSEL,LabT,Entity 
[ALPFILL | Fills in an area loop within an existing 2 D area (for models imported from CAD files).]
ALPFILL,LN1,LN2,LN3,LN4,LN5,LN6,LN7,LN8,LN9,LN10 
[ALPHAD | Defines the mass matrix multiplier for damping.]
ALPHAD,VALUE 
[AMAP | Generates a 2 D mapped mesh based on specified area corners.]
AMAP,AREA,KP1,KP2,KP3,KP4 
[AMESH | Generates nodes and area elements within areas.]
AMESH,NA1,NA2,NINC 
[ANCNTR | Produces an animated sequence of a contoured deformed shape.]
ANCNTR,NFRAM,DELAY,NCYCL 
[ANCUT | Produces an animated sequence of Q slices.]
ANCUT,NFRAM,DELAY,NCYCL,QOFF,KTOP,TOPOFF,NODE1,NODE2,NODE3 
[ANCYC | Applies a traveling wave animation to graphics data in a modal cyclic symmetry analysis.]
ANCYC,NUMFRAMES,KCYCL,DELAY 
[ANDATA | Produces a sequential contour animation over a range of results data.]
ANDATA,DELAY,NCYCL,RSLTDAT,MIN,MAX,INCR,FRCLST,AUTOCNTRKY 
[ANDSCL | Produces an animated sequence of a deformed shape.]
ANDSCL,NFRAM,DELAY,NCYCL 
[ANDYNA | Produces an animated sequence of contour values through substeps.]
ANDYNA,DELAY,NCYCL,START,END,INC,AUTOCONTOURKEY 
[ANFLOW | Produces an animated sequence of particle flow in a flowing fluid or a charged particle traveling in an electric or magnetic field.]
ANFLOW,NFRAM,DELAY,NCYCL,TIME,SPACING,SIZE,LENGTH 
[ANHARM | Produces a time transient animated sequence of time harmonic results (ANTYPE,HARMIC).]
ANHARM,NFRAM,DELAY,NCYCL 
[ANIM | Displays graphics data in animated form.]
ANIM,NCYCL,KCYCL,DELAY 
[ANISOS | Produces an animated sequence of an isosurface.]
ANISOS,NFRAM,DELAY,NCYCL 
[ANMODE | Produces an animated sequence of a mode shape.]
ANMODE,NFRAM,DELAY,NCYCL,KACCEL 
[ANMRES | Performs animation of results over multiple results files in an explicit dynamic analysis.]
ANMRES,DELAY,MIN,MAX,INC,AUTOCNTRKY,FREQ 
[ANORM | Reorients area normals.]
ANORM,ANUM,NOEFLIP 
[ANSOL | Specifies averaged nodal data to be stored from the results file in the solution coordinate system.]
ANSOL,NVAR,NODE,Item,Comp,Name,Mat,Real,Ename 
[ANTIME | Produces a sequential contour animation over a range of time.]
ANTIME,NFRAM,DELAY,NCYCL,AUTOCNTRKY,RSLTDAT,MIN,MAX 
[ANTYPE | Specifies the analysis type and restart status.]
ANTYPE,Antype,Status,LDSTEP,SUBSTEP,Action 
[AOFFST | Generates an area,offset from a given area.]
AOFFST,NAREA,DIST,KINC 
[AOVLAP | Overlaps areas.]
AOVLAP,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[APLOT | Displays the selected areas.]
APLOT,NA1,NA2,NINC,DEGEN,SCALE 
[APPEND | Reads data from the results file and appends it to the database.]
APPEND,LSTEP,SBSTEP,FACT,KIMG,TIME,ANGLE,NSET 
[APTN | Partitions areas.]
APTN,NA1,NA2,NA3,NA4,NA5,NA6,NA7,NA8,NA9 
[ARCLEN | Activates the arc length method.]
ARCLEN,Key,MAXARC,MINARC 
[ARCOLLAPSE | Collapses specified area to a specified line segment (for models imported from CAD files).]
ARCOLLAPSE,AREA,LINE 
[ARCTRM | Controls termination of the arc length solution.]
ARCTRM,Lab,VAL,NODE,DOF 
[ARDETACH | Detaches areas from neighboring geometrical entities (for models imported from CAD files).]
ARDETACH,AREA1,AREA2,AINC 
[AREAS |"Specifies""Areas""as the subsequent status topic."]
AREAS 
[AREFINE | Refines the mesh around specified areas.]
AREFINE,NA1,NA2,NINC,LEVEL,DEPTH,POST,RETAIN 
[AREVERSE | Reverses the normal of an area,regardless of its connectivity or mesh status.]
AREVERSE,ANUM,NOEFLIP 
[ARFILL | Creates an area based on a set of singly connected lines (for models imported from CAD files).]
ARFILL,LN1,LN2,LN3,LN4,LN5,LN6,LN7,LN8,LN9,LN10 
[ARMERGE | Merges two or more singly connected adjacent areas (for models imported from CAD files).]
ARMERGE,A1,A2,A3,A4,A5,A6,A7,A8,A9,A10 
[AROTAT | Generates cylindrical areas by rotating a line pattern about an axis.]
AROTAT,NL1,NL2,NL3,NL4,NL5,NL6,PAX1,PAX2,ARC,NSEG 
[ARSCALE | Generates a scaled set of areas from a pattern of areas.]
ARSCALE,NA1,NA2,NINC,RX,RY,RZ,KINC,NOELEM,IMOVE 
[ARSPLIT | Splits an area between two keypoints (for models imported from CAD files).]
ARSPLIT,AREA,KP1,KP2,TOL,Factor 
[ARSYM | Generates areas from an area pattern by symmetry reflection.]
ARSYM,Ncomp,NA1,NA2,NINC,KINC,NOELEM,IMOVE 
[ASBA | Subtracts areas from areas.]
ASBA,NA1,NA2,SEPO,KEEP1,KEEP2 
[ASBL | Subtracts lines from areas.]
ASBL,NA,NL,--,KEEPA,KEEPL 
[ASBV | Subtracts volumes from areas.]
ASBV,NA,NV,SEPO,KEEPA,KEEPV 
[ASBW | Subtracts the intersection of the working plane from areas (divides areas).]
ASBW,NA,SEPO,KEEP 
[ASEL | Selects a subset of areas.]
ASEL,Type,Item,Comp,VMIN,VMAX,VINC,KSWP 
[ASKIN |"Generates an area by""skinning""a surface through guiding lines."]
ASKIN,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[ASLL | Selects those areas containing the selected lines.]
ASLL,Type,ARKEY 
[ASLV | Selects those areas contained in the selected volumes.]
ASLV,Type 
[ASUB | Generates an area using the shape of an existing area.]
ASUB,NA1,P1,P2,P3,P4 
[ASUM | Calculates and prints geometry statistics of the selected areas.]
ASUM,LAB 
[ATAN | Forms the arctangent of a complex variable.]
ATAN,IR,IA,--,--,Name,--,--,FACTA 
[ATRAN | Transfers a pattern of areas to another coordinate system.]
ATRAN,KCNTO,NA1,NA2,NINC,KINC,NOELEM,IMOVE 
[ATYPE |"Specifies""Analysis types""as the subsequent status topic."]
ATYPE 
[AUTOTS | Specifies whether to use automatic time stepping or load stepping.]
AUTOTS,Key 
[AVPRIN | Specifies how principal and vector sums are to be calculated.]
AVPRIN,KEY,EFFNU 
[AVRES | Specifies how results data will be averaged when PowerGraphics is enabled.]
AVRES,KEY,Opt 
[BCSOPTION | Sets memory option for the sparse solver.]
BCSOPTION,--,Memory_Option,Memory_Size,--,--,Solve_Info 
[BELLOW | Defines a bellows in a piping run.]
BELLOW,NLOC,LENG,STIFF,FLEX,ELEM 
[BEND | Defines a bend in a piping run.]
BEND,NEL1,NEL2,RAD,NDIV,ESTRT,EINC 
[BETAD | Defines the stiffness matrix multiplier for damping.]
BETAD,VALUE 
[BF | Defines a nodal body force load.]
BF,NODE,Lab,VAL1,VAL2,VAL3,PHASE 
[BFA | Defines a body force load on an area.]
BFA,AREA,Lab,VAL1,VAL2,VAL3,PHASE 
[BFADELE | Deletes body force loads on an area.]
BFADELE,AREA,Lab 
[BFALIST | Lists the body force loads on an area.]
BFALIST,AREA,Lab 
[BFCUM | Specifies that nodal body force loads are to be accumulated.]
BFCUM,Lab,Oper,FACT,TBASE 
[BFDELE | Deletes nodal body force loads.]
BFDELE,NODE,Lab 
[BFE | Defines an element body force load.]
BFE,ELEM,Lab,STLOC,VAL1,VAL2,VAL3,VAL4 
[BFECUM | Specifies whether to ignore subsequent element body force loads.]
BFECUM,Lab,Oper,FACT,TBASE 
[BFEDELE | Deletes element body force loads.]
BFEDELE,ELEM,Lab 
[BFELIST | Lists the element body force loads.]
BFELIST,ELEM,Lab 
[BFESCAL | Scales element body force loads.]
BFESCAL,Lab,FACT,TBASE 
[BFINT | Activates the body force interpolation operation.]
BFINT,Fname1,Ext1,--,Fname2,Ext2,--,KPOS,Clab,KSHS,TOLOUT,TOLHGT 
[BFK | Defines a body force load at a keypoint.]
BFK,KPOI,Lab,VAL1,VAL2,VAL3,PHASE 
[BFKDELE | Deletes body force loads at a keypoint.]
BFKDELE,KPOI,Lab 
[BFKLIST | Lists the body force loads at keypoints.]
BFKLIST,KPOI,Lab 
[BFL | Defines a body force load on a line.]
BFL,LINE,Lab,VAL1,VAL2,VAL3,PHASE 
[BFLDELE | Deletes body force loads on a line.]
BFLDELE,LINE,Lab 
[BFLIST | Lists the body force loads on nodes.]
BFLIST,NODE,Lab 
[BFLLIST | Lists the body force loads on a line.]
BFLLIST,LINE,Lab 
[BFSCALE | Scales body force loads at nodes.]
BFSCALE,Lab,FACT,TBASE 
[BFTRAN | Transfers solid model body force loads to the finite element model.]
BFTRAN 
[BFUNIF | Assigns a uniform body force load to all nodes.]
BFUNIF,Lab,VALUE 
[BFV | Defines a body force load on a volume.]
BFV,VOLU,Lab,VAL1,VAL2,VAL3,PHASE 
[BFVDELE | Deletes body force loads on a volume.]
BFVDELE,VOLU,Lab 
[BFVLIST | Lists the body force loads on a volume.]
BFVLIST,VOLU,Lab 
[BIOOPT |"Specifies""Biot""Savart options""as the subsequent status topic."]
BIOOPT 
[BIOT | Calculates the Biot Savart source magnetic field intensity.]
BIOT,Label 
[BLC4 | Creates a rectangular area or block volume by corner points.]
BLC4,XCORNER,YCORNER,WIDTH,HEIGHT,DEPTH 
[BLC5 | Creates a rectangular area or block volume by center and corner points.]
BLC5,XCENTER,YCENTER,WIDTH,HEIGHT,DEPTH 
[BLOCK | Creates a block volume based on working plane coordinates.]
BLOCK,X1,X2,Y1,Y2,Z1,Z2 
[BOOL |"Specifies""Booleans""as the subsequent status topic."]
BOOL 
[BOPTN | Specifies Boolean operation options.]
BOPTN,Lab,Value 
[BRANCH | Defines the starting point for a piping branch.]
BRANCH,NODE,X,Y,Z 
[BSPLIN | Generates a single line from a spline fit to a series of keypoints.]
BSPLIN,P1,P2,P3,P4,P5,P6,XV1,YV1,ZV1,XV6,YV6,ZV6 
[BTOL | Specifies the Boolean operation tolerances.]
BTOL,PTOL 
[BUCOPT | Specifies buckling analysis options.]
BUCOPT,Method,NMODE,SHIFT,LDMULTE 
[C*** | Places a comment in the output.]
C***,Comment 
[CALC |"Specifies""Calculation settings""as the subsequent status topic."]
CALC 
[CBDOF | Activates cut boundary interpolation (for submodeling).]
CBDOF,Fname1,Ext1,--,Fname2,Ext2,--,KPOS,Clab,KSHS,TOLOUT,TOLHGT 
[CDREAD | Reads a file of solid model and database information into the database.]
CDREAD,Option,Fname,Ext,--,Fnamei,Exti 
[CDWRITE | Writes geometry and load database items to a file.]
CDWRITE,Option,Fname,Ext,--,Fnamei,Exti,Fmat 
[CE | Defines a constraint equation relating degrees of freedom.]
CE,NEQN,CONST,NODE1,Lab1,C1,NODE2,Lab2,C2,NODE3,Lab3,C3 
[CECMOD | Modifies the constant term of a constraint equation during solution.]
CECMOD,NEQN,CONST 
[CECYC | Generates the constraint equations for a cyclic symmetry analysis]
CECYC,Lowname,Highname,Nsector,HIndex,Tolerance,Kmove,Kpairs 
[CEDELE | Deletes constraint equations.]
CEDELE,NEQN1,NEQN2,NINC,Nsel 
[CEINTF | Generates constraint equations at an interface.]
CEINTF,TOLER,DOF1,DOF2,DOF3,DOF4,DOF5,DOF6,MoveTol 
[CELIST | Lists the constraint equations.]
CELIST,NEQN1,NEQN2,NINC,Nsel 
[CENTER | Defines a node at the center of curvature of 2 or 3 nodes.]
CENTER,NODE,NODE1,NODE2,NODE3,RADIUS 
[CEQN |"Specifies""Constraint equations""as the subsequent status topic."]
CEQN 
[CERIG | Defines a rigid region.]
CERIG,MASTE,SLAVE,Ldof,Ldof2,Ldof3,Ldof4,Ldof5 
[CESGEN | Generates a set of constraint equations from existing sets.]
CESGEN,ITIME,INC,NSET1,NSET2,NINC 
[CFACT | Defines complex scaling factors to be used with operations.]
CFACT,RFACTA,IFACTA,RFACTB,IFACTB,RFACTC,IFACTC 
[CGLOC | Specifies the origin location of the acceleration coordinate system.]
CGLOC,XLOC,YLOC,ZLOC 
[CGOMGA | Specifies the rotational velocity of the global origin.]
CGOMGA,CGOMX,CGOMY,CGOMZ 
[CIRCLE | Generates circular arc lines.]
CIRCLE,PCENT,RAD,PAXIS,PZERO,ARC,NSEG 
[CLOCAL | Defines a local coordinate system relative to the active coordinate system.]
CLOCAL,KCN,KCS,XL,YL,ZL,THXY,THYZ,THZX,PAR1,PAR2 
[CLOG | Forms the common log of a variable]
CLOG,IR,IA,--,--,Name,--,--,FACTA,FACTB 
[CLRMSHLN | Clears meshed entities.]
CLRMSHLN 
[CM | Groups geometry items into a component.]
CM,Cname,Entity 
[CMATRIX | Performs electrostatic field solutions and calculates the self and mutual capacitances between multiple conductors.]
CMATRIX,SYMFAC,Condname,NUMCOND,GRNDKEY,Capname 
[CMDELE | Deletes a component or assembly definition.]
CMDELE,Name 
[CMDOMEGA | Specifies the rotational acceleration of an element component about a user defined rotational axis.]
CMDOMEGA,CM_NAME,DOMEGAX,DOMEGAY,DOMEGAZ,X1,Y1,Z1,X2,Y2,Z2 
[CMEDIT | Edits an existing assembly.]
CMEDIT,Aname,Oper,Cnam1,Cnam2,Cnam3,Cnam4,Cnam5,Cnam6,Cnam7 
[CMGRP | Groups components and assemblies into an assembly.]
CMGRP,Aname,Cnam1,Cnam2,Cnam3,Cnam4,Cnam5,Cnam6,Cnam7,Cnam8 
[CMLIST | Lists the contents of a component or assembly.]
CMLIST,Name,Key,Entity 
[CMMOD | Modifies the specification of a component.]
CMMOD,Cname,Keyword,Value 
[CMOMEGA | Specifies the rotational velocity of an element component about a user defined rotational axis.]
CMOMEGA,CM_NAME,OMEGAX,OMEGAY,OMEGAZ,X1,Y1,Z1,X2,Y2,Z2,KSPIN 
[CMPLOT | Plots the entities contained in a component or assembly.]
CMPLOT,Label,Entity,Keyword 
[CMSEL | Selects a subset of components and assemblies.]
CMSEL,Type,Name,Entity 
[CNCHECK | Lists the initial status of contact pairs.]
CNCHECK,Levl,RID1,RID2,RINC 
[CNVTOL | Sets convergence values for nonlinear analyses.]
CNVTOL,Lab,VALUE,TOLER,NORM,MINREF 
[COMPRESS | Deletes all specified sets.]
COMPRESS 
[CON4 | Creates a conical volume anywhere on the working plane.]
CON4,XCENTER,YCENTER,RAD1,RAD2,DEPTH 
[CONE | Creates a conical volume centered about the working plane origin.]
CONE,RBOT,RTOP,Z1,Z2,THETA1,THETA2 
[CONJUG | Forms the complex conjugate of a variable.]
CONJUG,IR,IA,--,--,Name,--,--,FACTA 
[COUPLE |"Specifies""Node coupling""as the subsequent status topic."]
COUPLE 
[COVAL | Defines PSD cospectral values.]
COVAL,TBLNO1,TBLNO2,SV1,SV2,SV3,SV4,SV5,SV6,SV7 
[CP | Defines (or modifies) a set of coupled degrees of freedom.]
CP,NSET,Lab,NODE1,NODE2,NODE3,NODE4,NODE5,NODE6,NODE7,NODE8,NODE9,NODE10,NODE11,NODE12,NODE13,NODE14,NODE15,NODE16,NODE17
[CPCYC | Couples the two side faces of a cyclically symmetric model for loadings that are the same on every segment.]
CPCYC,Lab,TOLER,KCN,DX,DY,DZ,KNONROT 
[CPDELE | Deletes coupled degree of freedom sets.]
CPDELE,NSET1,NSET2,NINC,Nsel 
[CPINTF | Defines coupled degrees of freedom at an interface.]
CPINTF,Lab,TOLER 
[CPLGEN | Generates sets of coupled nodes from an existing set.]
CPLGEN,NSETF,Lab1,Lab2,Lab3,Lab4,Lab5 
[CPLIST | Lists the coupled degree of freedom sets.]
CPLIST,NSET1,NSET2,NINC,Nsel 
[CPMERGE | Merges different couple sets with duplicate degrees of freedom into one couple set.]
CPMERGE,Lab 
[CPNGEN | Defines,modifies,or adds to a set of coupled degrees of freedom.]
CPNGEN,NSET,Lab,NODE1,NODE2,NINC 
[CPSGEN | Generates sets of coupled nodes from existing sets.]
CPSGEN,ITIME,INC,NSET1,NSET2,NINC 
[CQC | Specifies the complete quadratic mode combination method.]
CQC,SIGNIF,Label 
[CRPLIM | Specifies the creep criterion for automatic time stepping.]
CRPLIM,CRCR,Option 
[CS | Defines a local coordinate system by three node locations.]
CS,KCN,KCS,NORIG,NXAX,NXYPL,PAR1,PAR2 
[CSCIR | Locates the singularity for non Cartesian local coordinate systems.]
CSCIR,KCN,KTHET,KPHI 
[CSDELE | Deletes local coordinate systems.]
CSDELE,KCN1,KCN2,KCINC 
[CSKP | Defines a local coordinate system by three keypoint locations.]
CSKP,KCN,KCS,PORIG,PXAXS,PXYPL,PAR1,PAR2 
[CSLIST | Lists coordinate systems.]
CSLIST,KCN1,KCN2,KCINC 
[CSWPLA | Defines a local coordinate system at the origin of the working plane.]
CSWPLA,KCN,KCS,PAR1,PAR2 
[CSYS | Activates a previously defined coordinate system.]
CSYS,KCN 
[CURR2D | Calculates current flow in a two dimensional conductor.]
CURR2D 
[CUTCONTROL | Controls time step cutback during a nonlinear solution.]
CUTCONTROL,Lab,VALUE,Option 
[CVAR | Computes covariance between two quantities.]
CVAR,IR,IA,IB,ITYPE,DATUM,Name 
[CYCLIC | Specifies a cyclic symmetry analysis.]
CYCLIC,NSECTOR,ANGLE,KCN,Name,USRCOMP 
[CYCOPT | Specifies solution options for a cyclic symmetry analysis.]
CYCOPT,OPTION,Value1,Value2,Value3,Value4,Value5,Value6,Value7 
[CYCPHASE | Provides tools for determining minimum and maximum possible result values from frequency couplets produced in a modal cyclic symmetry analysis.]
CYCPHASE,TYPE,OPTION 
[CYL4 | Creates a circular area or cylindrical volume anywhere on the working plane.]
CYL4,XCENTER,YCENTER,RAD1,THETA1,RAD2,THETA2,DEPTH 
[CYL5 | Creates a circular area or cylindrical volume by end points.]
CYL5,XEDGE1,YEDGE1,XEDGE2,YEDGE2,DEPTH 
[CYLIND | Creates a cylindrical volume centered about the working plane origin.]
CYLIND,RAD1,RAD2,Z1,Z2,THETA1,THETA2 
[D | Defines DOF constraints at nodes.]
D,NODE,Lab,VALUE,VALUE2,NEND,NINC,Lab2,Lab3,Lab4,Lab5,Lab6 
[DA | Defines DOF constraints on areas.]
DA,AREA,Lab,Value1,Value2 
[DADELE | Deletes DOF constraints on an area.]
DADELE,AREA,Lab 
[DALIST | Lists the DOF constraints on an area.]
DALIST,AREA 
[DAMORPH | Move nodes in selected areas to conform to structural displacements.]
DAMORPH,AREA,XLINE,RMSHKY 
[DATA | Reads data records from a file into a variable.]
DATA,IR,LSTRT,LSTOP,LINC,Name,KCPLX 
[DATADEF |"Specifies""Directly defined data status""as the subsequent status topic."]
DATADEF 
[DCGOMG | Specifies the rotational acceleration of the global origin.]
DCGOMG,DCGOX,DCGOY,DCGOZ 
[DCUM | Specifies that DOF constraint values are to be accumulated.]
DCUM,Oper,RFACT,IFACT,TBASE 
[DCVSWP | Performs a DC voltage sweep on a ROM element.]
DCVSWP,Option,Elem,Cnum,Vmax,Vinc1,Vinc2,Gap 
[DDELE | Deletes degree of freedom constraints.]
DDELE,NODE,Lab,NEND,NINC 
[DDSOPT | Initializes the Distributed Domain Solver (DDS) settings.]
DDSOPT,Configopt,Ndomains,Max_Iter 
[DEACT |"Specifies""Element birth and death""as the subsequent status topic."]
DEACT 
[DECOMP | Specifies method by which mesh will be decomposed into domains]
DECOMP,DDS,Ndomains 
[DEFINE |"Specifies""Data definition settings""as the subsequent status topic."]
DEFINE 
[DELETE | Specifies sets in the results file to be deleted before postprocessing.]
DELETE,SET,Nstart,Nend 
[DELTIM | Specifies the time step sizes to be used for this load step.]
DELTIM,DTIME,DTMIN,DTMAX,Carry 
[DEMORPH | Move nodes in selected elements to conform to structural displacements.]
DEMORPH,ELEM,DIMN,RMSHKY 
[DERIV | Differentiates a variable.]
DERIV,IR,IY,IX,--,Name,--,--,FACTA 
[DESIZE | Controls default element sizes.]
DESIZE,MINL,MINH,MXEL,ANGL,ANGH,EDGMN,EDGMX,ADJF,ADJM 
[DESOL | Defines or modifies solution results at a node of an element.]
DESOL,ELEM,NODE,Item,Comp,V1,V2,V3,V4,V5,V6 
[DETAB | Modifies element table results in the database.]
DETAB,ELEM,Lab,V1,V2,V3,V4,V5,V6 
[DIG | Digitizes nodes to a surface.]
DIG,NODE1,NODE2,NINC 
[DIGIT |"Specifies""Node digitizing""as the subsequent status topic."]
DIGIT 
[DISPLAY |"Specifies""Display settings""as the subsequent status topic."]
DISPLAY 
[DK | Defines DOF constraints at keypoints.]
DK,KPOI,Lab,VALUE,VALUE2,KEXPND,Lab2,Lab3,Lab4,Lab5,Lab6 
[DKDELE | Deletes DOF constraints at a keypoint.]
DKDELE,KPOI,Lab 
[DKLIST | Lists the DOF constraints at keypoints.]
DKLIST,KPOI 
[DL | Defines DOF constraints on lines.]
DL,LINE,AREA,Lab,Value1,Value2 
[DLDELE | Deletes DOF constraints on a line.]
DLDELE,LINE,Lab 
[DLIST | Lists DOF constraints.]
DLIST,NODE1,NODE2,NINC 
[DLLIST | Lists DOF constraints on a line.]
DLLIST,LINE 
[DMOVE | Digitizes nodes on surfaces and along intersections.]
DMOVE,NODE1,NODE2,NINC 
[DMPRAT | Sets a constant damping ratio.]
DMPRAT,RATIO 
[DNSOL | Defines or modifies solution results at a node.]
DNSOL,NODE,Item,Comp,V1,V2,V3,V4,V5,V6 
[DOF | Adds degrees of freedom to the current DOF set.]
DOF,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6,Lab7,Lab8,Lab9,Lab10 
[DOFSEL | Selects a DOF label set for reference by other commands.]
DOFSEL,Type,Dof1,Dof2,Dof3,Dof4,Dof5,Dof6 
[DOMEGA | Specifies the rotational acceleration of the structure.]
DOMEGA,DOMGX,DOMGY,DOMGZ 
[DSCALE | Scales DOF constraint values.]
DSCALE,RFACT,IFACT,TBASE 
[DSET | Sets the scale and drawing plane orientation for a digitizing tablet.]
DSET,NODE1,NODE2,NODE3,DDEV 
[DSUM | Specifies the double sum mode combination method.]
DSUM,SIGNIF,Label,TD 
[DSURF | Defines the surface upon which digitized nodes lie.]
DSURF,KCN,XSURF,YSURF,ZSURF 
[DSYM | Specifies symmetry or antisymmetry DOF constraints on nodes.]
DSYM,Lab,Normal,KCN 
[DSYS | Activates a display coordinate system for geometry listings and plots.]
DSYS,KCN 
[DTRAN | Transfers solid model DOF constraints to the finite element model.]
DTRAN 
[DUMP | Dumps the contents of a binary file.]
DUMP,NSTRT,NSTOP 
[DVMORPH | Move nodes in selected volumes to conform to structural displacements.]
DVMORPH,VOLU,XAREA,RMSHKY 
[DYNOPT |"Specifies""Dynamic analysis options""as the subsequent status topic."]
DYNOPT 
[E | Defines an element by node connectivity.]
E,I,J,K,L,M,N,O,P 
[EALIVE | Reactivates an element (for the birth and death capability).]
EALIVE,ELEM 
[EDADAPT | Activates adaptive meshing in an explicit dynamic analysis.]
EDADAPT,PART,Key 
[EDALE | Assigns mesh smoothing to explicit dynamic elements that use the ALE formulation.]
EDALE,Option,--,AFAC,BFAC,--,DFAC,EFAC,START,END 
[EDASMP | Creates a part assembly to be used in an explicit dynamic analysis.]
EDASMP,Option,ASMID,PART1,PART2,PART3,PART4,PART5,PART6,PART7,PART8,PART9,PART10,PART11,PART12,PART13,PART14,PART15,PART16 
[EDBOUND | Defines a boundary plane for sliding or cyclic symmetry.]
EDBOUND,Option,Lab,Cname,XC,YC,ZC,Cname2,COPT 
[EDBVIS | Specifies global bulk viscosity coefficients for an explicit dynamics analysis.]
EDBVIS,QVCO,LVCO 
[EDBX | Creates a box shaped volume to be used in a contact definition for explicit dynamics.]
EDBX,Option,BOXID,XMIN,XMAX,YMIN,YMAX,ZMIN,ZMAX 
[EDCADAPT | Specifies adaptive meshing controls for an explicit dynamic analysis.]
EDCADAPT,FREQ,TOL,OPT,MAXLVL,BTIME,DTIME,LCID,ADPSIZE,ADPASS,IREFLG,ADPENE,ADPTH,MAXEL 
[EDCGEN | Specifies contact parameters for an explicit dynamics analysis.]
EDCGEN,Option,Cont,Targ,FS,FD,DC,VC,VDC,V1,V2,V3,V4,BTIME,DTIME,BOXID1,BOXID2 
[EDCLIST | Lists contact entity specifications in an explicit dynamics analysis.]
EDCLIST,NUM 
[EDCMORE | Specifies additional contact parameters for a given contact definition in an explicit dynamic analysis.]
EDCMORE,Option,NUM,--,VAL1,VAL2 
[EDCNSTR | Defines various types of constraints for an explicit dynamic analysis.]
EDCNSTR,Option,Ctype,Comp1,Comp2,VAL1 
[EDCONTACT | Specifies contact surface controls for an explicit dynamics analysis.]
EDCONTACT,SFSI,RWPN,IPCK,SHTK,PENO,STCC,ORIE,CSPC,PENCHK 
[EDCPU | Specifies CPU time limit for an explicit dynamics analysis.]
EDCPU,CPUTIME 
[EDCRB | Constrains two rigid bodies to act as one in an explicit dynamics analysis.]
EDCRB,Option,NEQN,PARTM,PARTS 
[EDCSC | Specifies whether to use subcycling in an explicit dynamics analysis.]
EDCSC,Key 
[EDCTS | Specifies mass scaling and scale factor of computed time step for an explicit dynamics analysis.]
EDCTS,DTMS,TSSFAC 
[EDCURVE | Specifies data curves for an explicit dynamic analysis.]
EDCURVE,Option,LCID,Par1,Par2 
[EDDAMP | Defines mass weighted (Alpha) or stiffness weighted (Beta) damping for an explicit dynamics model.]
EDDAMP,PART,LCID,VALDMP 
[EDDBL | Selects a numerical precision type of the explicit dynamics analysis.]
EDDBL,KEY 
[EDDC | Deletes or deactivates/reactivates contact surface specifications in an explicit dynamic analysis.]
EDDC,Option,Ctype,Cont,Targ 
[EDDRELAX | Activates initialization to a prescribed geometry or dynamic relaxation for the explicit analysis.]
EDDRELAX,Option,NRCYCK,DRTOL,DFFCTR,DRTERM,TSSFDR,IRELAL,EDTTL 
[EDDUMP | Specifies output frequency for the explicit dynamic restart file (d3dump).]
EDDUMP,NUM,DT 
[EDELE | Deletes selected elements from the model.]
EDELE,IEL1,IEL2,INC 
[EDENERGY | Specifies energy dissipation controls for an explicit dynamics analysis.]
EDENERGY,HGEN,SWEN,SIEN,RLEN 
[EDFPLOT | Allows plotting of explicit dynamics forces and other load symbols.]
EDFPLOT,Key 
[EDGCALE | Defines global ALE controls for an explicit dynamic analysis.]
EDGCALE,NADV,METH 
[EDHGLS | Specifies the hourglass coefficient for an explicit dynamics analysis.]
EDHGLS,HGCO 
[EDHIST | Specifies time history output for an explicit dynamic analysis.]
EDHIST,Comp 
[EDHTIME | Specifies the time history output interval for an explicit dynamics analysis.]
EDHTIME,NSTEP,DT 
[EDINT | Specifies number of integration points for explicit shell and beam output.]
EDINT,SHELLIP,BEAMIP 
[EDIPART | Defines inertia for rigid parts in an explicit dynamics analysis.]
EDIPART,PART,Option,Cvect,TM,IRCS,Ivect,Vvect,CID 
[EDIS | Specifies stress initialization in an explicit dynamic full restart analysis.]
EDIS,Option,PIDN,PIDO 
[EDLCS | Defines a local coordinate system for use in explicit dynamics analysis.]
EDLCS,Option,CID,X1,Y1,Z1,X2,Y2,Z2,X3,Y3,Z3 
[EDLOAD | Specifies loads for an explicit dynamics analysis.]
EDLOAD,Option,Lab,KEY,Cname,Par1,Par2,PHASE,LCID,SCALE,BTIME,DTIME 
[EDMP | Defines material properties for an explicit dynamics analysis.]
EDMP,Lab,MAT,VAL1,VAL2,VAL3,VAL4,VAL5,VAL6 
[EDNB | Defines a nonreflecting boundary in an explicit dynamic analysis.]
EDNB,Option,Cname,AD,AS 
[EDNDTSD | Allows smoothing of noisy data for explicit dynamics analyses and provides a graphical representation of the data.]
EDNDTSD,Vect1,Vect2,DATAP,FITPT,Vect3,Vect4,DISP 
[EDNROT | Applies a rotated coordinate nodal constraint in an explicit dynamics analysis.]
EDNROT,Option,CID,Cname,DOF1,DOF2,DOF3,DOF4,DOF5,DOF6 
[EDOPT | Specifies the type of output for an explicit dynamics analysis.]
EDOPT,Option,--,Value 
[EDOUT | Specifies time history output (ASCII format) for an explicit dynamics analysis.]
EDOUT,Option 
[EDPART | Configures parts for an explicit dynamics analysis.]
EDPART,Option 
[EDPC | Selects and plots explicit dynamic contact entities.]
EDPC,MIN,MAX,INC 
[EDPL | Plots a time dependent load curve in an explicit dynamic analysis.]
EDPL,LDNUM 
[EDPVEL | Applies initial velocities to parts or part assemblies in an explicit dynamic analysis.]
EDPVEL,Option,PID,VX,VY,VZ,OMEGAX,OMEGAY,OMEGAZ,XC,YC,ZC,ANGX,ANGY,ANGZ 
[EDRC | Specifies rigid/deformable switch controls in an explicit dynamic analysis.]
EDRC,Option,NRBF,NCSF,--,DTMAX 
[EDRD | Switches a part from deformable to rigid or from rigid to deformable in an explicit dynamic analysis.]
EDRD,Option,PART,MRB 
[EDREAD | Reads explicit dynamics output into variables for time history postprocessing.]
EDREAD,NSTART,Label,NUM,STEP1,STEP2 
[EDRI | Defines inertia properties for a new rigid body that is created when a deformable part is switched to rigid in an explicit dynamic analysis.]
EDRI,Option,PART,XC,YC,ZC,TM,IXX,IYY,IZZ,IXY,IYZ,IXZ 
[EDRST | Specifies the output interval for an explicit dynamic analysis.]
EDRST,NSTEP,DT 
[EDRUN | Specify LS DYNA serial or parallel processing.]
EDRUN,Option,Cons 
[EDSHELL | Specifies shell computation controls for an explicit dynamics analysis.]
EDSHELL,WPAN,SHNU,SHTC,WPBT,SHPL,ITRST 
[EDSOLV |"Specifies""explicit dynamics solution""as the subsequent status topic."]
EDSOLV 
[EDSP | Specifies small penetration checking for contact entities in an explicit dynamic analysis.]
EDSP,Option,MIN,MAX,INC 
[EDSTART | Specifies status (new or restart) of an explicit dynamics analysis.]
EDSTART,RESTART,MEMORY,FSIZE,Dumpfile 
[EDTERM | Specifies termination criteria for an explicit dynamic analysis.]
EDTERM,Option,Lab,NUM,STOP,MAXC,MINC 
[EDTP | Plots explicit elements based on their time step size.]
EDTP,OPTION,VALUE1,VALUE2 
[EDVEL | Applies initial velocities to nodes or node components in an explicit dynamic analysis.]
EDVEL,Option,Cname,VX,VY,VZ,OMEGAX,OMEGAY,OMEGAZ,XC,YC,ZC,ANGX,ANGY,ANGZ 
[EDWELD | Defines a massless spotweld or generalized weld for use in an explicit dynamic analysis.]
EDWELD,Option,NWELD,N1,N2,SN,SS,EXPN,EXPS,EPSF,TFAIL,NSW,CID 
[EDWRITE | Writes explicit dynamics input to an LS DYNA input file.]
EDWRITE,Option,Fname,Ext,-- 
[EGEN | Generates elements from an existing pattern.]
EGEN,ITIME,NINC,IEL1,IEL2,IEINC,MINC,TINC,RINC,CINC,SINC,DX,DY,DZ 
[EINTF | Defines two noded elements between coincident or offset nodes.]
EINTF,TOLER,K,TLAB,KCN,DX,DY,DZ,KNONROT 
[EKILL | Deactivates an element (for the birth and death capability).]
EKILL,ELEM 
[ELEM |"Specifies""Elements""as the subsequent status topic."]
ELEM 
[ELIST | Lists the elements and their attributes.]
ELIST,IEL1,IEL2,INC,NNKEY,RKEY 
[EMAGERR | Calculates the relative error in an electrostatic or electromagnetic field analysis.]
EMAGERR 
[EMATWRITE | Forces the writing of all the element matrices to File.EMAT.]
EMATWRITE,Key 
[EMF | Calculates the electromotive force (emf),or voltage drop along a predefined path.]
EMF 
[EMID | Adds or removes midside nodes.]
EMID,Key,Edges 
[EMIS | Specifies emissivity as a material property for the Radiation Matrix method.]
EMIS,MAT,EVALU 
[EMODIF | Modifies a previously defined element.]
EMODIF,IEL,STLOC,I1,I2,I3,I4,I5,I6,I7,I8 
[EMORE | Adds more nodes to the just defined element.]
EMORE,Q,R,S,T,U,V,W,X 
[EMSYM | Specifies circular symmetry for electro magnetic sources.]
EMSYM,NSECT 
[EMTGEN | Generates a set of TRANS126 elements.]
EMTGEN,Ncomp,Ecomp,PNcomp,DOF,GAP,GAPMIN,FKN,Per0 
[EMUNIT | Specifies the system of units for magnetic field problems.]
EMUNIT,Lab,VALUE 
[EN | Defines an element by its number and node connectivity.]
EN,IEL,I,J,K,L,M,N,O,P 
[ENGEN | Generates elements from an existing pattern.]
ENGEN,IINC,ITIME,NINC,IEL1,IEL2,IEINC,MINC,TINC,RINC,CINC,SINC,DX,DY,DZ 
[ENORM | Reorients shell element normals.]
ENORM,ENUM 
[ENSYM | Generates elements by symmetry reflection.]
ENSYM,IINC,--,NINC,IEL1,IEL2,IEINC 
[EORIENT | Reorients solid element normals.]
EORIENT,Etype,Dir,TOLER 
[EPLOT | Produces an element display.]
EPLOT 
[EQSLV | Specifies the type of equation solver.]
EQSLV,Lab,TOLER,MULT 
[ERASE | Explicitly erases the current display.]
ERASE 
[EREAD | Reads elements from a file.]
EREAD,Fname,Ext,-- 
[EREFINE | Refines the mesh around specified elements.]
EREFINE,NE1,NE2,NINC,LEVEL,DEPTH,POST,RETAIN 
[ERESX | Specifies extrapolation of integration point results.]
ERESX,Key 
[ERNORM | Controls error estimation calculations.]
ERNORM,Key 
[ERRANG | Specifies the element range to be read from a file.]
ERRANG,EMIN,EMAX,EINC 
[ESEL | Selects a subset of elements.]
ESEL,Type,Item,Comp,VMIN,VMAX,VINC,KABS 
[ESCHECK | Perform element shape checking for a selected element set.]
ESCHECK,Sele,Levl,Defkey 
[ESIZE | Specifies the default number of line divisions.]
ESIZE,SIZE,NDIV 
[ESLA | Selects those elements associated with the selected areas.]
ESLA,Type 
[ESLL | Selects those elements associated with the selected lines.]
ESLL,Type 
[ESLN | Selects those elements attached to the selected nodes.]
ESLN,Type,EKEY,NodeType 
[ESLV | Selects elements associated with the selected volumes.]
ESLV,Type 
[ESOL | Specifies element data to be stored from the results file.]
ESOL,NVAR,ELEM,NODE,Item,Comp,Name 
[ESORT | Sorts the element table.]
ESORT,Item,Lab,ORDER,KABS,NUMB 
[ESSOLV | Performs a coupled electrostatic structural analysis.]
ESSOLV,Electit,Strutit,DIMN,MORPHOPT,Mcomp,Xcomp,ELECTOL,STRUTOL,MXLOOP,--,RUSEKY,RESTKY,EISCOMP 
[ESTIF | Specifies the matrix multiplier for deactivated elements.]
ESTIF,KMULT 
[ESURF | Generates elements overlaid on the free faces of existing selected elements.]
ESURF,XNODE,Tlab,Shape 
[ESYM | Generates elements from a pattern by a symmetry reflection.]
ESYM,--,NINC,IEL1,IEL2,IEINC 
[ESYS | Sets the element coordinate system attribute pointer.]
ESYS,KCN 
[ET | Defines a local element type from the element library.]
ET,ITYPE,Ename,KOP1,KOP2,KOP3,KOP4,KOP5,KOP6,INOPR 
[ETABLE | Fills a table of element values for further processing.]
ETABLE,Lab,Item,Comp 
[ETDELE | Deletes element types.]
ETDELE,ITYP1,ITYP2,INC 
[ETCHG | Changes element types to their corresponding types.]
ETCHG,Cnv 
[ETLIST | Lists currently defined element types.]
ETLIST,ITYP1,ITYP2,INC 
[ETYPE |"Specifies""Element types""as the subsequent status topic."]
ETYPE 
[EUSORT | Restores original order of the element table.]
EUSORT 
[EWRITE | Writes elements to a file.]
EWRITE,Fname,Ext,--,KAPPND,Format 
[EXP | Forms the exponential of a variable.]
EXP,IR,IA,--,--,Name,--,--,FACTA,FACTB 
[EXPAND | Displays the results of a modal cyclic symmetry analysis.]
EXPAND,Nrepeat,MODAL,HIndex,Icsys,SctAng,--,Phase 
[EXPASS | Specifies an expansion pass of an analysis.]
EXPASS,Key 
[EXPSOL | Specifies the solution to be expanded for reduced analyses.]
EXPSOL,LSTEP,SBSTEP,TIMFRQ,Elcalc 
[EXTOPT | Controls options relating to the generation of volume elements from area elements.]
EXTOPT,Lab,Val1,Val2,Val3 
[EXTREM | Lists the extreme values for variables.]
EXTREM,NVAR1,NVAR2,NINC 
[F | Specifies force loads at nodes.]
F,NODE,Lab,VALUE,VALUE2,NEND,NINC 
[FATIGUE |"Specifies""Fatigue data status""as the subsequent status topic."]
FATIGUE 
[FC | Provides failure criteria information and activates a data table to input temperature dependent stress and strain limits.]
FC,MAT,Lab1,Lab2,DATA1-6 
[FCDELE | Deletes previously defined failure criterion data for the given material.]
FCDELE,MAT 
[FCCHECK | Checks both the strain and stress input criteria for all materials.]
FCCHECK 
[FCLIST | To list what the failure criteria is that you have input.]
FCLIST,MAT,,TEMP 
[FCUM | Specifies that force loads are to be accumulated.]
FCUM,Oper,RFACT,IFACT 
[FDELE | Deletes force loads on nodes.]
FDELE,NODE,Lab,NEND,NINC 
[FE | Defines a set of fatigue event parameters.]
FE,NEV,CYCLE,FACT,Title 
[FEBODY |"Specifies""Body loads on elements""as the subsequent status topic."]
FEBODY 
[FECONS |"Specifies""Constraints on nodes""as the subsequent status topic."]
FECONS 
[FEFOR |"Specifies""Forces on nodes""as the subsequent status topic."]
FEFOR 
[FELIST | Lists the fatigue event parameters.]
FELIST,NEV1,NEV2,NINC 
[FESURF |"Specifies""Surface loads on elements""as the subsequent status topic."]
FESURF 
[FILE | Specifies the data file where results are to be found.]
FILE,Fname,Ext,-- 
[FILEAUX2 | Specifies the binary file to be dumped.]
FILEAUX2,Fname,Ident,-- 
[FILEAUX3 | Specifies the results file to be edited.]
FILEAUX3,Fname,Ext,-- 
[FILEDISP | Specifies the file containing the graphics data.]
FILEDISP,Fname,Ext,-- 
[FILL | Generates a line of nodes between two existing nodes.]
FILL,NODE1,NODE2,NFILL,NSTRT,NINC,ITIME,INC,SPACE 
[FILLDATA | Fills a variable by a ramp function.]
FILLDATA,IR,LSTRT,LSTOP,LINC,VALUE,DVAL 
[FINISH | Exits normally from a processor.]
FINISH 
[FITEM | Identifies items chosen by a picking operation (GUI).]
FITEM,NFIELD,ITEM,ITEMY,ITEMZ 
[FK | Defines force loads at keypoints.]
FK,KPOI,Lab,VALUE,VALUE2 
[FKDELE | Deletes force loads at a keypoint.]
FKDELE,KPOI,Lab 
[FKLIST | Lists the forces at keypoints.]
FKLIST,KPOI,Lab 
[FL | Defines a set of fatigue location parameters.]
FL,NLOC,NODE,SCFX,SCFY,SCFZ,Title 
[FLANGE | Defines a flange in a piping run.]
FLANGE,NLOC,LENG,MASS,SIF,FLEX,ARINS,ELEM 
[FLDATA | Sets up a FLOTRAN analysis.]
FLDATA,Name,Label,Value 
[FLDATA1 | Controls which features of the solution algorithm are activated.]
FLDATA1,SOLU,Label,Value 
[FLDATA10 | Specifies the COF2 coefficient of the fluid property equation.]
FLDATA10,COF2,Label,Value 
[FLDATA11 | Specifies the COF3 coefficient of the fluid property equation.]
FLDATA11,COF3,Label,Value 
[FLDATA12 | Sets the property update frequency flag.]
FLDATA12,PROP,Label,Value 
[FLDATA13 | Sets the property variation flag.]
FLDATA13,VARY,Label,Value 
[FLDATA14 | Specifies the reference temperature.]
FLDATA14,TEMP,Label,Value 
[FLDATA15 | Specifies the reference pressure.]
FLDATA15,PRES,Label,Value 
[FLDATA16 | Specifies the bulk modulus parameter.]
FLDATA16,BULK,Label,Value 
[FLDATA17 | Specifies the specific heat ratio.]
FLDATA17,GAMM,Label,Value 
[FLDATA18 | Selects the algebraic solver.]
FLDATA18,METH,Label,Value 
[FLDATA19 | Specifies the number of TDMA sweeps.]
FLDATA19,TDMA,Label,Value 
[FLDATA2 | Sets iteration and output controls for steady state analyses.]
FLDATA2,ITER,Label,Value 
[FLDATA20 | Specifies the number of conjugate direction search vectors.]
FLDATA20,SRCH,Label,Value 
[FLDATA20A | Specifies the amount of fill in when preconditioning the coefficient matrix.]
FLDATA20A,PGMR,Label,Value 
[FLDATA20B | Specifies the number of fill ins for the ILU preconditioner.]
FLDATA20B,PBCGM,Label,Value 
[FLDATA21 | Specifies the convergence criterion for FLOTRAN algebraic solvers.]
FLDATA21,CONV,Label,Value 
[FLDATA22 | Specifies the maximum number of semi direct iterations.]
FLDATA22,MAXI,Label,Value 
[FLDATA23 | Specifies the solver minimum normalized rate of change.]
FLDATA23,DELT,Label,Value 
[FLDATA24 | Sets the turbulence model and the constants used in the Standard k epsilon Model and the Zero Equation Turbulence Model.]
FLDATA24,TURB,Label,Value 
[FLDATA24A | Sets constants for the Re Normalized Group Turbulence Model (RNG).]
FLDATA24A,RNGT,Label,Value 
[FLDATA24B | Sets constants for the k ? Turbulence Model due to Shih (NKE).]
FLDATA24B,NKET,Label,Value 
[FLDATA24C | Sets constants for the Nonlinear Turbulence Model of Girimaji (GIR).]
FLDATA24C,GIRT,Label,Value 
[FLDATA24D | Sets constants for the Shih,Zhu,Lumley Turbulence Model (SZL).]
FLDATA24D,SZLT,Label,Value 
[FLDATA25 | Sets solution and property relaxation factors.]
FLDATA25,RELX,Label,Value 
[FLDATA26 | Sets stability controls.]
FLDATA26,STAB,Label,Value 
[FLDATA27 | Controls dependent variable printing.]
FLDATA27,PRIN,Label,Value 
[FLDATA28 | Specifies that variable results are to be replaced.]
FLDATA28,MODR,Label,Value 
[FLDATA29 | Re initializes a results variable.]
FLDATA29,MODV,Label,Value 
[FLDATA3 | Sets the convergence monitors for the degree of freedom set.]
FLDATA3,TERM,Label,Value 
[FLDATA30 | Controls the quadrature orders.]
FLDATA30,QUAD,Label,Value 
[FLDATA31 | Specifies dependent variable caps.]
FLDATA31,CAPP,Label,Value 
[FLDATA32 | Controls restart options.]
FLDATA32,REST,Label,Value,Value2,Fname,Ext,-- 
[FLDATA33 | Specifies the approach to discretize the advection term.]
FLDATA33,ADVM,Label,Value 
[FLDATA34 | Sets modified inertial relaxation factors.]
FLDATA34,MIR,Label,Value 
[FLDATA35 | Specifies tolerances for the lower and upper bound of the volume fraction.]
FLDATA35,VFTOL,Label,Value 
[FLDATA36 | Specifies ambient reference values outside of the fluid for the volume of fluid (VOF) method.]
FLDATA36,AMBV,Label,Value 
[FLDATA37 | Specifies segregated solution or film coefficient algorithms.]
FLDATA37,ALGR,Label,Value 
[FLDATA38 | Specifies the mass type for a fluid transient analysis.]
FLDATA38,MASS,Label,Value 
[FLDATA4 | Sets controls for transient analyses based on transient time and convergence monitors or sets time integration method.]
FLDATA4,TIME,Label,Value 
[FLDATA4A | Sets controls for transient analyses based on the number of time steps.]
FLDATA4A,STEP,Label,Value 
[FLDATA5 | Sets output and storage controls.]
FLDATA5,OUTP,Label,Value 
[FLDATA6 | Controls the output of the convergence monitor.]
FLDATA6,CONV,Label,Value 
[FLDATA7 | Specifies the type of fluid property.]
FLDATA7,PROT,Label,Value 
[FLDATA8 | Specifies the NOMI coefficient of the fluid property equation.]
FLDATA8,NOMI,Label,Value 
[FLDATA9 | Specifies the COF1 coefficient of the fluid property equation.]
FLDATA9,COF1,Label,Value 
[FLIST | Lists force loads on the nodes.]
FLIST,NODE1,NODE2,NINC 
[FLLIST | Lists the fatigue location parameters.]
FLLIST,NLOC1,NLOC2,NINC 
[FLOCHECK | Sets up and runs a zero iteration FLOTRAN analysis.]
FLOCHECK,Key 
[FLOTRAN |"Specifies""FLOTRAN data settings""as the subsequent status topic."]
FLOTRAN 
[FLREAD | Reads the residual file written by the FLOTRAN CFD option.]
FLREAD,Fname,Ext,-- 
[FLST | Specifies data required for a picking operation (GUI).]
FLST,NFIELD,NARG,TYPE,Otype,LENG 
[FLUXV | Calculates the flux passing through a closed contour.]
FLUXV 
[FMAGBC | Applies force and torque boundary conditions to an element component.]
FMAGBC,Cnam1,Cnam2,Cnam3,Cnam4,Cnam5,Cnam6,Cnam7,Cnam8,Cnam9 
[FMAGSUM | Summarizes electromagnetic force calculations on element components.]
FMAGSUM,Cnam1,Cnam2,Cnam3,Cnam4,Cnam5,Cnam6,Cnam7,Cnam8,Cnam9 
[FOR2D | Calculates magnetic forces on a body.]
FOR2D 
[FORCE | Selects the element nodal force type for output.]
FORCE,Lab 
[FORM | Specifies the format of the file dump.]
FORM,Lab 
[FP | Defines the fatigue S vs. N and Sm vs. T tables.]
FP,STITM,C1,C2,C3,C4,C5,C6 
[FPLIST | Lists the property table stored for fatigue evaluation.]
FPLIST 
[FREQ | Defines the frequency points for the SV vs. FREQ tables.]
FREQ,FREQ1,FREQ2,FREQ3,FREQ4,FREQ5,FREQ6,FREQ7,FREQ8,FREQ9 
[FS | Stores fatigue stress components at a node.]
FS,NODE,NEV,NLOD,STITM,C1,C2,C3,C4,C5,C6 
[FSAN | Turns a fluid solid interaction analysis on or off.]
FSAN,Key 
[FSCALE | Scales force load values in the database.]
FSCALE,RFACT,IFACT 
[FSCO | Sets convergence values for a fluid solid interaction analysis.]
FSCO,Lab,VALUE 
[FSDELE | Deletes a stress condition for a fatigue location,event,and loading.]
FSDELE,NLOC,NEV,NLOD 
[FSDT | Sets time step increment for a fluid solid interaction analysis.]
FSDT,INC 
[FSIN | Specifies the interface load transfer option for a fluid solid interaction analysis.]
FSIN,Opt 
[FSIT | Sets the maximum number of stagger iterations for a fluid solid interaction analysis.]
FSIT,Val1 
[FSLIST | Lists the stresses stored for fatigue evaluation.]
FSLIST,NLOC1,NLOC2,NINC,NEV,NLOD 
[FSNODE | Calculates and stores the stress components at a node for fatigue.]
FSNODE,NODE,NEV,NLOD 
[FSOR | Specifies analysis order for a fluid solid interaction analysis.]
FSOR,First,Second 
[FSOU | Sets output frequency for a fluid solid interaction analysis.]
FSOU,Freq 
[FSPLOT | Displays a fatigue stress item for a fatigue location and event.]
FSPLOT,NLOC,NEV,ITEM 
[FSRE | Sets relaxation values for a fluid solid interaction analysis.]
FSRE,Lab,VALUE 
[FSRS | Specifies time or load step number for restart of a fluid structure interaction analysis.]
FSRS,Opt,VALUE 
[FSSECT | Calculates and stores total linearized stress components.]
FSSECT,RHO,NEV,NLOD,KBR 
[FSSOLV | Performs a coupled steady state fluid structural analysis.]
FSSOLV,Fluitit,Strutit,DIMN,Mcomp,Xcomp,FORCTOL,MOMETOL,STRUTOL,MXLOOP,FLUITER,RUSEKY,RESTKY 
[FSSTAT | Lists the settings for a fluid solid interaction analysis.]
FSSTAT 
[FSTI | Sets end time and load time for a fluid solid interaction analysis.]
FSTI,ENDTIME,LOADTIME 
[FSTR | Specifies static or transient analyses for a fluid solid interaction analysis.]
FSTR,Field,Type 
[FSUM | Sums the nodal force and moment contributions of elements.]
FSUM,LAB,ITEM 
[FTCALC | Performs fatigue calculations for a particular node location.]
FTCALC,NLOC,NODE 
[FTRAN | Transfers solid model forces to the finite element model.]
FTRAN 
[FTSIZE | Defines the fatigue data storage array.]
FTSIZE,MXLOC,MXEV,MXLOD 
[FTWRITE | Writes all currently stored fatigue data on a file.]
FTWRITE,Fname,Ext,-- 
[FVMESH | Generates nodes and tetrahedral volume elements from detached exterior area elements (facets).]
FVMESH,KEEP 
[GAP |"Specifies""Reduced transient gap conditions""as the subsequent status topic."]
GAP 
[GAPF | Defines the gap force data to be stored in a variable.]
GAPF,NVAR,NUM,Name 
[GAPFINISH | Exits from the CAD import topology repair stage.]
GAPFINISH 
[GAPLIST | Lists all joined or disjoined lines in a model (for models imported from CAD files).]
GAPLIST,Lab 
[GAPMERGE | Merges adjacent disjoined lines (for models imported from CAD files).]
GAPMERGE,Lab,VAL1,VAL2,VAL3 
[GAPOPT | Sets preferences for the CAD import repair commands.]
GAPOPT,Lab,Value 
[GAPPLOT | Plots all joined or disjoined lines (for models imported from CAD files).]
GAPPLOT,Lab 
[GAUGE | Gauges the problem domain for an edge element formulation.]
GAUGE,Opt 
[GCGEN | Generates 2 D or 3 D contact elements.]
GCGEN,Ccomp,Tcomp,NUMC,RADC,Tlab,Shape 
[GENOPT |"Specifies""General options""as the subsequent status topic."]
GENOPT 
[GEOM | Defines the geometry specifications for the radiation matrix calculation.]
GEOM,K2D,NDIV 
[GEOMETRY |"Specifies""Geometry""as the subsequent status topic."]
GEOMETRY 
[GMFACE | Specifies the facet representation used to form solid models.]
GMFACE,Lab,N 
[GP | Defines a gap condition for transient analyses.]
GP,NODE1,NODE2,Lab,STIF,GAP,DAMP 
[GPDELE | Deletes gap conditions.]
GPDELE,GAP1,GAP2,GINC 
[GPLIST | Lists the gap conditions.]
GPLIST,GAP1,GAP2,GINC 
[GPLOT | Controls general plotting.]
GPLOT 
[GRP | Specifies the grouping mode combination method.]
GRP,SIGNIF,Label 
[GSBDATA | Specifies the constraints or applies the load at the ending point for generalized plane strain option.]
GSBDATA,LabZ,VALUEZ,LabX,VALUEX,LabY,VALUEY 
[GSGDATA | Specifies the reference point and defines the geometry in the fiber direction for the generalized plane strain element option.]
GSGDATA,LFIBER,XREF,YREF,ROTX0,ROTY0 
[GSLIST | When using generalized plane strain,lists the input data or solutions.]
GSLIST,Lab 
[GSSOL | Specifies which results to store from the results file when using generalized plane strain.]
GSSOL,NVAR,Item,Comp,Name 
[GSUM | Calculates and prints geometry items.]
GSUM 
[HARFRQ | Defines the frequency range in the harmonic response analysis.]
HARFRQ,FREQB,FREQE 
[HELP | Displays help information on ANSYS commands and element types.]
HELP,Name 
[HELPDISP | Displays help information on DISPLAY program commands.]
HELPDISP,Commandname 
[HEMIOPT | Specifies options for Hemicube view factor calculation.]
HEMIOPT,HRES 
[HFANG | Defines or displays spatial angles of a spherical radiation surface for antenna parameter calculations.]
HFANG,Lab,PHI1,PHI2,THETA1,THETA2 
[HFEIGOPT | Specifies high frequency electromagnetic modal analysis options.]
HFEIGOPT,Lab,Val1 
[HFEREFINE | Refines 3 D High Frequency Tetrahedral elements (HF119).]
HFEREFINE,FACTOR 
[HFNEAR | Calculates the electromagnetic field at points in the near zone exterior to the equivalent source surface (flagged with the Maxwell surface flag in the preprocessor).]
HFNEAR,Lab,VAL,X,Y,Z,CS 
[HFPCSWP | Calculates the propagating constants of a transmission line or waveguide over a frequency range.]
HFPCSWP,FREQB,FREQE,FREQINC,Nummode 
[HFPORT | Specifies a time harmonic guided wave excitation for a waveguide port.]
HFPORT,Portnum,Porttype,Local,Opt1,Opt2,VAL1,VAL2,VAL3,VAL4,VAL5 
[HFSCAT | Specifies a high frequency scattering analysis.]
HFSCAT,Lab 
[HFSWEEP | Performs a harmonic response for a high frequency electromagnetic wave guide analysis.]
HFSWEEP,FREQB,FREQE,FREQINC,Portin,Port2,Port3,Port4,Pvolt,Pang,Pdist,Vpath,Ipath,Vsymm,Isymm 
[HFSYM | Indicates the presence of symmetry planes for the computation of high frequency electromagnetic fields in the near and far field domains (beyond the finite element region).]
HFSYM,KCN,Xkey,Ykey,Zkey 
[HMAGSOLV | Specifies 2 D or axisymmetric harmonic magnetic solution options and initiates the solution.]
HMAGSOLV,FREQ,NRAMP,CNVA,CNVV,CNVC,CNVE,NEQIT 
[HPGL | Specifies various HP options.]
HPGL,Kywrd,Opt1,Opt2 
[HPTCREATE | Defines a hard point.]
HPTCREATE,TYPE,ENTITY,NHP,LABEL,VAL1,VAL2,VAL3 
[HPTDELETE | Deletes selected hardpoints.]
HPTDELETE,NP1,NP2,NINC 
[HRCPLX | Computes and stores in the database the time harmonic solution at a prescribed phase angle.]
HRCPLX,LOADSTEP,SUBSTEP,OMEGAT,1STLCASE,2NDLCASE 
[HREXP | Specifies the phase angle for the harmonic analysis expansion pass.]
HREXP,ANGLE 
[HROPT | Specifies harmonic analysis options.]
HROPT,Method,MAXMODE,MINMODE 
[HROUT | Specifies the harmonic analysis output options.]
HROUT,Reimky,Clust,Mcont 
[CHECK | Checks current database items for completeness.]
CHECK,Sele,Levl 
[CHKMSH | Checks area and volume entities for previous meshes.]
CHKMSH,Comp 
[IC | Specifies initial conditions at nodes.]
IC,NODE,Lab,VALUE,VALUE2,NEND,NINC 
[ICDELE | Deletes initial conditions at nodes.]
ICDELE 
[ICE | Specifies initial conditions on elements.]
ICE,ELEM,Lab,VALUE 
[ICEDELE | Deletes initial conditions on elements.]
ICEDELE,ELEM,Lab 
[ICELIST | Lists initial conditions on elements.]
ICELIST,ELEM,Lab 
[ICLIST | Lists the initial conditions.]
ICLIST,NODE1,NODE2,NINC,Lab 
[ICVFRC | Sets the initial volume fraction field for a geometry.]
ICVFRC,Geom,VAL1,VAL2,VAL3,VAL4 
[IGESIN | Transfers IGES data from a file into ANSYS.]
IGESIN,Fname,Ext,-- 
[IGESOUT | Writes solid model data to a file in IGES Version 5.1 format.]
IGESOUT,Fname,Ext,--,ATT 
[IMAGIN | Forms an imaginary variable from a complex variable.]
IMAGIN,IR,IA,--,--,Name,--,--,FACTA 
[IMESH | Generates nodes and interface elements along lines or areas.]
IMESH,LAKY,NSLA,NTLA,KCN,DX,DY,DZ,TOL 
[IMMED | Allows immediate display of a model as it is generated.]
IMMED,KEY 
[IMPD | Calculates the impedance of a conductor at a reference plane.]
IMPD,Vpath,Ipath,Vsymm,Isymm 
[INRES | Identifies the data to be retrieved from the results file.]
INRES,Item1,Item2,Item3,Item4,Item5,Item6,Item7,Item8 
[INRTIA |"Specifies""Inertial loads""as the subsequent status topic."]
INRTIA 
[INT1 | Integrates a variable.]
INT1,IR,IY,IX,���,Name,���,���,FACTA,FACTB,CONST 
[INTSRF | Integrates nodal results on an exterior surface.]
INTSRF,Lab 
[IOPTN | Controls options relating to importing a model.]
IOPTN,Lab,VAL1 
[IRLF | Specifies that inertia relief calculations are to be performed.]
IRLF,KEY 
[IRLIST | Prints inertia relief summary table.]
IRLIST 
[ISFILE | Reads an initial stress state from a file into ANSYS.]
ISFILE,Option,Fname,Ext,--,LOC,MAT1,MAT2,MAT3,MAT4,MAT5,MAT6,MAT7,MAT8,MAT9,MAT10 
[ISTRESS | Defines a set of initial stress values.]
ISTRESS,Sx,Sy,Sz,Sxy,Syz,Sxz,MAT1,MAT2,MAT3,MAT4,MAT5,MAT6,MAT7,MAT8,MAT9,MAT10 
[ISWRITE | Writes an ASCII file containing the initial stress values.]
ISWRITE,Switch 
[JPEG | Provides JPEG file export for ANSYS displays.]
JPEG,Kywrd,OPT 
[K | Defines a keypoint.]
K,NPT,X,Y,Z 
[KATT | Associates attributes with the selected,unmeshed keypoints.]
KATT,MAT,REAL,TYPE,ESYS 
[KBC | Specifies stepped or ramped loading within a load step.]
KBC,KEY 
[KBETW | Creates a keypoint between two existing keypoints.]
KBETW,KP1,KP2,KPNEW,Type,VALUE 
[KCALC | Calculates stress intensity factors in fracture mechanics analyses.]
KCALC,KPLAN,MAT,KCSYM,KLOCPR 
[KCENTER | Creates a keypoint at the center of a circular arc defined by three locations.]
KCENTER,Type,VAL1,VAL2,VAL3,VAL4,KPNEW 
[KCLEAR | Deletes nodes and point elements associated with selected keypoints.]
KCLEAR,NP1,NP2,NINC 
[KDELE | Deletes unmeshed keypoints.]
KDELE,NP1,NP2,NINC 
[KDIST | Calculates and lists the distance between two keypoints.]
KDIST,KP1,KP2 
[KEEP | Stores POST26 definitions and data during active session.]
KEEP,Key 
[KESIZE | Specifies the edge lengths of the elements nearest a keypoint.]
KESIZE,NPT,SIZE,FACT1,FACT2 
[KEYOPT | Sets element key options.]
KEYOPT,ITYPE,KNUM,VALUE 
[KEYPTS |"Specifies""Keypoints""as the subsequent status topic."]
KEYPTS 
[KEYW | Sets a keyword used by the GUI for context filtering (GUI).]
KEYW,Keyword,KEY 
[KFILL | Generates keypoints between two keypoints.]
KFILL,NP1,NP2,NFILL,NSTRT,NINC,SPACE 
[KGEN | Generates additional keypoints from a pattern of keypoints.]
KGEN,ITIME,NP1,NP2,NINC,DX,DY,DZ,KINC,NOELEM,IMOVE 
[KL | Generates a keypoint at a specified location on an existing line.]
KL,NL1,RATIO,NK1 
[KLIST | Lists the defined keypoints or hard points.]
KLIST,NP1,NP2,NINC,Lab 
[KMESH | Generates nodes and point elements at keypoints.]
KMESH,NP1,NP2,NINC 
[KMODIF | Modifies an existing keypoint.]
KMODIF,NPT,X,Y,Z 
[KMOVE | Calculates and moves a keypoint to an intersection.]
KMOVE,NPT,KC1,X1,Y1,Z1,KC2,X2,Y2,Z2 
[KNODE | Defines a keypoint at an existing node location.]
KNODE,NPT,NODE 
[KPLOT | Displays the selected keypoints.]
KPLOT,NP1,NP2,NINC,Lab 
[KPSCALE | Generates a scaled set of (meshed) keypoints from a pattern of keypoints.]
KPSCALE,NP1,NP2,NINC,RX,RY,RZ,KINC,NOELEM,IMOVE 
[KREFINE | Refines the mesh around specified keypoints.]
KREFINE,NP1,NP2,NINC,LEVEL,DEPTH,POST,RETAIN 
[KSCALE | Generates a scaled pattern of keypoints from a given keypoint pattern.]
KSCALE,KINC,NP1,NP2,NINC,RX,RY,RZ 
[KSCON | Specifies a keypoint about which an area mesh will be skewed.]
KSCON,NPT,DELR,KCTIP,NTHET,RRAT 
[KSEL | Selects a subset of keypoints or hard points.]
KSEL,Type,Item,Comp,VMIN,VMAX,VINC,KABS 
[KSLL | Selects those keypoints contained in the selected lines.]
KSLL,Type 
[KSLN | Selects those keypoints associated with the selected nodes.]
KSLN,Type 
[KSUM | Calculates and prints geometry statistics of the selected keypoints.]
KSUM 
[KSYMM | Generates a reflected set of keypoints.]
KSYMM,Ncomp,NP1,NP2,NINC,KINC,NOELEM,IMOVE 
[KTRAN | Transfers a pattern of keypoints to another coordinate system.]
KTRAN,KCNTO,NP1,NP2,NINC,KINC,NOELEM,IMOVE 
[KUSE | Specifies whether or not to reuse the triangularized matrix.]
KUSE,KEY 
[KWPAVE | Moves the working plane origin to the average location of keypoints.]
KWPAVE,P1,P2,P3,P4,P5,P6,P7,P8,P9 
[KWPLAN | Defines the working plane using three keypoints.]
KWPLAN,WN,KORIG,KXAX,KPLAN 
[L | Defines a line between two keypoints.]
L,P1,P2,NDIV,SPACE,XV1,YV1,ZV1,XV2,YV2,ZV2 
[L2ANG | Generates a line at an angle with two existing lines.]
L2ANG,NL1,NL2,ANG1,ANG2,PHIT1,PHIT2 
[L2TAN | Generates a line tangent to two lines.]
L2TAN,NL1,NL2 
[LANG | Generates a straight line at an angle with a line.]
LANG,NL1,P3,ANG,PHIT,LOCAT 
[LARC | Defines a circular arc.]
LARC,P1,P2,PC,RAD 
[LAREA | Generates the shortest line between two keypoints on an area.]
LAREA,P1,P2,NAREA 
[LARGE | Finds the largest (the envelope) of three variables.]
LARGE,IR,IA,IB,IC,Name,--,--,FACTA,FACTB,FACTC 
[LATT | Associates element attributes with the selected,unmeshed lines.]
LATT,MAT,REAL,TYPE,--,KB,KE,SECNUM 
[LAYER | Specifies the element layer for which data are to be processed.]
LAYER,NUM 
[LAYERP26 | Specifies the element layer for which data are to be stored.]
LAYERP26,NUM 
[LAYLIST | Lists real constants material properties for layered elements.]
LAYLIST,IEL,LAYR1,LAYR2,Mplab1,Mplab2 
[LAYPLOT | Displays the layer stacking sequence for layered elements.]
LAYPLOT,IEL,LAYR1,LAYR2 
[LCABS | Specifies absolute values for load case operations.]
LCABS,LCNO,KABS 
[LCASE | Reads a load case into the database.]
LCASE,LCNO 
[LCCALC |"Specifies""Load case settings""as the subsequent status topic."]
LCCALC 
[LCCAT | Concatenates multiple lines into one line for mapped meshing.]
LCCAT,NL1,NL2 
[LCDEF | Creates a load case from a set of results on a results file.]
LCDEF,LCNO,LSTEP,SBSTEP,KIMG 
[LCFACT | Defines scale factors for load case operations.]
LCFACT,LCNO,FACT 
[LCFILE | Creates a load case from an existing load case file.]
LCFILE,LCNO,Fname,Ext,-- 
[LCLEAR | Deletes nodes and line elements associated with selected lines.]
LCLEAR,NL1,NL2,NINC 
[LCOMB | Combines adjacent lines into one line.]
LCOMB,NL1,NL2,KEEP 
[LCOPER | Performs load case operations.]
LCOPER,Oper,LCASE1,Oper2,LCASE2 
[LCSEL | Selects a subset of load cases.]
LCSEL,Type,LCMIN,LCMAX,LCINC 
[LCSL | Divides intersecting lines at their point(s) of intersection.]
LCSL,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LCSUM | Specifies whether to process non summable items in load case operations.]
LCSUM,Lab 
[LCWRITE | Creates a load case by writing results to a load case file.]
LCWRITE,LCNO,Fname,Ext,-- 
[LCZERO | Zeroes the results portion of the database.]
LCZERO 
[LDELE | Deletes unmeshed lines.]
LDELE,NL1,NL2,NINC,KSWP 
[LDIV | Divides a single line into two or more lines.]
LDIV,NL1,RATIO,PDIV,NDIV,KEEP 
[LDRAG | Generates lines by sweeping a keypoint pattern along path.]
LDRAG,NK1,NK2,NK3,NK4,NK5,NK6,NL1,NL2,NL3,NL4,NL5,NL6 
[LDREAD | Reads results from the results file and applies them as loads.]
LDREAD,Lab,LSTEP,SBSTEP,TIME,KIMG,Fname,Ext,-- 
[LESIZE | Specifies the divisions and spacing ratio on unmeshed lines.]
LESIZE,NL1,SIZE,ANGSIZ,NDIV,SPACE,KFORC,LAYER1,LAYER2,KYNDIV 
[LEXTND | Extends a line at one end by using its slope.]
LEXTND,NL1,NK1,DIST,KEEP 
[LFILLT | Generates a fillet line between two intersecting lines.]
LFILLT,NL1,NL2,RAD,PCENT 
[LFSURF | Generates surface elements overlaid on the edge of existing solid elements and assigns the extra node as the closest fluid element node.]
LFSURF,SLINE,TLINE 
[LGEN | Generates additional lines from a pattern of lines.]
LGEN,ITIME,NL1,NL2,NINC,DX,DY,DZ,KINC,NOELEM,IMOVE 
[LGLUE |"Generates new lines by""gluing""lines."]
LGLUE,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LGWRITE | Writes the database command log to a file.]
LGWRITE,Fname,Ext,--,Kedit 
[LINA | Finds the intersection of a line with an area.]
LINA,NL,NA 
[LINE |"Specifies""Lines""as the subsequent status topic."]
LINE 
[LINES | Specifies the length of a printed page.]
LINES,N 
[LINL | Finds the common intersection of lines.]
LINL,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LINP | Finds the pairwise intersection of lines.]
LINP,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LINV | Finds the intersection of a line with a volume.]
LINV,NL,NV 
[LIST | Lists out the sets in the results file.]
LIST,LEVEL 
[LLIST | Lists the defined lines.]
LLIST,NL1,NL2,NINC,Lab 
[LMATRIX | Calculates an inductance matrix and the total flux linkage for an N winding coil system.]
LMATRIX,Symfac,Coilname,Curname,Indname 
[LMESH | Generates nodes and line elements along lines.]
LMESH,NL1,NL2,NINC 
[LNCOLLAPSE | Collapse a line segment to a keypoint (for models imported from CAD files).]
LNCOLLAPSE,LINE,KEYPOINT 
[LNDETACH | Detaches lines from neighboring geometric entity (for models imported from CAD files).]
LNDETACH,LINE1,LINE2,LNINC 
[LNFILL | Creates a straight line between two keypoints (for models imported from CAD files).]
LNFILL,KP1,KP2 
[LNMERGE | Merges two or more connected line segments (for models imported from CAD files).]
LNMERGE,LN1,LN2,LN3,LN4,LN4,LN6,LN7,LN8,LN9,LN10 
[LNSPLIT | Splits a line segment into two line segments (for models imported from CAD files).]
LNSPLIT,LINE,PARAM 
[LNSRCH | Activates a line search to be used with Newton Raphson.]
LNSRCH,Key 
[LOCAL | Defines a local coordinate system by a location and orientation.]
LOCAL,KCN,KCS,XC,YC,ZC,THXY,THYZ,THZX,PAR1,PAR2 
[LOVLAP | Overlaps lines.]
LOVLAP,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LPLOT | Displays the selected lines.]
LPLOT,NL1,NL2,NINC 
[LPTN | Partitions lines.]
LPTN,NL1,NL2,NL3,NL4,NL5,NL6,NL7,NL8,NL9 
[LREFINE | Refines the mesh around specified lines.]
LREFINE,NL1,NL2,NINC,LEVEL,DEPTH,POST,RETAIN 
[LREVERSE | Reverses the normal of a line,regardless of its connectivity or mesh status.]
LREVERSE,LNUM,NOEFLIP 
[LROTAT | Generates circular lines by rotating a keypoint pattern about an axis.]
LROTAT,NK1,NK2,NK3,NK4,NK5,NK6,PAX1,PAX2,ARC,NSEG 
[LSBA | Subtracts areas from lines.]
LSBA,NL,NA,SEPO,KEEPL,KEEPA 
[LSBL | Subtracts lines from lines.]
LSBL,NL1,NL2,SEPO,KEEP1,KEEP2 
[LSBV | Subtracts volumes from lines.]
LSBV,NL,NV,SEPO,KEEPL,KEEPV 
[LSBW | Subtracts the intersection of the working plane from lines (divides lines).]
LSBW,NL,SEPO,KEEP 
[LSCLEAR | Clears loads and load step options from the database.]
LSCLEAR,Lab 
[LSDELE | Deletes load step files.]
LSDELE,LSMIN,LSMAX,LSINC 
[LSEL | Selects a subset of lines.]
LSEL,Type,Item,Comp,VMIN,VMAX,VINC,KSWP 
[LSLA | Selects those lines contained in the selected areas.]
LSLA,Type 
[LSLK | Selects those lines containing the selected keypoints.]
LSLK,Type,LSKEY 
[LSOPER |"Specifies""Load step operations""as the subsequent status topic."]
LSOPER 
[LSREAD | Reads load and load step option data into the database.]
LSREAD,LSNUM 
[LSSCALE | Generates a scaled set of lines from a pattern of lines.]
LSSCALE,NL1,NL2,NINC,RX,RY,RZ,KINC,NOELEM,IMOVE 
[LSSOLVE | Reads and solves multiple load steps.]
LSSOLVE,LSMIN,LSMAX,LSINC 
[LSTR | Defines a straight line irrespective of the active coordinate system.]
LSTR,P1,P2 
[LSUM | Calculates and prints geometry statistics of the selected lines.]
LSUM 
[LSWRITE | Writes load and load step option data to a file.]
LSWRITE,LSNUM 
[LSYMM | Generates lines from a line pattern by symmetry reflection.]
LSYMM,Ncomp,NL1,NL2,NINC,KINC,NOELEM,IMOVE 
[LTAN | Generates a line at the end of,and tangent to,an existing line.]
LTAN,NL1,P3,XV3,YV3,ZV3 
[LTRAN | Transfers a pattern of lines to another coordinate system.]
LTRAN,KCNTO,NL1,NL2,NINC,KINC,NOELEM,IMOVE 
[LUMPM | Specifies a lumped mass matrix formulation.]
LUMPM,Key 
[LVSCALE | Scales the load vector for mode superposition analyses.]
LVSCALE,FACT 
[LWPLAN | Defines the working plane normal to a location on a line.]
LWPLAN,WN,NL1,RATIO 
[M | Defines master degrees of freedom for reduced and superelement generation analyses.]
M,NODE,Lab1,NEND,NINC,Lab2,Lab3,Lab4,Lab5,Lab6 
[MAGOPT | Specifies options for a 3 D magnetostatic field analysis.]
MAGOPT,VALUE 
[MAGSOLV | Specifies magnetic solution options and initiates the solution.]
MAGSOLV,OPT,NRAMP,CNVCSG,CNVFLUX,NEQIT,BIOT 
[MASTER |"Specifies""Master DOF""as the subsequent status topic."]
MASTER 
[MAT | Sets the element material attribute pointer.]
MAT,MAT 
[MATER |"Specifies""Material properties""as the subsequent status topic."]
MATER 
[MDAMP | Defines the damping ratios as a function of mode.]
MDAMP,STLOC,V1,V2,V3,V4,V5,V6 
[MDELE | Deletes master degrees of freedom.]
MDELE,NODE,Lab1,NEND,NINC,Lab2,Lab3,Lab4,Lab5,Lab6 
[MEMM | Allows the current session to keep allocated memory]
MEMM,Lab,Kywrd 
[MESHING |"Specifies""Meshing""as the subsequent status topic."]
MESHING 
[MGEN | Generates additional MDOF from a previously defined set.]
MGEN,ITIME,INC,NODE1,NODE2,NINC 
[MCHECK | Checks mesh connectivity.]
MCHECK,Lab 
[MITER | Defines a mitered bend in a piping run.]
MITER,NEL1,NEL2,RAD,NDIV,ESTRT,EINC 
[MLIST | Lists the MDOF of freedom.]
MLIST,NODE1,NODE2,NINC 
[MMF | Calculates the magnetomotive force along a path.]
MMF 
[MODE | Specifies the harmonic loading term for this load step.]
MODE,MODE,ISYM 
[MODIFY | Changes the listed values of the data in a set.]
MODIFY,SET,LSTEP,ITER,CUMIT,TIME,Ktitle 
[MODMSH | Controls the relationship of the solid model and the FE model.]
MODMSH,Lab 
[MODOPT | Specifies modal analysis options.]
MODOPT,Method,NMODE,FREQB,FREQE,PRMODE,Nrmkey,,Cekey 
[MONITOR | Controls contents of three variable fields in nonlinear solution monitor file.]
MONITOR,VAR,Node,Lab 
[MOPT | Specifies meshing options.]
MOPT,Lab,Value 
[MOVE | Calculates and moves a node to an intersection.]
MOVE,NODE,KC1,X1,Y1,Z1,KC2,X2,Y2,Z2 
[MP | Defines a linear material property as a constant or a function of temperature.]
MP,Lab,MAT,C0,C1,C2,C3,C4 
[MPAMOD | Modifies temperature dependent coefficients of thermal expansion.]
MPAMOD,MAT,DEFTEMP 
[MPCOPY | Copies linear material model data from one material reference number to another.]
MPCOPY,--,MATF,MATT 
[MPDATA | Defines property data to be associated with the temperature table.]
MPDATA,Lab,MAT,STLOC,C1,C2,C3,C4,C5,C6 
[MPDELE | Deletes linear material properties.]
MPDELE,Lab,MAT1,MAT2,INC 
[MPDRES | Reassembles existing material data with the temperature table.]
MPDRES,LabF,MATF,LabT,MATT 
[MPCHG | Changes the material number attribute of an element.]
MPCHG,MAT,ELEM 
[MPLIST | Lists linear material properties.]
MPLIST,MAT1,MAT2,INC,Lab,TEVL 
[MPPLOT | Plots linear material properties as a function of temperature.]
MPPLOT,Lab,MAT,TMIN,TMAX,PMIN,PMAX 
[MPREAD | Reads a file containing material properties.]
MPREAD,Fname,Ext,--,LIB 
[MPRINT | Specifies that radiation matrices are to be printed.]
MPRINT,KEY 
[MPTEMP | Defines a temperature table for material properties.]
MPTEMP,STLOC,T1,T2,T3,T4,T5,T6 
[MPTGEN | Adds temperatures to the temperature table by generation.]
MPTGEN,STLOC,NUM,TSTRT,TINC 
[MPTRES | Restores a temperature table previously defined.]
MPTRES,Lab,MAT 
[MPWRITE | Writes linear material properties in the database to a file (if the LIB option is not specified) or writes both linear and nonlinear material properties (if LIB is specified) from the database to a file.]
MPWRITE,Fname,Ext,--,LIB,MAT 
[MSADV | Specifies the approach to discretize the advection term in a species transport equation.]
MSADV,SPNUM,MTHA 
[MSAVE | Memory savingwhen generating stiffness matrixSets the solver memory saving option. This option only applies to the PCG solver.Solver,memory saving feature]
MSAVE,Key 
[MSCAP | Activates and controls mass fraction capping for a species.]
MSCAP,SPNUM,Capkey,UPPER,LOWER 
[MSDATA | Defines multiple species data applicable to all species.]
MSDATA,ALGEB,UGAS 
[MSHAPE | For elements that support multiple shapes,specifies the element shape to be used for meshing.]
MSHAPE,KEY,Dimension 
[MSHCOPY | Simplifies the generation of meshes that have matching node element patterns on two different line groups (in 2 D) or area groups (3 D).]
MSHCOPY,KEYLA,LAPTRN,LACOPY,KCN,DX,DY,DZ,TOL,LOW,HIGH 
[MSHKEY | Specifies whether free meshing or mapped meshing should be used to mesh a model.]
MSHKEY,KEY 
[MSHMID | Specifies placement of midside nodes.]
MSHMID,KEY 
[MSHPATTERN | Specifies pattern to be used for mapped triangle meshing.]
MSHPATTERN,KEY 
[MSMASS | Specifies the mass type for a transient species analysis.]
MSMASS,SPNUM,Value 
[MSMETH | Specifies the method of solution of the species transport equations.]
MSMETH,SPNUM,KEY 
[MSMIR | Sets modified inertial relaxation factors for multiple species.]
MSMIR,SPNUM,Value 
[MSNOMF | Specifies the initial value of nominal mass fraction for a species.]
MSNOMF,SPNUM,FRACTION 
[MSPROP | Defines the fluid properties of a species.]
MSPROP,SPNUM,Label,Type,NOMINAL,COF1,COF2,COF3 
[MSQUAD | Specifies the quadrature order for multiple species elements.]
MSQUAD,QDIF,QSRC 
[MSRELAX | Specifies relaxation factors for a multiple species transport analysis.]
MSRELAX,SPNUM,CONC,MDIF,EMDI,STAB 
[MSSOLU | Specifies solution options for multiple species transport.]
MSSOLU,SPNUM,NSWEEP,MAXI,NSRCH,CONV,DELMAX 
[MSSPEC | Specifies the name,molecular weight,and Schmidt number of a species.]
MSSPEC,SPNUM,Name,MOLWT,SCHMIDT 
[MSTERM | Sets the convergence monitors for species.]
MSTERM,SPNUM,STER,TTER 
[MSVARY | Allows species properties to vary between global iterations.]
MSVARY,SPNUM,Lab,Key 
[MXPAND | Specifies the number of modes to expand and write for a modal or buckling analysis.]
MXPAND,NMODE,FREQB,FREQE,Elcalc,SIGNIF 
[N | Defines a node.]
N,NODE,X,Y,Z,THXY,THYZ,THZX 
[NANG | Rotates a nodal coordinate system by direction cosines.]
NANG,NODE,X1,X2,X3,Y1,Y2,Y3,Z1,Z2,Z3 
[NCNV | Sets the key to terminate an analysis.]
NCNV,KSTOP,DLIM,ITLIM,ETLIM,CPLIM 
[NDELE | Deletes nodes.]
NDELE,NODE1,NODE2,NINC 
[NDIST | Calculates and lists the distance between two nodes.]
NDIST,ND1,ND2 
[NDSURF | Generates surface elements overlaid on the edge of existing elements and assigns the extra node as the closest fluid element node.]
NDSURF,Snode,Telem,DIMN 
[NEQIT | Specifies the maximum number of equilibrium iterations for nonlinear analyses.]
NEQIT,NEQIT 
[NFORCE | Sums the nodal forces and moments of elements attached to nodes.]
NFORCE,ITEM 
[NGEN | Generates additional nodes from a pattern of nodes.]
NGEN,ITIME,INC,NODE1,NODE2,NINC,DX,DY,DZ,SPACE 
[NKPT | Defines a node at an existing keypoint location.]
NKPT,NODE,NPT 
[NLGEOM | Includes large deflection effects in a static or full transient analysis.]
NLGEOM,Key 
[NLIST | Lists nodes.]
NLIST,NODE1,NODE2,NINC,Lcoord,SORT1,SORT2,SORT3 
[NLOG | Forms the natural log of a variable.]
NLOG,IR,IA,--,--,Name,--,--,FACTA,FACTB 
[NLOPT |"Specifies""Nonlinear analysis options""as the subsequent status topic."]
NLOPT 
[NMODIF | Modifies an existing node.]
NMODIF,NODE,X,Y,Z,THXY,THYZ,THZX 
[NOCOLOR | Removes color from graphics displays.]
NOCOLOR,KEY 
[NODES |"Specifies""Nodes""as the subsequent status topic."]
NODES 
[NOOFFSET | Prevents the CDREAD command from offsetting specified data items]
NOOFFSET,Label 
[NOORDER | Re establishes the original element ordering.]
NOORDER,Lab 
[NORA | Rotates nodal coordinate systems to surface normal]
NORA,AREA,NDIR 
[NORL | Rotates nodal coordinate systems perpendicular to line normal]
NORL,LINE,AREA,NDIR 
[NPLOT | Displays nodes.]
NPLOT,KNUM 
[NPRINT | Defines which time points stored are to be listed.]
NPRINT,N 
[NREAD | Reads nodes from a file.]
NREAD,Fname,Ext,-- 
[NREFINE | Refines the mesh around specified nodes.]
NREFINE,NN1,NN2,NINC,LEVEL,DEPTH,POST,RETAIN 
[NRLSUM | Specifies the Naval Research Laboratory (NRL) sum mode combination method.]
NRLSUM,SIGNIF,Label 
[NROPT | Specifies the Newton Raphson options in a static or full transient analysis.]
NROPT,Option,--,Adptky 
[NROTAT | Rotates nodal coordinate systems into the active system.]
NROTAT,NODE1,NODE2,NINC 
[NRRANG | Specifies the range of nodes to be read from the node file.]
NRRANG,NMIN,NMAX,NINC 
[NRRES | Writes Newton Raphson residual information to a file for the specified number of equilibrium iterations.]
NRRES,Key,MaxFile 
[NSCALE | Generates a scaled set of nodes from a pattern of nodes.]
NSCALE,INC,NODE1,NODE2,NINC,RX,RY,RZ 
[NSEL | Selects a subset of nodes.]
NSEL,Type,Item,Comp,VMIN,VMAX,VINC,KABS 
[NSLA | Selects those nodes associated with the selected areas.]
NSLA,Type,NKEY 
[NSLE | Selects those nodes attached to the selected elements.]
NSLE,Type,NodeType,Num 
[NSLK | Selects those nodes associated with the selected keypoints.]
NSLK,Type 
[NSLL | Selects those nodes associated with the selected lines.]
NSLL,Type,NKEY 
[NSLV | Selects those nodes associated with the selected volumes.]
NSLV,Type,NKEY 
[NSMOOTH | Smooths selected nodes among selected elements.]
NSMOOTH,NPASS 
[NSOL | Specifies nodal data to be stored from the results file.]
NSOL,NVAR,NODE,Item,Comp,Name 
[NSORT | Sorts nodal data.]
NSORT,Item,Comp,ORDER,KABS,NUMB,SEL 
[NSTORE | Defines which time points are to be stored.]
NSTORE,TINC 
[NSUBST | Specifies the number of substeps to be taken this load step.]
NSUBST,NSBSTP,NSBMX,NSBMN,Carry 
[NSVR | Defines the number of variables for user programmable element options.]
NSVR,ITYPE,NSTV 
[NSYM | Generates a reflected set of nodes.]
NSYM,Ncomp,INC,NODE1,NODE2,NINC 
[NUMCMP | Compresses the numbering of defined items.]
NUMCMP,Label 
[NUMEXP | Specifies solutions to be expanded from reduced analyses.]
NUMEXP,NUM,BEGRNG,ENDRNG,Elcalc 
[NUMMRG | Merges coincident or equivalently defined items.]
NUMMRG,Label,TOLER,GTOLER,Action,Switch 
[NUMOFF | Adds a number offset to defined items.]
NUMOFF,Label,VALUE 
[NUMSTR | Establishes starting numbers for automatically numbered items.]
NUMSTR,Label,VALUE 
[NUMVAR | Specifies the number of variables allowed in POST26.]
NUMVAR,NV 
[NUSORT | Restores original order for nodal data.]
NUSORT 
[NWPAVE | Moves the working plane origin to the average location of nodes.]
NWPAVE,N1,N2,N3,N4,N5,N6,N7,N8,N9 
[NWPLAN | Defines the working plane using three nodes.]
NWPLAN,WN,NORIG,NXAX,NPLAN 
[NWRITE | Writes nodes to a file.]
NWRITE,Fname,Ext,--,KAPPND 
[OMEGA | Specifies the rotational velocity of the structure.]
OMEGA,OMEGX,OMEGY,OMEGZ,KSPIN 
[OPADD | Forms a set of optimization parameters by adding two sets.]
OPADD,NRES,NUM1,NUM2,C1,C2 
[OPANL | Defines the analysis file to be used for optimization looping.]
OPANL,Fname,Ext,-- 
[OPCLR | Clears the optimization database.]
OPCLR 
[OPDATA | Identifies the file where optimization data is to be saved.]
OPDATA,Fname,Ext,-- 
[OPDEL | Deletes optimization design sets.]
OPDEL,NSET1,NSET2 
[OPEQN | Controls curve fitting for the subproblem approximation method.]
OPEQN,KFOBJ,KFSV,KWGHT,KOPPR,INOPT 
[OPERATE |"Specifies""Operation data""as the subsequent status topic."]
OPERATE 
[OPEXE | Initiates optimization looping.]
OPEXE 
[OPFACT | Defines the type of factorial evaluation to be performed.]
OPFACT,Type 
[OPFRST | Defines specifications for the first order optimization method.]
OPFRST,NITR,SIZE,DELTA 
[OPGRAD | Specifies which design set will be used for gradient evaluation.]
OPGRAD,Dset,DELTA 
[OPKEEP | Specifies whether to save the best set results and database file.]
OPKEEP,Key 
[OPLFA | Displays the results of a factorial evaluation.]
OPLFA,Name,Effect,EMIN,EMAX 
[OPLGR | Graphs the results of a gradient evaluation.]
OPLGR,Pname,Dvnam1,Dvnam2,Dvnam3,Dvnam4,Dvnam5,Dvnam6 
[OPLIST | Displays the parameters for design sets.]
OPLIST,SET1,SET2,LKEY 
[OPLOOP | Specifies controls for optimization looping.]
OPLOOP,Read,Dvar,Parms 
[OPLSW | Graphs the results of a global sweep generation.]
OPLSW,Pname,Dvnam1,Dvnam2,Dvnam3,Dvnam4,Dvnam5,Dvnam6 
[OPMAKE | Creates a design set using active scalar parameter values.]
OPMAKE 
[OPNCONTROL | Sets decision parameter for automatically increasing the time step interval.]
OPNCONTROL,Lab,VALUE,NUMSTEP 
[OPPRNT | Activates detailed optimization summary printout.]
OPPRNT,Key 
[OPRAND | Defines the number of iterations for a random optimization.]
OPRAND,NITR,NFEAS 
[OPRESU | Reads optimization data into the optimization database.]
OPRESU,Fname,Ext,-- 
[OPRFA | Prints the results of a factorial evaluation.]
OPRFA,Name 
[OPRGR | Prints the results of a gradient evaluation.]
OPRGR,Name 
[OPRSW | Prints the results of a global sweep generation.]
OPRSW,Name 
[OPSAVE | Writes all optimization data to a file.]
OPSAVE,Fname,Ext,-- 
[OPSEL | Selects design sets for subsequent optimization looping.]
OPSEL,NSEL 
[OPSUBP | Defines number of iterations for subproblem approximation method.]
OPSUBP,NITR,NINFS 
[OPSWEEP | Specifies the reference point and number of evaluation points for a sweep generation.]
OPSWEEP,Dset,NSPS 
[OPTYPE | Specifies the optimization method to be used.]
OPTYPE,Mname 
[OPUSER | Defines specifications for user supplied external optimization.]
OPUSER,NITR,VAL1,VAL2,VAL3,VAL4,VAL5,VAL6,VAL7,VAL8 
[OPVAR | Specifies the parameters to be treated as optimization variables.]
OPVAR,Name,Type,MIN,MAX,TOLER 
[OUTOPT |"Specifies""Output options""as the subsequent status topic."]
OUTOPT 
[OUTPR | Controls the solution printout.]
OUTPR,Item,FREQ,Cname 
[OUTRES | Controls the solution data written to the database.]
OUTRES,Item,FREQ,Cname 
[PADELE | Deletes a defined path.]
PADELE,DELOPT 
[PAGET | Writes current path information into an array variable.]
PAGET,PARRAY,POPT 
[PAPUT | Retrieves path information from an array variable.]
PAPUT,PARRAY,POPT 
[PARESU | Restores previously saved paths from a file.]
PARESU,Lab,Fname,Ext,-- 
[PARRES | Reads parameters from a file.]
PARRES,Lab,Fname,Ext,-- 
[PARSAV | Writes parameters to a file.]
PARSAV,Lab,Fname,Ext,-- 
[PARTSEL | Selects a subset of parts in an explicit dynamic analysis.]
PARTSEL,Type,PMIN,PMAX,PINC 
[PASAVE | Saves selected paths to an external file.]
PASAVE,Lab,Fname,Ext,-- 
[PATH | Defines a path name and establishes parameters for the path.]
PATH,NAME,nPts,nSets,nDiv 
[PCALC | Forms additional labeled path items by operating on existing path items.]
PCALC,Oper,LabR,Lab1,Lab2,FACT1,FACT2,CONST 
[PCIRC | Creates a circular area centered about the working plane origin.]
PCIRC,RAD1,RAD2,THETA1,THETA2 
[PCONV | Sets convergence values for p method solutions.]
PCONV,TOLER,Item,Comp,NODE,Surf 
[PCORRO | Specifies the allowable exterior corrosion thickness for a piping run.]
PCORRO,CTK 
[PCROSS | Calculates the cross product of two path vectors along the current path.]
PCROSS,LabXR,LabYR,LabZR,LabX1,LabY1,LabZ1,LabX2,LabY2,LabZ2 
[PDANL | Defines the analysis file to be used for probabilistic looping.]
PDANL,Fname,Ext,-- 
[PDCDF | Plots the cumulative distribution function.]
PDCDF,Rlab,Name,Type,CONF,NMAX 
[PDCFLD | Calculates a correlation field and stores it into an ANSYS array.]
PDCFLD,ParR,Entity,Ctype,CLENGTH 
[PDCLR | Clears the probabilistic design database.]
PDCLR,Type 
[PDCMAT | Prints the correlation coefficient matrix.]
PDCMAT,Rlab,Matrix,Name1,Name2,Corr,SLEVEL,Popt 
[PDCORR | Specifies the correlation between two random input variables.]
PDCORR,Name1,Name2,CORR 
[PDDMCS | Specifies options for Monte Carlo Simulations using direct sampling.]
PDDMCS,NSIM,--,Astop,ACCMEAN,ACCSTDEV,CHECK,Seed 
[PDDOEL | Defines design of experiment levels for an individual random input variable.]
PDDOEL,Name,Method,Vtype,Lopt,VAL1,VAL2,VAL3,VAL4,VAL5 
[PDEF | Interpolates an item onto a path.]
PDEF,Lab,Item,Comp,Avglab 
[PDEXE | Executes the probabilistic analysis.]
PDEXE,Slab,MRUN,NFAIL,FOPT,Fname 
[PDHIST | Plots the frequency histogram.]
PDHIST,Rlab,Name,NCL,Type 
[PDINQR | Evaluates statistical characteristics of a random input variable.]
PDINQR,Rpar,Name,Type,VAL 
[PDLHS | Specifies options for Monte Carlo Simulations using Latin Hypercube sampling.]
PDLHS,NSIM,NREP,ISopt,--,Astop,ACCMEAN,ACCSTDV,CHECK,Seed 
[PDMETH | Specifies the probabilistic analysis method.]
PDMETH,Method,Samp 
[PDOT | Calculates the dot product of two path vectors along the current path.]
PDOT,LabR,LabX1,LabY1,LabZ1,LabX2,LabY2,LabZ2 
[PDPINV | Prints the result of the inversion of a probability.]
PDPINV,Rlab,Name,PROB,--,CONF 
[PDPLOT | Plots the distribution curves of a defined random input variable.]
PDPLOT,Name,PLOW,PUP 
[PDPROB | Prints a probability result.]
PDPROB,Rlab,Name,Relation,LIMIT,--,CONF 
[PDRAG | Defines the external fluid drag loading for a piping run.]
PDRAG,PX1,PY1,PZ1,H1,PX2,PY2,PZ2,H2,Kcord 
[PDRESU | Reads the probabilistic model data and loads it into the database.]
PDRESU,Fname,Ext,-- 
[PDROPT | Specifies the options for an HTML report.]
PDROPT,RVAR,CORR,STAT,SHIS,HIST,CDF,SENS,CMAT,CONF 
[PDSAVE | Writes the probabilistic model data to a file.]
PDSAVE,Fname,Ext,-- 
[PDSCAT | Plots a scatter graph.]
PDSCAT,Rlab,Name1,Name2,Type,ORDER,NMAX 
[PDSENS | Plots the probabilistic sensitivities.]
PDSENS,Rlab,Name,Chart,Type,SLEVEL 
[PDSHIS | Plots the sample history values.]
PDSHIS,Rlab,Name,Type,CONF 
[PDUSER | Specifies options for user specified sampling methods.]
PDUSER,Fname,Ext,-- 
[PDVAR | Specifies the parameters to be treated as probabilistic design variables.]
PDVAR,Name,Type,PAR1,PAR2,PAR3,PAR4 
[PDWRITE | Generates an HTML report for the probabilistic analyses.]
PDWRITE,File,Fnam,Lnam 
[PEMOPTS | Defines percentage tolerance and error estimation method for electrostatic p Method solution.]
PEMOPTS,TOLER,Method 
[PERBC2D | Generates periodic constraints for 2 D planar magnetic field analyses.]
PERBC2D,LOC1,LOC2,LOCTOL,R1,R2,TOLR,OPT,PLNOPT 
[PERI | Specifies periodic boundary conditions in an incompressible flow analysis.]
PERI,DX,DY,DZ 
[PEXCLUDE | Specifies elements to be excluded from p level escalations.]
PEXCLUDE,ELEM 
[PFACT | Calculates participation factors for the PSD or multi point response spectrum table.]
PFACT,TBLNO,Excit,Parcor 
[PFLUID | Defines the contained fluid density for a piping run.]
PFLUID,DENS 
[PGAP | Defines a spring gap constraint in a piping run.]
PGAP,NLOC,K,DX,DY,DZ,GAP,ELEM 
[PGRAPH | Specifies the location from which graphics data will be retrieved for viewing.]
PGRAPH,Option,Fname,Fext,-- 
[PGRSET | Defines the data set to be read from the PGR file.]
PGRSET,Lstep,SBSTEP,--,KIMG,TIME,--,NSET 
[PGSAVE | Creates a PowerGraphics (PGR) file from results data.]
PGSAVE,Fname,Fext,--,DataType,InteriorKey,Append 
[PGSELE | Select a subset of elements for display with the PGR viewer.]
PGSELE,Type,Item,,VMIN,VMAX,VINC 
[PGWRITE | Writes selected solution data to the PGR file for faster post processing access.]
PGWRITE,Label,Fname,Fext,--,DataType,InteriorKey,Append 
[PHYSICS | Writes,reads,or lists all element information]
PHYSICS,Option,Title,Fname,Ext,-- 
[PINCLUDE | Specifies elements to be included in p level escalations.]
PINCLUDE,ELEM 
[PINSUL | Defines the external insulation constants in a piping run.]
PINSUL,DENS,ITK 
[PIPE |"Specifies""Pipe modeling""as the subsequent status topic."]
PIPE 
[PIVCHECK | Prevents a batch mode,linear static analysis from stopping when a negative or zero equation solver pivot value is encountered.]
PIVCHECK,KEY 
[PLCONV | Plots the convergence curve for specified items from a p method solution.]
PLCONV,Item,Comp,NODE,Surf 
[PLCPLX | Specifies the part of a complex variable to display.]
PLCPLX,KEY 
[PLCRACK | Displays cracking and crushing locations in SOLID65 elements.]
PLCRACK,LOC,NUM 
[PLDISP | Displays the displaced structure.]
PLDISP,KUND 
[PLESOL | Displays the solution results as discontinuous element contours.]
PLESOL,Item,Comp,KUND,Fact 
[PLETAB | Displays element table items.]
PLETAB,Itlab,Avglab 
[PLF2D | Generates a contour line plot of equipotentials.]
PLF2D,NCONT,OLAY,ANUM,WIN 
[PLHFFAR | Displays electromagnetic far fields far field parameters.]
PLHFFAR,Opt,Lab,PHI1,PHI2,NPHI,THETA1,THETA2,NTHETA,RADIUS,CS,Comp
[PLLS | Displays element table items as contoured areas along elements.]
PLLS,LabI,LabJ,Fact,KUND 
[PLNSOL | Displays results as continuous contours.]
PLNSOL,Item,Comp,KUND,Fact,FileID 
[PLOT | Forms a display.]
PLOT,NSTRT,NEND,NINC 
[PLOTTING |"Specifies""Plotting settings""as the subsequent status topic."]
PLOTTING 
[PLPAGM | Displays path items along the path geometry.]
PLPAGM,Item,Gscale,Nopt 
[PLPATH | Displays path items on a graph.]
PLPATH,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6 
[PLSECT | Displays membrane and membrane plus bending linearized stresses.]
PLSECT,Item,Comp,RHO,KBR 
[PLSP | Displays S parameters on an XY graph.]
PLSP,Opt,Pnum1,Pnum2,Pnum3,Pnum4,Pnum5,Pnum6 
[PLTIME | Defines the time range for which data are to be displayed.]
PLTIME,TMIN,TMAX 
[PLTRAC | Displays a particle flow or charged particle trace on an element display.]
PLTRAC,Analopt,Item,Comp,TRPNum,Name,MXLOOP,TOLER,OPTION 
[PLVAR | Displays up to ten variables in the form of a graph.]
PLVAR,NVAR1,NVAR2,NVAR3,NVAR4,NVAR5,NVAR6,NVAR7,NVAR8,NVAR9,NVAR10 
[PLVAROPT | Displays up to ten parameters in the form of a graph.]
PLVAROPT,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6,Lab7,Lab8,Lab9,Lab10 
[PLVECT | Displays results as vectors.]
PLVECT,Item,Lab2,Lab3,LabP,Mode,Loc,Edge 
[PLVFRC | Displays volume fractions in a volume of fluid (VOF) analysis.]
PLVFRC,CONT 
[PLWAVE | Specifies a free space time harmonic incident plane electromagnetic wave.]
PLWAVE,Ex,Ey,Ez,AngX,AngZ 
[PMAP | Creates mapping of the path geometry by defining path interpolation division points.]
PMAP,FORM,DISCON 
[PMETH |"Specifies""p""Method""as the subsequent status topic."]
PMETH 
[PMGTRAN | Summarizes electromagnetic results from a transient analysis.]
PMGTRAN,Fname,FREQ,Fcnam1,Fcnam2,Pcnam1,Pcnam2,Ecnam1,Ccnam1 
[PMLOPT | Defines perfectly matched layers (PMLs) for a high frequency analysis.]
PMLOPT,ESYS,Lab,Xminus,Xplus,Yminus,Yplus,Zminus,Zplus 
[PMOPTS | Defines percentage tolerance for a p Method solution.]
PMOPTS,TOLER 
[PNGR | Provides PNG file export for ANSYS displays.]
PNGR,Kywrd,OPT,VAL 
[POINT |"Specifies""Point flow tracing settings""as the subsequent status topic."]
POINT 
[POLY | Creates a polygonal area based on working plane coordinate pairs.]
POLY 
[POPT | Selects the piping analysis standard for a piping run.]
POPT,Lop1 
[POUTRES | controls the nodal DOF and computed element results graphics data that is written to the PGR file.]
POUTRES,Item1,Item2,Item2,.........Item12,
[POWERH | Calculates the rms power loss in a conductor or lossy dielectric.]
POWERH 
[PPATH | Defines a path by picking or defining nodes,or locations on the currently active working plane,or by entering specific coordinate locations.]
PPATH,POINT,NODE,X,Y,Z,CS 
[PPLOT | Displays an element plot indicating each element's final p level.]
PPLOT 
[PPRANGE | Specifies a range of p level values for use in a p method solution.]
PPRANGE,START,MAX 
[PPRES | Defines the internal pressure for a piping run.]
PPRES,PRESS 
[PRANGE | Determines the pathrange.]
PRANGE,LINC,VMIN,VMAX,XVAR 
[PRCONV | Lists convergence values versus characteristic p level.]
PRCONV 
[PRCPLX | Defines the output form for complex variables.]
PRCPLX,KEY 
[PRECISION | Specifies machine precision for solvers (currently valid only for PCG solvers).]
PRECISION,LABEL 
[PRED | Activates a predictor in a nonlinear analysis.]
PRED,Sskey,--,Lskey 
[PRERR | Prints SEPC and TEPC.]
PRERR 
[PRESOL | Prints the solution results for elements.]
PRESOL,Item,Comp 
[PRETAB | Prints the element table items.]
PRETAB,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6,Lab7,Lab8,Lab9 
[PRHFFAR | Prints electromagnetic far fields and far field parameters.]
PRHFFAR,Opt,Lab,PHI1,PHI2,NPHI,THETA1,THETA2,NTHETA,RADIUS,CS,Comp 
[PRI2 | Creates a polygonal area or a prism volume by vertices (GUI).]
PRI2,P51X,Z1,Z2 
[PRIM |"Specifies""Solid model primitives""as the subsequent status topic."]
PRIM 
[PRINT |"Specifies""Print settings""as the subsequent status topic."]
PRINT 
[PRISM | Creates a prism volume based on working plane coordinate pairs.]
PRISM,Z1,Z2 
[PRITER | Prints solution summary data.]
PRITER 
[PRNLD | Prints the summed element nodal loads.]
PRNLD,Lab,TOL,Item 
[PRNSOL | Prints the nodal solution results.]
PRNSOL,Item,Comp 
[PROD | Multiplies variables.]
PROD,IR,IA,IB,IC,Name,--,--,FACTA,FACTB,FACTC 
[PRPATH | Prints path items along a geometry path.]
PRPATH,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6 
[PRRFOR | Used with the FORCE command. Prints the constrained node reaction solution.]
PRRFOR,Lab 
[PRRSOL | Prints the constrained node reaction solution.]
PRRSOL,Lab 
[PRSECT | Calculates and prints linearized stresses along a section path.]
PRSECT,RHO,KBR 
[PRSSOL | Prints BEAM188 and BEAM189 section results.]
PRSSOL,Item,Comp 
[PRTIME | Defines the time range for which data are to be listed.]
PRTIME,TMIN,TMAX 
[PRVAR | Lists variables vs. time (or frequency).]
PRVAR,NVAR1,NVAR2,NVAR3,NVAR4,NVAR5,NVAR6 
[PRVAROPT | Lists up to ten optimization parameters.]
PRVAROPT,Lab1,Lab2,Lab3,Lab4,Lab5,Lab6,Lab7,Lab8,Lab9,Lab10 
[PRVECT | Prints results as vector magnitude and direction cosines.]
PRVECT,Item,Lab2,Lab3,LabP 
[PSCR | Specifies various PostScript options.]
PSCR,Kywrd,KEY 
[PSDCOM | Specifies the power spectral density mode combination method.]
PSDCOM,SIGNIF,COMODE 
[PSDFRQ | Defines the frequency points for the input spectrum vs. FREQ tables of PSD and multi point spectrum analyses.]
PSDFRQ,TBLNO1,TBLNO2,FREQ1,FREQ2,FREQ3,FREQ4,FREQ5,FREQ6,FREQ7 
[PSDGRAPH | Displays input PSD curves]
PSDGRAPH,TBLNO1,TBLNO2 
[PSDRES | Controls solution output written to the results file from a PSD analysis.]
PSDRES,Lab,RelKey 
[PSDSPL | Defines a partially correlated excitation in a PSD analysis.]
PSDSPL,TBLNO,RMIN,RMAX 
[PSDUNIT | Defines the type of PSD or multi point response spectrum.]
PSDUNIT,TBLNO,Type,GVALUE 
[PSDVAL | Defines PSD or multi point response spectrum values.]
PSDVAL,TBLNO,SV1,SV2,SV3,SV4,SV5,SV6,SV7 
[PSDWAV | Defines a wave propagation excitation in a PSD analysis.]
PSDWAV,TBLNO,VX,VY,VZ 
[PSEL | Selects a path or paths.]
PSEL,Type,Pname1,Pname2,Pname3,Pname4,Pname5,Pname6,Pname7,Pname8,Pname9,Pname10 
[PSMESH | Create and mesh a pretension section]
PSMESH,SECID,Name,P0,Egroup,NUM,KCN ,KDIR,VALUE,NDPLANE,PSTOL,PSTYPE,ECOMP,NCOMP 
[PSOLVE | Directs the program to perform a partial solution.]
PSOLVE,Lab 
[PSPEC | Defines pipe material and dimensions.]
PSPEC,MAT,DNOM,SCHED,OD,TK 
[PSPRNG | Defines a spring constraint in a piping run.]
PSPRNG,NLOC,TYPE,K,DX,DY,DZ,ELEM 
[PSTRES | Specifies whether prestress effects are to be included.]
PSTRES,Key 
[PTEMP | Defines the pipe wall temperatures in a piping run.]
PTEMP,TOUT,TIN 
[PTXY | Defines coordinate pairs for use in polygons and prisms.]
PTXY,X1,Y1,X2,Y2,X3,Y3,X4,Y4 
[PUNIT | Selects the system of length units to be used in a piping run.]
PUNIT,KOPT 
[PVECT | Interpolates a set of items onto a path.]
PVECT,Oper,LabXR,LabYR,LabZR 
[QDVAL | Defines PSD quadspectral values.]
QDVAL,TBLNO1,TBLNO2,SV1,SV2,SV3,SV4,SV5,SV6,SV7
[QFACT | Calculates the quality factor for high frequency electromagnetic resonators.]
QFACT 
[QSOPT | Specifies quasi static radiation options.]
QSOPT,Opt 
[QUAD | Generates a quadratic line of nodes from three nodes.]
QUAD,NODE1,NINTR,NODE2,NFILL,NSTRT,NINC,PKFAC 
[QUOT | Divides two variables.]
QUOT,IR,IA,IB,--,Name,--,--,FACTA,FACTB
[R | Defines the element real constants.]
R,NSET,R1,R2,R3,R4,R5,R6 
[RACE |"Defines a""racetrack""current source."]
RACE,XC,YC,RAD,TCUR,DY,DZ,--,--,Cname
[RADOPT | Specifies Gauss Seidel Radiosity Solver options.]
RADOPT,FLUXRELX,FLUXTOL,SOLVER,MAXITER,TOLER,OVERRLEX 
[RALL | Calculates solver statistics and run time estimates.]
RALL 
[RAPPND | Appends results data from the database to the results file.]
RAPPND,LSTEP,TIME 
[RATE | Specifies whether the effect of creep strain rate will be used in the solution of a load step.]
RATE,Option 
[RBE3 | Distributes the force/moment applied at the master node to a set of slave nodes,taking into account the geometry of the slave nodes as well as weighting factors.]
RBE3,Master,DOF,Slaves,Wtfact 
[RCON |"Specifies""Real constants""as the subsequent status topic."]
RCON 
[RDELE | Deletes real constant sets.]
RDELE,NSET1,NSET2,NINC 
[REAL | Sets the element real constant set attribute pointer.]
REAL,NSET 
[REALVAR | Forms a variable using only the real part of a complex variable.]
REALVAR,IR,IA,--,--,Name,--,--,FACTA
[RECTNG | Creates a rectangular area anywhere on the working plane.]
RECTNG,X1,X2,Y1,Y2 
[REDUCE | Defines a reducer in a piping run.]
REDUCE,NLOC,LENG,ELEM 
[REFLCOEF |"Calculates the voltage reflection coefficient (REFLC),standing wave ratio (VSWR),and return loss (RL) in a COAX fed device; at postprocessing of an HF electromagnetic analysis."]
REFLCOEF,Portin,Pvolt,Pang,Pdist,Vpathy 
[REORDER |"Specifies""Model reordering""as the subsequent status topic."]
REORDER 
[RESCONTROL | Controls file writing for multiframe restarts.]
RESCONTROL,Action,Ldstep,Frequency,MAXFILES 
[RESET | Resets all POST1 or POST26 specifications to initial defaults.]
RESET 
[RESP | Generates a response spectrum.]
RESP,IR,LFTAB,LDTAB,ITYPE,RATIO,DTIME,TMIN,TMAX 
[RESUME | Resumes the database from the database file.]
RESUME,Fname,Ext,--,NOPAR,KNOPLOT 
[REXPORT | Exports displacements from an implicit run to ANSYS LS DYNA.]
REXPORT,Target,--,--,LSTEP,SBSTEP,Fname,Ext,-- 
[RFILSZ | Estimates file sizes.]
RFILSZ 
[RFORCE | Specifies the total reaction force data to be stored.]
RFORCE,NVAR,NODE,Item,Comp,Name 
[RIGID | Specifies known rigid body modes (if any) of the model.]
RIGID,Dof1,Dof2,Dof3,Dof4,Dof5,Dof6 
[RIMPORT | Imports initial stresses from an explicit dynamics run into ANSYS.]
RIMPORT,Source,Type,Loc,LSTEP,SBSTEP,Fname,Ext,--,SPSCALE,MSCALE
[RITER | Supplies an estimate of the number of iterations for time estimates.]
RITER,NITER 
[RLIST | Lists the real constant sets.]
RLIST,NSET1,NSET2,NINC 
[RMALIST | Lists all defined master nodes for a ROM method.]
RMALIST 
[RMANL | Assigns model database,dimensionality,and operating direction for the ROM method.]
RMANL,Fname,Ext,--,Dimn,Oper
[RMASTER | Defines master nodes for the ROM method.]
RMASTER,Node,Lab 
[RMCAP | Defines lumped capacitance pairs between conductors C1 and C2 for a ROM method.]
RMCAP,RefName,C1,C2 
[RMCLIST | Lists all lumped capacitance pairs defined.]
RMCLIST 
[RMEMRY | Prints memory statistics for the current model.]
RMEMRY 
[RMLVSCALE | Defines element load vector scaling for a ROM use pass.]
RMLVSCALE,Nload,Fact1,Fact2,Fact3,Fact4,Fact5 
[RMMLIST | Lists all mode specifications for the ROM method.]
RMMLIST 
[RMMRANGE | Defines and edits various modal parameters for the ROM method.]
RMMRANGE,Mode,Key,Min,Max,Nstep,Damp,Scale 
[RMMSELECT | Selects modes for the ROM method.]
RMMSELECT,Nmode,Method,Dmin,Dmax 
[RMNDISP | Extracts neutral plane displacements from a test load or element load solution for the ROM method.]
RMNDISP,LoadT,Loc 
[RMNEVEC | Extracts neutral plane eigenvectors from a modal analysis for the ROM method.]
RMNEVEC 
[RMODIF | Modifies real constant sets.]
RMODIF,NSET,STLOC,V1,V2,V3,V4,V5,V6
[RMORE | Adds real constants to a set.]
RMORE,R7,R8,R9,R10,R11,R12 
[RMPORDER | Defines polynomial orders for ROM functions.]
RMPORDER,Ord1,Ord2,Ord3,Ord4,Ord5,Ord6,Ord7,Ord8,Ord9
[RMRESUME | Resumes ROM data from a file.]
RMRESUME,Fname,Ext,-- 
[RMRGENERATE | Performs fitting procedure for all ROM functions to generate response surfaces.]
RMRGENERATE 
[RMROPTIONS | Defines options for ROM response surface fitting.]
RMROPTIONS,RefName,Type,Invert 
[RMRPLOT | Plots response surface of ROM function or its derivatives with respect to the dominant mode(s).]
RMRPLOT,RefName,Type,Mode1,Mode2 
[RMRSTATUS | Prints status of response surface for ROM function.]
RMRSTATUS,RefName 
[RMSAVE | Saves ROM data to file.]
RMSAVE,Fname,Ext,-- 
[RMSMPLE | Runs finite element solutions and obtains sample points for the ROM method.]
RMSMPLE,Nlgeom,Cap,Seqslv,Eeqslv 
[RMUSE | Activates ROM use pass for ROM elements.]
RMUSE,Option,Usefil 
[RMXPORT | Exports ROM model to external VHDL AMS simulator.]
RMXPORT 
[ROCK | Specifies a rocking response spectrum.]
ROCK,CGX,CGY,CGZ,OMX,OMY,OMZ 
[RPOLY | Creates a regular polygonal area centered about the working plane origin.]
RPOLY,NSIDES,LSIDE,MAJRAD,MINRAD 
[RPR4 | Creates a regular polygonal area or prism volume anywhere on the working plane.]
RPR4,NSIDES,XCENTER,YCENTER,RADIUS,THETA,DEPTH 
[RPRISM | Creates a regular prism volume centered about the working plane origin.]
RPRISM,Z1,Z2,NSIDES,LSIDE,MAJRAD,MINRAD 
[RPSD | Computes response power spectral density (PSD).]
RPSD,IR,IA,IB,ITYPE,DATUM,Name 
[RSFIT | Fit a response surface for an output parameter in a solution set.]
RSFIT,RSlab,Slab,Name,Rmod,Ytrans,Yval,Xfilt,CONF
[RSPEED | Supplies system performance information for use in time estimates.]
RSPEED,MIPS,SMFLOP,VMFLOP 
[RSPLOT | Plot a response surface.]
RSPLOT,RSlab,YName,X1Name,X2Name,Type,NPTS,PLOW,PUP
[RSPRNT | Print a response surface.]
RSPRNT,RSlab,YName 
[RSSIMS | Performs Monte Carlo simulations on response surface(s).]
RSSIMS,RSlab,NSIM,Seed 
[RSTAT | Prints the FE model statistics of the model.]
RSTAT 
[RSYS | Activates a coordinate system for printout or display of results.]
RSYS,KCN 
[RTHICK | Defines variable thickness at nodes for shell elements.]
RTHICK,Par,ILOC,JLOC,KLOC,LLOC 
[RTIMST | Prints runtime estimates.]
RTIMST 
[RUN | Defines a pipe run.]
RUN,DX,DY,DZ,NDIV,NEND,ESTRT,EINC
[RWFRNT | Generates wavefront statistics and memory requirements.]
RWFRNT 
[SABS | Specifies absolute values for element table operations.]
SABS,KEY 
[SADD | Forms an element table item by adding two existing items.]
SADD,LabR,Lab1,Lab2,FACT1,FACT2,CONST 
[SALLOW | Defines the allowable stress table for safety factor calculations.]
SALLOW,STRS1,STRS2,STRS3,STRS4,STRS5,STRS6 
[SARPLOT | Displays areas smaller than a specified size (for models imported from CAD files).]
SARPLOT,Prefer,VALUE 
[SAVE | Saves all current database information.]
SAVE,Fname,Ext,--,Slab 
[SBCLIST | Lists solid model boundary conditions.]
SBCLIST 
[SBCTRAN | Transfers solid model loads and boundary conditions to the FE model.]
SBCTRAN 
[SDELETE | DeletingsectionsCross sectionsSectionsDeletes cross sections from the ANSYS database.]
SDELETE,SFIRST,SLAST,SINC,KNOCLEAN 
[SE | Defines a superelement.]
SE,File,--,--,TOLER 
[SECCONTROLS | Overrides program calculated properties.]
SECCONTROLS VAL1,VAL2,VAL3,VAL4,VAL5,VAL6,VAL7 
[SECDATA | Sectionsdescribing geometry ofSubtypes of sectionsSectionssubtypesDescribes the geometry of a section.]
SECDATA,VAL1,VAL2,VAL3,VAL4,VAL5,VAL6,VAL7,VAL8,VAL9,VAL10
[SECFUNCTION | Specifies shell section thickness as a tabular function.]
SECFUNCTION,TABLE 
[SECMODIF | Modifies a pretension section]
SECMODIF,SECID,Kywrd 
[SECNUM | Section IDSets the element section attribute pointer.]
SECNUM,SECID 
[SECOFFSET | Sectionsdefining offset ofOffsets for sectionsDefines the section offset for cross sections.]
SECOFFSET,Location,OFFSET1,OFFSET2,CG-Y,CG-Z,SH-Y,SH-Z
[SECPLOT | PlottingsectionsPlots the geometry of a beam or shell section to scale.]
SECPLOT,SECID,VAL1,VAL2 
[SECREAD | Readinguser defined section libraryReads a customized beam section library or a user defined beam section mesh into ANSYS.]
SECREAD,Fname,Ext,--,Option 
[SECTYPE | Sectionsassociating subtype with ID numberAssociates section type information with a section ID number.]
SECTYPE,SECID,Type,Subtype,Name,REFINEKEY 
[SECWRITE | User mesh section filesWritinguser mesh section informationCreates an ASCII file containing user mesh section information.]
SECWRITE,Fname,Ext,--,ELEM_TYPE 
[SED | Defines the excitation direction for a single point response spectrum.]
SED,SEDX,SEDY,SEDZ 
[SEDLIST | Lists the DOF solution of a superelement after the use pass.]
SEDLIST,Sename,KOPT 
[SEEXP | Specifies options for the substructure expansion pass.]
SEEXP,Sename,Usefil,Imagky 
[SELIST | Lists the contents of a superelement matrix file.]
SELIST,Sename,KOPT 
[SELM |"Specifies""Superelements""as the subsequent status topic."]
SELM 
[SENERGY | Determines the stored magnetic energy or co energy.]
SENERGY,OPT,ANTYPE 
[SEOPT | Specifies substructure analysis options.]
SEOPT,Sename,SEMATR,SEPR,SESST,EXPMTH 
[SESYMM | Performs a symmetry operation on a superelement within the use pass.]
SESYMM,Sename,Ncomp,INC,File,Ext,-- 
[SET | Defines the data set to be read from the results file.]
SET,Lstep,SBSTEP,FACT,KIMG,TIME,ANGLE,NSET,ORDER 
[SETRAN | Creates a superelement from an existing superelement.]
SETRAN,Sename,KCNTO,INC,File,Ext,--,DX,DY,DZ,NOROT
[SEXP | Forms an element table item by exponentiating and multiplying.]
SEXP,LabR,Lab1,Lab2,EXP1,EXP2 
[SF | Specifies surface loads on nodes.]
SF,Nlist,Lab,VALUE,VALUE2 
[SFA | Specifies surface loads on the selected areas.]
SFA,AREA,LKEY,Lab,VALUE,VALUE2 
[SFACT | Allows safety factor or margin of safety calculations to be made.]
SFACT,TYPE 
[SFADELE | Deletes surface loads from areas.]
SFADELE,AREA,LKEY,Lab 
[SFALIST | Lists the surface loads for the specified area.]
SFALIST,AREA,Lab 
[SFBEAM | Specifies surface loads on beam elements.]
SFBEAM,ELEM,LKEY,Lab,VALI,VALJ,VAL2I,VAL2J,IOFFST,JOFFST
[SFCALC | Calculates the safety factor or margin of safety.]
SFCALC,LabR,LabS,LabT,TYPE 
[SFCUM | Specifies that surface loads are to be accumulated.]
SFCUM,Lab,Oper,FACT,FACT2 
[SFDELE | Deletes surface loads.]
SFDELE,Nlist,Lab 
[SFE | Specifies surface loads on elements.]
SFE,ELEM,LKEY,Lab,KVAL,VAL1,VAL2,VAL3,VAL4
[SFEDELE | Deletes surface loads from elements.]
SFEDELE,ELEM,LKEY,Lab 
[SFELIST | Lists the surface loads for elements.]
SFELIST,ELEM,Lab 
[SFFUN | Specifies a varying surface load.]
SFFUN,Lab,Par,Par2 
[SFGRAD | Specifies a gradient (slope) for surface loads.]
SFGRAD,Lab,SLKCN,Sldir,SLZER,SLOPE 
[SFL | Specifies surface loads on lines of an area.]
SFL,LINE,Lab,VALI,VALJ,VAL2I,VAL2J 
[SFLDELE | Deletes surface loads from lines.]
SFLDELE,LINE,Lab 
[SFLIST | Lists surface loads.]
SFLIST,NODE,Lab 
[SFLLIST | Lists the surface loads for lines.]
SFLLIST,LINE,Lab 
[SFSCALE | Scales surface loads on elements.]
SFSCALE,Lab,FACT,FACT2 
[SFTRAN | Transfer the solid model surface loads to the finite element model.]
SFTRAN 
[SHELL | Selects a shell element or shell layer location for results output.]
SHELL,Loc 
[SHPP | Controls element shape checking.]
SHPP,Lab,VALUE1,VALUE2 
[SLIST | Listingsection propertiesSummarizes the section properties for all defined sections in the current session of ANSYS.]
SLIST,SFIRST,SLAST,SINC,Details,Type 
[SLOAD | Load a pretension section.]
SLOAD,SECID,STLOC,VAL1,VAL2,VAL3,VAL4,VAL5,VAL6
[SLPPLOT | Displays line loops smaller than a specified size (for models imported from CAD files).]
SLPPLOT,Prefer,VALUE 
[SLSPLOT | Displays line segments smaller than a specified size (for models imported from CAD files).]
SLSPLOT,Prefer,VALUE 
[SMALL | Finds the smallest of three variables.]
SMALL,IR,IA,IB,IC,Name,--,--,FACTA,FACTB,FACTC
[SMAX | Forms an element table item from the maximum of two other items.]
SMAX,LabR,Lab1,Lab2,FACT1,FACT2 
[SMBODY |"Specifies""Body loads on the solid model""as the subsequent status topic."]
SMBODY 
[SMCONS |"Specifies""Constraints on the solid model""as the subsequent status topic."]
SMCONS 
[SMFOR |"Specifies""Forces on the solid model""as the subsequent status topic."]
SMFOR 
[SMIN | Forms an element table item from the minimum of two other items.]
SMIN,LabR,Lab1,Lab2,FACT1,FACT2 
[SMOOTH | Allows smoothing of noisy data and provides a graphical representation of the data.]
SMOOTH,Vect1,Vect2,DATAP,FITPT,Vect3,Vect4,DISP 
[SMRTSIZE | Specifies meshing parameters for automatic (smart) element sizing.]
SMRTSIZE,SIZLVL,FAC,EXPND,TRANS,ANGL,ANGH,GRATIO,SMHLC,SMANC,MXITR,SPRX
[SMSURF |"Specifies""Surface loads on the solid model""as the subsequent status topic."]
SMSURF 
[SMULT | Forms an element table item by multiplying two other items.]
SMULT,LabR,Lab1,Lab2,FACT1,FACT2 
[SOLCONTROL | Specifies whether to use optimized nonlinear solution defaults and some enhanced internal solution algorithms.]
SOLCONTROL,Key1,Key2,Key3,Vtol 
[SOLU | Specifies solution summary data per substep to be stored.]
SOLU,NVAR,Item,Comp,Name 
[SOLUOPT |"Specifies""Solution options""as the subsequent status topic."]
SOLUOPT 
[SOLVE | Starts a solution.]
SOLVE 
[SORT |"Specifies""Sort settings""as the subsequent status topic."]
SORT 
[SOURCE | Defines a default location for undefined nodes or keypoints. ]
SOURCE,X,Y,Z 
[SPACE | Defines a space node for radiation using the Radiation Matrix method. ]
SPACE,NODE 
[SPARM | Calculates scattering (S) parameters between ports of a network system. ]
SPARM,Porti,Portj 
[SPCNOD | Defines a space node for radiation using the Radiosity method. ]
SPCNOD,ENCL,NODE 
[SPCTEMP | Defines a free space ambient temperature for radiation using the Radiosity method. ]
SPCTEMP,ENCL,TEMP 
[SPEC |"Specifies""Miscellaneous specifications""as the subsequent status topic."]
SPEC 
[SPH4 | Creates a spherical volume anywhere on the working plane. ]
SPH4,XCENTER,YCENTER,RAD1,RAD2
[SPH5 | Creates a spherical volume by diameter end points.]
SPH5,XEDGE1,YEDGE1,XEDGE2,YEDGE2 
[SPHERE | Creates a spherical volume centered about the working plane origin.]
SPHERE,RAD1,RAD2,THETA1,THETA2 
[SPLINE | Generates a segmented spline through a series of keypoints.]
SPLINE,P1,P2,P3,P4,P5,P6,XV1,YV1,ZV1,XV6,YV6,ZV6
[SPLOT | Displays the selected areas and a faceted view of their underlying surfaces]
SPLOT,NA1,NA2,NINC,MESH 
[SPOINT | Defines a point for moment summations.]
SPOINT,NODE,X,Y,Z 
[SPOPT | Selects the spectrum type and other spectrum options.]
SPOPT,Sptype,NMODE,Elcalc 
[SPREAD | Turns on a dashed tolerance curve for the subsequent curve plots.]
SPREAD,VALUE 
[SPSWP | Computes S parameters over a frequency range and writes them to a file.]
SPSWP,FREQB,FREQE,FREQINC,SwpOpt,EFAcc,OutPut,FileOpt 
[SPTOPT |"Specifies""Spectrum analysis options""as the subsequent status topic."]
SPTOPT 
[SQRT | Forms the square root of a variable.]
SQRT,IR,IA,--,--,Name,--,--,FACTA
[SRSS | Specifies the square root of sum of squares mode combination method.]
SRSS,SIGNIF,Label 
[SSLN | Selects and displays small lines in the model.]
SSLN,FACT,SIZE 
[SSTIF | Activates stress stiffness effects in a nonlinear analysis.]
SSTIF,Key 
[SSUM | Calculates and prints the sum of element table items.]
SSUM 
[STAT | Displays the status of database settings.]
STAT 
[STEF | Specifies Stefan Boltzmann radiation constant.]
STEF,VALUE 
[STORE | Stores data in the database for the defined variables.]
STORE,Lab,NPTS 
[SUBOPT | Specifies options for subspace iteration eigenvalue extraction.]
SUBOPT,SUBSIZ,NPAD,NPERBK,NUMSSI,NSHIFT,Strmck,JCGITR 
[SUBSET | Reads results for the selected portions of the model.]
SUBSET,Lstep,SBSTEP,FACT,KIMG,TIME,ANGLE,NSET 
[SUMTYPE | Sets the type of summation to be used in the following load case operations.]
SUMTYPE,Label 
[SV | Defines spectrum values to be associated with frequency points.]
SV,DAMP,SV1,SV2,SV3,SV4,SV5,SV6,SV7,SV8,SV9
[SVTYP | Defines the type of single point response spectrum.]
SVTYP,KSV,FACT 
[SXFREQ | Defines the frequency as input variable for the FS Module or the FEMXplorer.]
SXFREQ,Name,MIN,MAX,INC,RedOpt 
[TALLOW | Defines the temperature table for safety factor calculations.]
TALLOW,TEMP1,TEMP2,TEMP3,TEMP4,TEMP5,TEMP6 
[TB | Activates a data table for nonlinear material properties or special element input.]
TB,Lab,MAT,NTEMP,NPTS,TBOPT,EOSOPT 
[TBCOPY | Copies a data table from one material to another (see ).]
TBCOPY,Lab,MATF,MATT 
[TBDATA | Defines data for the data table.]
TBDATA,STLOC,C1,C2,C3,C4,C5,C6 
[TBDELE | Deletes previously defined data tables.]
TBDELE,Lab,MAT1,MAT2,INC 
[TBFT | Performs curve fitting operations on materials.]
TBFT,Oper,ID,Option1,Option2,Option3,Option4,Option5,Option6,Option7
[TBLE |"Specifies""Data table properties""as the subsequent status topic."]
TBLE 
[TBLIST | Lists the data tables.]
TBLIST,Lab,MAT 
[TBMODIF | Modifies data for the data table (GUI).]
TBMODIF,ROW,COL,VALUE 
[TBPLOT | Displays the data table.]
TBPLOT,Lab,MAT,TBOPT,TEMP,SEGN 
[TBPT | Defines a point on a stress strain,B H,or gasket pressure closure curve.]
TBPT,Oper,X,Y 
[TBTEMP | Defines a temperature for the data table.]
TBTEMP,TEMP,KMOD 
[TEE | Defines a tee in a piping run.]
TEE,NCENT,TYPE,ELEM,EINC,L1,L2,L3
[TERM | Specifies various terminal driver options.]
TERM,Kywrd,Opt1,Opt2,Opt3 
[THOPT | Nonlinear transient thermal solution option.]
THOPT,Refopt,REFORMTOL,NTABPOINTS,TEMPMIN,TEMPMAX 
[TCHG | Converts 20 node degenerate tetrahedral elements to their 10 node non degenerate counterparts.]
TCHG,ELEM1,ELEM2,ETYPE2 
[TIFF | Provides TIFF file Export for ANSYS Displays.]
TIFF,Kywrd,OPT 
[TIME | Sets the time for a load step.]
TIME,TIME 
[TIMERANGE | Specifies the time range for which data are to be stored.]
TIMERANGE,TMIN,TMAX 
[TIMINT | Turns on transient effects.]
TIMINT,Key,Lab 
[TIMP | Improves the quality of tetrahedral elements that are not associated with a volume.]
TIMP,ELEM,CHGBND,IMPLEVEL 
[TINTP | Defines transient integration parameters.]
TINTP,GAMMA,ALPHA,DELTA,THETA,OSLM,TOL,--,--,AVSMOOTH 
[TLSPRM | Computes S parameters of a transmission line port.]
TLSPRM,Nr,Ns,Vpath1,Ipath1,Vpath2,Ipath2,Vsymm1,Isymm1,Vsymm2,Isymm2
[TOCOMP | Defines single or multiple compliance as the topological optimization function.]
TOCOMP,Refname,Type,NUMLC,LCARR 
[TODEF | Defines parameters for and initializes topological optimization.]
TODEF,ACCUR 
[TOEXE | Executes one topological optimization iteration.]
TOEXE 
[TOFFST | Specifies the temperature offset from absolute zero to zero.]
TOFFST,VALUE 
[TOFREQ | Defines single or mean frequency formulation as the topological optimization function.]
TOFREQ,Refname,Type,Nfreq,Frqarr,Targval
[TOGRAPH | Plots iteration solution of topological optimization.]
TOGRAPH,Type,Refname 
[TOLIST | Lists all topological optimization functions currently defined.]
TOLIST 
[TOLOOP | Execute several topological optimization iterations.]
TOLOOP,NITER,PLOT 
[TOPLOT | Plot current topological density distribution.]
TOPLOT,AVRG 
[TOPRINT | Print iteration solution history of topological optimization.]
TOPRINT,Type,Refname 
[TORQ2D | Calculates torque on a body in a magnetic field.]
TORQ2D 
[TORQC2D | Calculates torque on a body in a magnetic field based on a circular path.]
TORQC2D,RAD,NUMN,LCSYS 
[TORQSUM | Summarizes electromagnetic torque calculations on element components.]
TORQSUM,Cnam1,Cnam2,Cnam3,Cnam4,Cnam5,Cnam6,Cnam7,Cnam8,Cnam9
[TORUS | Creates a toroidal volume.]
TORUS,RAD1,RAD2,RAD3,THETA1,THETA2 
[TOSTAT | Displays topological optimization status and results information.]
TOSTAT 
[TOTAL | Specifies automatic MDOF generation.]
TOTAL,NTOT,NRMDF 
[TOTYPE | Specifies solution method for topological optimization.]
TOTYPE,Type 
[TOVAR | Specifies the objective and constraints for the topological optimization problem.]
TOVAR,Refname,Type,LOWER,UPPER,Boundtype 
[TRANS | Reformats File.GRPH for improved performance with plotters.]
TRANS,Fname,Ext,-- 
[TRANSFER | Transfers a pattern of nodes to another coordinate system.]
TRANSFER,KCNTO,INC,NODE1,NODE2,NINC 
[TREF | Defines the reference temperature for the thermal strain calculations.]
TREF,TREF 
[TRNOPT | Specifies transient analysis options.]
TRNOPT,Method,MAXMODE,Dmpkey,MINMODE 
[TRPDEL | Deletes particle flow or charged particle trace points.]
TRPDEL,NTRP1,NTRP2,TRPINC 
[TRPLIS | Lists the particle flow or charged particle trace points.]
TRPLIS,NTRP1,NTRP2,TRPINC 
[TRPOIN | Defines a point through which a particle flow or charged particle trace will travel.]
TRPOIN,X,Y,Z,VX,VY,VZ,CHRG,MASS
[TRTIME | Defines the options used for the PLTRAC (particle flow or charged particle trace) command.]
TRTIME,TIME,SPACING,OFFSET,SIZE,LENGTH 
[TSHAP | Defines simple 2 D and 3 D geometric surfaces for target segment elements. ]
TSHAP,Shape 
[TSRES | Defines an array of keytimes at which the time stepping strategy changes. ]
TSRES,Array 
[TUNIF | Assigns a uniform temperature to all nodes. ]
TUNIF,TEMP 
[TVAR | Changes time to the cumulative iteration number. ]
TVAR,KEY 
[TYPE | Sets the element type attribute pointer. ]
TYPE,ITYPE 
[TZAMESH | Meshes the areas of a volume to create Trefftz nodes. ]
TZAMESH,Tvolu,SIZE,NDIV 
[TZDELE | Deletes the Trefftz superelement,associated constraint equations and all supporting Trefftz files. ]
TZDELE 
[TZEGEN | Generates a Trefftz domain substructure and defines a Trefftz superelement for use in electrostatic analysis. ]
TZEGEN 
[UIMP | Defines constant material properties (GUI).]
UIMP,MAT,Lab1,Lab2,Lab3,VAL1,VAL2,VAL3 
[UNDELETE | Removes results sets from the group of sets selected for editing.]
UNDELETE,Option,Nstart,Nend 
[UNDO | Allows the user to modify or save commands issued since the last RESUME or SAVE command.]
UNDO,Kywrd 
[UPCOORD | Modifies the coordinates of the active set of nodes,based on the current displacements.]
UPCOORD,FACTOR,Key 
[UPGEOM | Adds displacements from a previous analysis and updates the geometry of the finite element model to the deformed configuration.]
UPGEOM,FACTOR,LSTEP,SBSTEP,Fname,Ext,-- 
[USRCAL | Allows user solution subroutines to be activated or deactivated.]
USRCAL,Rnam1,Rnam2,Rnam3,Rnam4,Rnam5,Rnam6,Rnam7,Rnam8,Rnam9
[V | Defines a volume through keypoints.]
V,P1,P2,P3,P4,P5,P6,P7,P8 
[V2DOPT | Specifies 2 D/axisymmetric view factor calculation options.]
V2DOPT,GEOM,NDIV,HIDOPT,NZONE 
[VA | Generates a volume bounded by existing areas.]
VA,A1,A2,A3,A4,A5,A6,A7,A8,A9,A10
[VADD | Adds separate volumes to create a single volume.]
VADD,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9 
[VALVE | Defines a valve in a piping run.]
VALVE,NLOC,LENG,MASS,SIF,FLEX,ARINS,ELEM 
[VARDEL | Deletes a variable (GUI).]
VARDEL,NVAR 
[VARNAM | Names (or renames) a variable.]
VARNAM,IR,Name 
[VATT | Associates element attributes with the selected,unmeshed volumes.]
VATT,MAT,REAL,TYPE,ESYS 
[VCLEAR | Deletes nodes and volume elements associated with selected volumes.]
VCLEAR,NV1,NV2,NINC 
[VCROSS | Forms element table items from the cross product of two vectors.]
VCROSS,LabXR,LabYR,LabZR,LabX1,LabY1,LabZ1,LabX2,LabY2,LabZ2 
[VCVFILL | Fills cavities and bosses in volumes (for models imported from CAD files).]
VCVFILL,A1,A2,A3,A4,A5,A6,A7,A9,A9,A10 
[VDDAM | Specifies the velocity spectrum computation constants for the analysis of shock resistance of shipboard structures.]
VDDAM,VF,VA,VB,VC 
[VDELE | Deletes unmeshed volumes.]
VDELE,NV1,NV2,NINC,KSWP 
[VDGL | Lists keypoints of a volume that lie on a parametric degeneracy.]
VDGL,NV1,NV2,NINC 
[VDOT | Forms an element table item from the dot product of two vectors.]
VDOT,LabR,LabX1,LabY1,LabZ1,LabX2,LabY2,LabZ2 
[VDRAG | Generates volumes by dragging an area pattern along a path.]
VDRAG,NA1,NA2,NA3,NA4,NA5,NA6,NLP1,NLP2,NLP3,NLP4,NLP5,NLP6
[VEXT | Generates additional volumes by extruding areas.]
VEXT,NA1,NA2,NINC,DX,DY,DZ,RX,RY,RZ 
[VFCALC | Computes and stores Hemicube view factors.]
VFCALC,Fname,Ext,-- 
[VFOPT | Specifies options for view factor file.]
VFOPT,Opt,Filename,Ext,Dir,Format 
[VFQUERY | Queries and prints element Hemicube view factors and average view factor.]
VFQUERY,SRCELEM,TARELEM 
[VGEN | Generates additional volumes from a pattern of volumes.]
VGEN,ITIME,NV1,NV2,NINC,DX,DY,DZ,KINC,NOELEM,IMOVE
[VGET | Moves a variable into an array parameter vector.]
VGET,Par,IR,TSTRT,KCPLX 
[VGLUE |"Generates new volumes by""gluing""volumes."]
VGLUE,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9 
[VIMP | Improves the quality of the tetrahedral elements in the selected volume(s).]
VIMP,VOL,CHGBND,IMPLEVEL 
[VINP | Finds the pairwise intersection of volumes.]
VINP,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9 
[VINV | Finds the intersection of volumes.]
VINV,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9 
[VLIST | Lists the defined volumes.]
VLIST,NV1,NV2,NINC 
[VLSCALE | Generates a scaled set of volumes from a pattern of volumes.]
VLSCALE,NV1,NV2,NINC,RX,RY,RZ,KINC,NOELEM,IMOVE
[VMESH | Generates nodes and volume elements within volumes.]
VMESH,NV1,NV2,NINC 
[VOFFST | Generates a volume,offset from a given area.]
VOFFST,NAREA,DIST,KINC 
[VOLUMES |"Specifies""Volumes""as the subsequent status topic."]
VOLUMES 
[VOVLAP | Overlaps volumes.]
VOVLAP,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9
[VPLOT | Displays the selected volumes.]
VPLOT,NV1,NV2,NINC,DEGEN,SCALE 
[VPTN | Partitions volumes.]
VPTN,NV1,NV2,NV3,NV4,NV5,NV6,NV7,NV8,NV9
[VPUT | Moves an array parameter vector into a variable.]
VPUT,Par,IR,TSTRT,KCPLX 
[VROTAT | Generates cylindrical volumes by rotating an area pattern about an axis.]
VROTAT,NA1,NA2,NA3,NA4,NA5,NA6,PAX1,PAX2,ARC,NSEG
[VSBA | Subtracts areas from volumes.]
VSBA,NV,NA,SEPO,KEEPV,KEEPA 
[VSBV | Subtracts volumes from volumes.]
VSBV,NV1,NV2,SEPO,KEEP1,KEEP2 
[VSBW | Subtracts intersection of the working plane from volumes (divides volumes).]
VSBW,NV,SEPO,KEEP 
[VSEL | Selects a subset of volumes.]
VSEL,Type,Item,Comp,VMIN,VMAX,VINC,KSWP 
[VSLA | Selects those volumes containing the selected areas.]
VSLA,Type,VLKEY 
[VSUM | Calculates and prints geometry statistics of the selected volumes.]
VSUM,LAB 
[VSWEEP | Fills an existing unmeshed volume with elements by sweeping the mesh from an adjacent area through the volume.]
VSWEEP,VNUM,SRCA,TRGA,LSMO 
[VSYMM | Generates volumes from a volume pattern by symmetry reflection.]
VSYMM,Ncomp,NV1,NV2,NINC,KINC,NOELEM,IMOVE
[VTRAN | Transfers a pattern of volumes to another coordinate system.]
VTRAN,KCNTO,NV1,NV2,NINC,KINC,NOELEM,IMOVE
[VTYPE | Specifies the viewing procedure used to determine the form factors for the Radiation Matrix method.]
VTYPE,NOHID,NZONE 
[WAVES | Initiates reordering.]
WAVES,Wopt,OLDMAX,OLDRMS 
[WERASE | Erases all reordering wave lists.]
WERASE 
[WFRONT | Estimates wavefront statistics.]
WFRONT,KPRNT,KCALC 
[WMID | Specifies reordering options for the WAVES command.]
WMID,Key 
[WMORE | Adds more nodes to the starting wave list.]
WMORE,NODE1,NODE2,NINC,ITIME,INC 
[WPAVE | Moves the working plane origin to the average of specified points.]
WPAVE,X1,Y1,Z1,X2,Y2,Z2,X3,Y3,Z3 
[WPCSYS | Defines the working plane location based on a coordinate system.]
WPCSYS,WN,KCN 
[WPLANE | Defines a working plane to assist in picking operations.]
WPLANE,WN,XORIG,YORIG,ZORIG,XXAX,YXAX,ZXAX,XPLAN,YPLAN,ZPLAN
[WPOFFS | Offsets the working plane.]
WPOFFS,XOFF,YOFF,ZOFF 
[WPROTA | Rotates the working plane.]
WPROTA,THXY,THYZ,THZX 
[WPSTYL | Controls the display and style of the working plane.]
WPSTYL,SNAP,GRSPAC,GRMIN,GRMAX,WPTOL,WPCTYP,GRTYPE,WPVIS,SNAPANG 
[WRITE | Writes the radiation matrix file.]
WRITE,Fname 
[WSORT | Initiates element reordering based upon a geometric sort.]
WSORT,Lab,KORD,--,Wopt,OLDMAX,OLDRMS
[WSPRINGS | Creates weak springs on corner nodes of a bounding box of the currently selected elements.]
WSPRINGS 
[WSTART | Defines a starting wave list.]
WSTART,NODE1,NODE2,NINC,ITIME,INC 
[XVAR | Specifies the X variable to be displayed.]
XVAR,N 
[XVAROPT | Specifies the parameter to be used as the X axis variable.]
XVAROPT,Lab
