Linux Hardware Compatibility HOWTO

FRiC, <frac@pobox.com> v6969, 14 November 1995

This document lists most of the hardware supported by Linux and helps you locate any necessary drivers.

Contents

1 Introduction 4 1.1 Welcome : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 4 1.2 Copyright : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 4 1.3 System architectures : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 4

2 Computers/Motherboards/BIOS 5 2.1 Specific systems : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 5

3 Laptops 5 3.1 Specific laptops : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 6 3.2 PCMCIA : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 6

4 CPU/FPU 7

5 Video cards 7 5.1 Diamond video cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 7 5.2 SVGALIB (graphics for console) : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 8 5.3 XFree86 3.1.2 : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 8 5.3.1 Accelerated : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 8 5.3.2 Unaccelerated : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9 5.3.3 Monochrome : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9 5.3.4 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 5.3.5 Works in progress : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 5.4 Commercial X servers : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 5.4.1 Accelerated-X 1.2 : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 5.4.2 Metro-X 2.3 : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11

6 Controllers (hard drive) 11

7 Controllers (SCSI) 11 7.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 7.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 12 7.3 Unsupported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 13

8 Controllers (I/O) 13

9 Controllers (multiport) 13 9.1 Non-intelligent cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 13 9.1.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 13 9.2 Intelligent cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14 9.2.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14 9.2.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14

10 Network adapters 15 10.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 15 10.1.1 Ethernet : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 15 10.1.2 Pocket and portable adapters : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 16 10.1.3 Slotless : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 16 10.1.4 ARCnet : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 16 10.1.5 Token Ring : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 16 10.1.6 Amateur radio (AX.25) : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 16 10.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 17 10.2.1 Ethernet : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 17 10.2.2 ISDN : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 17 10.2.3 PCMCIA cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 17 10.2.4 ATM : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 17 10.2.5 Frame Relay : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 18 10.3 Unsupported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 18

11 Sound cards 18 11.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 18

11.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 19 11.3 Unsupported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 19

12 Hard drives 19

13 Tape drives 20 13.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 20 13.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 20 13.3 Unsupported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 20

14 CD-ROM drives 21 14.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 21 14.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 21 14.3 Notes : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 21

15 Removable drives 22

16 Mice 22 16.1 Supported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 22 16.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 22 16.3 Notes : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 23

17 Modems 23

18 Printers/Plotters 23 18.1 Ghostscript : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 23 18.1.1 Ghostscript supported printers : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 24 18.1.2 Others : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 24

19 Scanners 25

20 Other hardware 25 20.1 VESA Power Savings Protocol (DPMS) monitors : : : : : : : : : : : : : : : : : : : : : : : : : 25 20.2 Joysticks : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 26 20.3 Video capture boards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 26 20.4 UPS : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 26

1. Introduction 4

20.5 Data acquisition : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 26 20.6 Miscellaneous : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 27

21 Related sources of information 27

22 Acknowledgments 28

23 Appendix A. S3 cards supported by XFree86 3.1.2. 29

24 Appendix B. Supported PCMCIA cards 30 24.1 Ethernet cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 30 24.2 Modem cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 31 24.3 Memory cards : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 31 24.4 SCSI adapters : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 31 24.5 Unsupported : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 31

1 Introduction

1.1 Welcome

Welcome to the Linux Hardware Compatibility HOWTO. This document lists most of the hardware supported by Linux, now if only people would read this first before posting their questions on Usenet. Subsections titled Others list hardware with alpha or beta drivers in varying degrees of usability or other drivers that aren’t included in standard kernels. Note that some drivers only exist in alpha kernels, so if you see something listed as supported but isn’t in your version of the Linux kernel, upgrade. The latest version of this document can be found on the net at the usual sites where the Linux HOWTO’s are kept.

If you know of any Linux hardware (in)compatibilities not listed here please let me know, just send mail or find me on IRC. Thanks.

1.2 Copyright

Standard LDP copyrights apply. If you use this or any other Linux HOWTO’s in a commercial distribution, it would be nice to send the authors a complimentary copy of your product.

1.3 System architectures

This document only deals with Linux for Intel platforms, for other platforms check the following:

2. Computers/Motherboards/BIOS 5

ffl ARM Linux

<http://whirligig.ecs.soton.ac.uk/~rmk92/armlinux.html>

ffl Linux/68k

<http://www-users.informatik.rwth-aachen.de/~hn/linux68k.html>

ffl Linux/8086

<http://www.linux.org.uk/Linux8086.html>

ffl Linux/Alpha

<http://www.azstarnet.com/~axplinux/>

ffl Linux/MIPS

<http://www.waldorf-gmbh.de/linux-mips-faq.html>

ffl Linux/PowerPC

<http://liber.stanford.edu/linuxppc/>

ffl Linux for Acorn

<http://www.ph.kcl.ac.uk/~amb/linux.html>

ffl MacLinux

<http://www.ibg.uu.se/maclinux/>

2 Computers/Motherboards/BIOS

ISA, VLB, EISA, and PCI buses are all supported.

PS/2 and Microchannel (MCA) is not supported in the standard kernel. Alpha test PS/2 MCA kernels are available but not yet recommended for beginners or serious use.

2.1 Specific systems

ffl Compaq Deskpro XL

<http://www-c724.uibk.ac.at/XL/>

ffl IBM PS/2 MCA systems

<ftp://invaders.dcrl.nd.edu/pub/misc/>

3 Laptops

ffl Linux Laptop Homepage

<http://www.cs.utexas.edu/users/kharker/linux-laptop/>

ffl APM

<ftp://ftp.cs.unc.edu/pub/users/faith/linux/>

3. Laptops 6

ffl non-blinking cursor

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/console/noblink-1.5.tar.gz>

ffl power savings (WD7600 chipset)

<ftp://sunsite.unc.edu/pub/Linux/system/Misc/low-level/pwrm-1.0.tar.Z>

ffl other general info

<ftp://tsx-11.mit.edu/pub/linux/packages/laptops/>

3.1 Specific laptops

ffl Compaq Concerto (pen driver)

<http://www.cs.nmsu.edu/~pfeiffer/>

ffl Compaq Contura Aero

<http://domen.uninett.no/~hta/linux/aero-faq.html>

ffl IBM ThinkPad

<http://peipa.essex.ac.uk/tp-linux/tp-linux.html>

ffl Linux and X on notebook computers

<http://www.castle.net/~darin/>

ffl NEC Versa M and P

<http://www.santafe.edu:80/~nelson/versa-linux/>

ffl Tadpole P1000

<http://www.tadpole.com/Support/online/linux.html>

ffl Tadpole P1000 (another one)

<http://peipa.essex.ac.uk/tadpole-linux/tadpole-linux.html>

ffl TI TravelMate 4000M

<ftp://ftp.biomath.jussieu.fr/pub/linux/TM4000M-mini-HOWTO.txt.Z>

ffl TI TravelMate 5100

<http://www.wri.com/~cwikla/ti5100.html>

ffl Toshiba Satellite Pro 400CDT

<http://terra.mpikg-teltow.mpg.de/~burger/T400CDT-Linux.html>

3.2 PCMCIA

ffl PCMCIA

<http://hyper.stanford.edu/~dhinds/pcmcia/>

PCMCIA drivers currently support all common PCMCIA controllers, including Databook TCIC/2, Intel i82365SL, Cirrus PD67xx, and Vadem VG-468 chipsets. Motorola 6AHC05GA controller used in some Hyundai laptops is not supported. And see Appendix B for list of supported PCMCIA cards.

4. CPU/FPU 7

4 CPU/FPU

Intel/AMD/Cyrix 386SX/DX/SL/DXL/SLC, 486SX/DX/SL/SX2/DX2/DX4, Pentium. Basically all 386 or better processors will work. Linux has built-in FPU emulation if you don’t have a math coprocessor.

Experimental SMP (multiple CPU) support is included in kernel 1.3.31 and newer. Check the Linux/SMP Project page for details and updates.

ffl Linux/SMP Project

<http://www.linux.org.uk/SMP/title.html>

A few very early AMD 486DX’s may hang in some special situations. All current chips should be okay and getting a chip swap for old CPU’s should not be a problem.

ULSI Math*Co series has a bug in the FSAVE and FRSTOR instructions that causes problems with all protected mode operating systems. Some older IIT and Cyrix chips may also have this problem.

There are problems with TLB flushing in UMC U5S chips in very old kernels. (1.1.x)

ffl enable cache on Cyrix processors

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/CxPatch030.tar.z>

ffl Cyrix software cache control

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/linux.cxpatch>

5 Video cards

Linux will work with all video cards in text mode, VGA cards not listed below probably will still work with mono VGA and/or standard VGA drivers.

If you’re looking into buying a cheap video card to run X, keep in mind that accelerated cards (ATI Mach, ET4000/W32p, S3) are MUCH faster than unaccelerated or partially accelerated (Cirrus, WD) cards. S3 Trio64 based cards with 2 megs DRAM go for around US$160 and S3 868 based cards with 2 megs DRAM are around US$200.

“32 bpp” is actually 24 bit color aligned on 32 bit boundaries. It does NOT mean the cards are capable of 32 bit color, they still display 24 bit color (16,777,216 colors). 24 bit packed pixels modes are not supported in XFree86, so cards that can do 24 bit modes to get higher resolutions in other OS’s are not able to do this in X using XFree86. These cards include Mach32, Cirrus 542x, S3 801/805/868/968, ET4000, and others.

5.1 Diamond video cards

Most currently available Diamond cards ARE supported by the current release of XFree86. Early Diamond cards may not be officially supported by XFree86, but there are ways of getting them to work. Diamond is now actively supporting the XFree86 Project.

ffl Diamond support for XFree86

<http://www.diamondmm.com/linux.html>

ffl Diamond FAQ (for older cards)

<ftp://sunsite.unc.edu/pub/Linux/X11/Diamond.FAQ>

ffl Diamond Disgruntled Users Page (for older cards)

<http://gladstone.uoregon.edu/~trenton/diamond/>

5.2 SVGALIB (graphics for console)

ffl VGA ffl EGA ffl ARK Logic ARK1000PV/2000PV ffl ATI VGA Wonder ffl ATI Mach32 ffl Cirrus 542x, 543x ffl OAK OTI-037/67/77/87 ffl S3 (limited support) ffl Trident TVGA8900/9000 ffl Tseng ET3000/ET4000/W32

5.3 XFree86 3.1.2

5.3.1 Accelerated ffl ATI Mach8 ffl ATI Mach32 (16 bpp (does not work with all Mach32 cards)) ffl ATI Mach64 (16/32 bpp (support depends on RAMDAC)) ffl Cirrus Logic 5420, 542x/5430 (16 bpp), 5434 (16/32 bpp), 62x5 ffl IBM 8514/A ffl IBM XGA, XGA-II ffl IIT AGX-010/014/015/016 (16 bpp) ffl Oak OTI-087 ffl S3 911, 924, 801, 805, 928, 864, 964, Trio32, Trio64, 868, 968

{ see Appendix A for list of supported S3 cards ffl Tseng ET4000/W32/W32i/W32p ffl Weitek P9000 (16/32 bpp)

{ Diamond Viper VLB/PCI { Orchid P9000 ffl Western Digital WD90C31/33

5.3.2 Unaccelerated ffl ARK Logic ARK1000PV/VL, ARK2000PV ffl ATI VGA Wonder series ffl Avance Logic AL2101/2228/2301/2302/2308/2401 ffl Chips & Technologies 65520/65530/65540/65545 ffl Cirrus Logic 6420/6440 ffl Compaq AVGA ffl Genoa GVGA ffl MCGA (320x200) ffl MX MX68000/MX68010 ffl NCR 77C22, 77C22E, 77C22E+ ffl Oak OTI-067, OTI-077 ffl RealTek RTG3106 ffl Trident TVGA8800, TVGA8900, TVGA9xxx (no support for TGUI chipsets) ffl Tseng ET3000, ET4000AX ffl VGA (standard VGA, 4 bit, slow) ffl Video 7 / Headland Technologies HT216-32 ffl Western Digital/Paradise PVGA1, WD90C00/10/11/24/30/31/33

5.3.3 Monochrome ffl Hercules mono ffl Hyundai HGC-1280 ffl Sigma LaserView PLUS ffl VGA mono

5.3.4 Others

ffl EGA (ancient, from c. 1992)

<ftp://ftp.funet.fi/pub/OS/Linux/BETA/Xega/>

ffl ET4000/W32 and ICS5341 GenDAC

<ftp://sunsite.unc.edu/pub/Linux/X11/X-servers/>

ffl Trident TGUI9440

<ftp://sunsite.unc.edu/pub/Linux/X11/X-servers/>

5.3.5 Works in progress

ffl Compaq QVision ffl Number Nine Imagine 128 No, I do not know when support for these cards will be finished, please don’t ask me. If you want support for these cards now get Accelerated-X.

5.4 Commercial X servers

Commercial X servers provide support for cards not supported by XFree86, and might give better performances for cards that are supported by XFree86. In general they support many more cards than XFree86, so I’ll onlys list cards that aren’t supported by XFree86 here. Contact the vendors directly or check the Commercial HOWTO for more info.

5.4.1 Accelerated-X 1.2

ffl Chips & Technologies 82C45x, 82C48x, F655xx ffl Compaq QVision 2000 ffl Matrox MGA, Millenium ffl Number Nine I-128 / I-128 Pro ffl Weitek P9100 $199, X Inside, Inc. <info@xinside.com> Accel-X supports most cards in 16 and 32 bpp modes and it also supports 24 bit packed pixel modes for cards that have these modes, including ATI Mach32, Mach64 (1280x1024@24bpp), ET4000/W32p, S3- 866/868/968, and more. Accel-X also supports other input hardware like graphics tablets and touchscreens. Accel-X also supports XVideo (Xv) extensions (on Matrox Comet, Marvel-II, and SPEA ShowTime Plus), PEX, and XIE.

6. Controllers (hard drive) 11

5.4.2 Metro-X 2.3 $199, Metro Link <sales@metrolink.com> Metro-X supports more boards than XFree but less than Accel-X, however I don’t have much more information as I can’t seem to view the PostScript files they sent me. Mail them directly for more info.

6 Controllers (hard drive)

Linux will work with standard IDE, MFM and RLL controllers. When using MFM/RLL controllers it is important to use ext2fs and the bad block checking options when formatting the disk. Enhanced IDE (EIDE) interfaces are supported. With up to two IDE interfaces and up to four hard drives and/or CD-ROM drives. Linux will detect these EIDE interfaces.

ffl CMD-640 ffl DTC 2278D ffl FGI/Holtek HT-6560B ffl RZ1000 ffl Triton (82371FB) IDE (with busmaster DMA) ESDI controllers that emulate the ST-506 (MFM/RLL/IDE) interface will also work. The bad block checking comment also applies to these controllers. Generic 8 bit XT controllers also work.

7 Controllers (SCSI)

It is important to pick a SCSI controller carefully. Many cheap ISA SCSI controllers are designed to drive CD-ROM’s rather than anything else. Such low end SCSI controllers are no better than IDE. See the SCSI HOWTO and look at performance figures before buying a SCSI card.

7.1 Supported

ffl AMI Fast Disk VLB/EISA (BusLogic compatible) ffl Adaptec AVA-1505/1515 (ISA) (Adaptec 152x compatible) ffl Adaptec AHA-1510/152x (ISA) (AIC-6260/6360) ffl Adaptec AHA-154x (ISA) (all models) ffl Adaptec AHA-174x (EISA) (in enhanced mode)

7. Controllers (SCSI) 12

ffl Adaptec AHA-274x (EISA) / 284x (VLB) (AIC-7770) ffl Adaptec AHA-2940/3940 (PCI) (AIC-7870) (since 1.3.6) ffl Always IN2000 ffl BusLogic (ISA/EISA/VLB/PCI) (all models) ffl DPT PM2001, PM2012A (EATA-PIO) ffl DPT Smartcache (EATA-DMA) (ISA/EISA/PCI) (all models) ffl DTC 329x (EISA) (Adaptec 154x compatible) ffl Future Domain TMC-16x0, TMC-3260 (PCI) ffl Future Domain TMC-8xx, TMC-950 ffl Media Vision Pro Audio Spectrum 16 SCSI (ISA) ffl NCR 5380 generic cards ffl NCR 53c400 (Trantor T130B) (use generic NCR 5380 SCSI support) ffl NCR 53c406a (Acculogic ISApport / Media Vision Premium 3D SCSI) ffl NCR 53c7x0, 53c8x0 (PCI) ffl Qlogic / Control Concepts SCSI/IDE (FAS408) (ISA/VLB) ffl Seagate ST-01/ST-02 (ISA) ffl SoundBlaster 16 SCSI-2 (Adaptec 152x compatible) (ISA) ffl Trantor T128/T128F/T228 (ISA) ffl UltraStor 14F (ISA), 24F (EISA), 34F (VLB) ffl Western Digital WD7000 SCSI

7.2 Others

ffl AMD AM53C974, AM79C974 (PCI) (Compaq, HP, Zeos onboard SCSI)

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/scsi/AM53C974-0.3.tgz>

ffl Adaptec ACB-40xx SCSI-MFM/RLL bridgeboard

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/scsi/adaptec-40XX.tar.gz>

ffl Always Technologies AL-500

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/scsi/al500-0.2.tar.gz>

ffl BusLogic (ISA/EISA/VLB/PCI) (new beta driver)

<ftp://ftp.dandelion.com/BusLogic-1.0-beta.tar.gz>

8. Controllers (I/O) 13

ffl Iomega PC2/2B

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/scsi/iomega pc2-1.1.x.tar.gz>

ffl Qlogic (ISP1020) (PCI)

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/scsi/isp1020-0.5.gz>

ffl Ricoh GSI-8

<ftp://tsx-11.mit.edu/pub/linux/ALPHA/scsi/gsi8.tar.gz>

7.3 Unsupported

ffl Parallel port SCSI adapters

ffl Non Adaptec compatible DTC boards (327x, 328x)

8 Controllers (I/O)

Any standard serial/parallel/joystick/combo cards. Linux supports 8250, 16450, 16550, and 16550A UART’s. Cards that support non-standard IRQ’s (IRQ > 9) can be used.

See National Semiconductor’s “Application Note AN-493” by Martin S. Michael. Section 5.0 describes in detail the differences between the NS16550 and NS16550A. Briefly, the NS16550 had bugs in the FIFO circuits, but the NS16550A (and later) chips fixed those. However, there were very few NS16550’s produced by National, long ago, so these should be very rare. And many of the “16550” parts in actual modern boards are from the many manufacturers of compatible parts, which may not use the National “A” suffix. Also, some multiport boards will use 16552 or 16554 or various other multiport or multifunction chips from National or other suppliers (generally in a dense package soldered to the board, not a 40 pin DIP). Mostly, don’t worry about it unless you encounter a very old 40 pin DIP National “NS16550” (no A) chip loose or in an old board, in which case treat it as a 16450 (no FIFO) rather than a 16550A. - Zhahai Stewart <zstewart@hisys.com>

9 Controllers (multiport)

9.1 Non-intelligent cards

9.1.1 Supported

ffl AST FourPort and clones (4 port)

ffl Accent Async-4 (4 port)

ffl Arnet Multiport-8 (8 port)

ffl Bell Technologies HUB6 (6 port)

ffl Boca BB-1004, 1008 (4, 8 port) - no DTR, DSR, and CD

9. Controllers (multiport) 14

ffl Boca BB-2016 (16 port) ffl Boca IO/AT66 (6 port) ffl Boca IO 2by4 (4 serial / 2 parallel, uses 5 IRQ’s) ffl Computone ValuePort (4, 6, 8 port) (AST FourPort compatible) ffl DigiBoard PC/X (4, 8, 16 port) ffl Comtrol Hostess 550 (4, 8 port) ffl PC-COMM 4-port (4 port) ffl SIIG I/O Expander 4S (4 port, uses 4 IRQ’s) ffl STB 4-COM (4 port) ffl Twincom ACI/550 ffl Usenet Serial Board II (4 port) Non-intelligent cards usually come in two varieties, one using standard com port addresses and use 4 IRQ’s, and another that’s AST FourPort compatible and uses a selectable block of addresses and a single IRQ. (Addresses and IRQ’s are set using setserial.) If you’re getting one of these cards, be sure to check which standard it conforms to, prices are no indication.

9.2 Intelligent cards

9.2.1 Supported

ffl Cyclades Cyclom-8Y/16Y (8, 16 port) (ISA/PCI) ffl Stallion EasyIO (ISA) / EasyConnection 8/32 (ISA/MCA) ffl Stallion EasyConnection 8/64 / ONboard (ISA/EISA/MCA) / Brumby / Stallion (ISA)

9.2.2 Others

ffl Comtrol RocketPort (8/16/32 port)

<ftp://tsx-11.mit.edu/pub/linux/packages/comtrol/>

ffl Computone IntelliPort II (4/8/16 port)

contact Michael H. Warfield <mhw@wittsend.atl.ga.us> ffl DigiBoard COM/Xi

contact Simon Park <si@wimpol.demon.co.uk> ffl DigiBoard PC/Xe (ISA) and PC/Xi (EISA)

<ftp://ftp.digibd.com/drivers/linux/> ffl Hayes ESP8

contact Dennis Boylan <dennis@lan.com> ffl Moxa C218 (8 port) / C320 (8/16/24/32 expandable)

<ftp://ftp.moxa.com.tw/drivers/c-218-320/linux/>

ffl Specialix SIO/XIO (modular, 4 to 32 ports)

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/serial/sidrv0 5.taz>

10 Network adapters

Ethernet adapters vary greatly in performance. In general the newer the design the better. Some very old cards like the 3Com 3C501 are only useful because they can be found in junk heaps for $5 a time. Be careful with clones, not all are good clones and bad clones often cause erratic lockups under Linux. Read the Ethernet HOWTO for detailed descriptions of various cards.

10.1 Supported

10.1.1 Ethernet

ffl 3Com 3C501 - “avoid like the plague” ffl 3Com 3C503, 3C505, 3C507, 3C509/3C509B (ISA) / 3C579 (EISA) ffl AMD LANCE (79C960) / PCnet-ISA/PCI (AT1500, HP J2405A, NE1500/NE2100) ffl AT&T GIS WaveLAN ffl Allied Telesis AT1700 ffl Ansel Communications AC3200 EISA ffl Apricot Xen-II ffl Cabletron E21xx ffl DEC DE425 (EISA) / DE434/DE435 (PCI) ffl DEC DEPCA and EtherWORKS ffl HP PCLAN (27245 and 27xxx series) ffl HP PCLAN PLUS (27247B and 27252A) ffl HP 10/100VG PCLAN (ISA/EISA/PCI) ffl Intel EtherExpress ffl Intel EtherExpress Pro ffl NE2000/NE1000 (be careful with clones) ffl New Media Ethernet ffl Racal-Interlan NI5210 (i82586 Ethernet chip) ffl Racal-Interlan NI6510 (am7990 lance chip) - doesn’t work with more than 16 megs RAM ffl PureData PDUC8028, PDI8023 ffl SEEQ 8005 ffl SMC Ultra ffl Schneider & Koch G16 ffl Western Digital WD80x3 ffl Zenith Z-Note / IBM ThinkPad 300 built-in adapter

10.1.2 Pocket and portable adapters ffl AT-Lan-Tec/RealTek parallel port adapter ffl D-Link DE600/DE620 parallel port adapter

10.1.3 Slotless

ffl SLIP/CSLIP/PPP (serial port) ffl EQL (serial IP load balancing) ffl PLIP (parallel port) - using “LapLink cable” or bi-directional cable

10.1.4 ARCnet

ffl works with all ARCnet cards

10.1.5 Token Ring

ffl IBM Tropic chipset cards

10.1.6 Amateur radio (AX.25) ffl Ottawa PI/PI2 ffl Most generic 8530 based HDLC boards

10.2 Others

10.2.1 Ethernet

ffl 3Com Demon Ethercards (3C592, 3C597 (100 mbps)) (EISA)

<http://cesdis.gsfc.nasa.gov/linux/drivers/vortex.html>

ffl 3Com Vortex Ethercards (3C590, 3C595 (100 mbps)) (PCI)

<http://cesdis.gsfc.nasa.gov/linux/drivers/vortex.html>

ffl DEC 21040/21140 “Tulip” / SMC PCI EtherPower 10/100

<http://cesdis.gsfc.nasa.gov/linux/drivers/tulip.html>

ffl HP J2585 (PCI) / HP J2573 (ISA) (ATT2MDx1 / 100VG)

<http://cesdis1.gsfc.nasa.gov:80/linux/drivers/100vg.html>

10.2.2 ISDN

ffl Linux ISDN WWW page

<http://www.ix.de/ix/linux/linux-isdn.html>

ffl 3Com Sonix Arpeggio

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/network/sonix.tgz>

ffl Combinet EVERYWARE 1000 ISDN

<ftp://sunsite.unc.edu/pub/Linux/patches/network/combinet1000isdn-1.02.tar.gz>

ffl Diehl SCOM card

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/network/isdndrv-0.1.1.tar.gz>

ffl ICN ISDN / Teles ISDN / Creatix AVM ISDN cards

<ftp://ftp.franken.de/pub/isdn4linux/>

ISDN cards that emulate standard modems or common Ethernet adapters don’t need any special drivers to work.

10.2.3 PCMCIA cards

ffl See Appendix B for complete list

10.2.4 ATM

ffl Efficient Networks ENI155P-MF 155 Mbps ATM adapter (PCI)

<http://lrcwww.epfl.ch/linux-atm/>

11. Sound cards 18

10.2.5 Frame Relay

ffl Sangoma S502 56K Frame Relay card

<ftp://ftp.sovereign.org/pub/wan/fr/>

10.3 Unsupported

ffl Xircom adapters (PCMCIA and parallel port) are not supported.

11 Sound cards

11.1 Supported

ffl 6850 UART MIDI ffl Adlib (OPL2) ffl Audio Excell DSP16 ffl Aztech Sound Galaxy NX Pro ffl Crystal CS4232 (PnP) based cards ffl ECHO-PSS cards (Orchid SoundWave32, Cardinal DSP16) ffl Ensoniq SoundScape ffl Gravis Ultrasound ffl Gravis Ultrasound 16-bit sampling daughterboard ffl Gravis Ultrasound MAX ffl Logitech SoundMan Games (SBPro, 44kHz stereo support) ffl Logitech SoundMan Wave (Jazz16/OPL4) ffl Logitech SoundMan 16 (PAS-16 compatible) ffl MPU-401 MIDI ffl MediaTriX AudioTriX Pro ffl Media Vision Premium 3D (Jazz16) ffl Media Vision Pro Sonic 16 (Jazz) ffl Media Vision Pro Audio Spectrum 16 ffl Microsoft Sound System (AD1848)

12. Hard drives 19

ffl OAK OTI-601D cards (Mozart) ffl OPTi 82C928/82C929 cards (MAD16/MAD16 Pro) ffl Sound Blaster ffl Sound Blaster Pro ffl Sound Blaster 16 ffl Turtle Beach Wavefront cards (Maui, Tropez) ffl Wave Blaster (and other daughterboards)

11.2 Others

ffl MPU-401 MIDI (intelligent mode)

<ftp://sunsite.unc.edu/pub/Linux/kernel/sound/mpu401-0.2.tar.gz>

ffl PC speaker / Parallel port DAC

<ftp://ftp.informatik.hu-berlin.de/pub/os/linux/hu-sound/>

ffl Turtle Beach MultiSound/Tahiti/Monterey

<ftp://ftp.cs.colorado.edu/users/mccreary/archive/tbeach/multisound/>

11.3 Unsupported

The ASP chip on Sound Blaster 16 series and AWE32 is not supported. AWE32’s onboard E-mu MIDI synthesizer is not supported.

Nathan Laredo <laredo@gnu.ai.mit.edu> is willing to write AWE32 drivers if you send him a complimentary card. He is also willing to write drivers for almost any hardware if you send him free samples of your hardware.

Sound Blaster 16’s with DSP 4.11 and 4.12 have a hardware bug that causes hung/stuck notes when playing MIDI and digital audio at the same time. The problem can happen with either Wave Blaster daughterboards or MIDI devices attached to the MIDI port. There is no known fix.

12 Hard drives

All hard drives should work if the controller is supported.

(From the SCSI HOWTO) All direct access SCSI devices with a block size of 256, 512, or 1024 bytes should work. Other block sizes will not work (Note that this can often be fixed by changing the block and/or sector sizes using the MODE SELECT SCSI command).

Large IDE (EIDE) drives work fine with newer kernels. The boot partition must lie in the first 1024 cylinders due to PC BIOS limitations.

13. Tape drives 20

Some Conner CFP1060S drives may have problems with Linux and ext2fs. The symptoms are inode errors during e2fsck and corrupt file systems. Conner has released a firmware upgrade to fix this problem, contact Conner at 1-800-4CONNER (US) or +44-1294-315333 (Europe). Have the microcode version (found on the drive label, 9WA1.6x) handy when you call.

Certain Micropolis drives have problems with Adaptec and BusLogic cards, contact the drive manufacturers for firmware upgrades if you suspect problems.

ffl Multiple device driver (RAID-0, RAID-1)

<ftp://sweet-smoke.ufr-info-p7.ibp.fr/public/Linux/>

13 Tape drives

13.1 Supported

ffl SCSI tape drives

(From the SCSI HOWTO) Drives using both fixed and variable length blocks smaller than the driver buffer length (set to 32k in the distribution sources) are supported. Virtually all drives should work. (Send mail if you know of any incompatible drives.)

ffl QIC-02 drives

13.2 Others

ffl QIC-117, QIC-40/80, QIC-3010/3020 (QIC-WIDE) drives

Most tape drives using the floppy controller should work. Various dedicated controllers (Colorado FC-10/FC-20, Mountain Mach-2, Iomega Tape Controller II) are also supported

<ftp://sunsite.unc.edu/pub/Linux/kernel/tapes>

13.3 Unsupported

ffl Emerald and Tecmar QIC-02 tape controller cards - Chris Ulrich <insom@math.ucr.edu>

ffl Drives that connect to the parallel port (eg: Colorado Trakker)

ffl Some high speed tape controllers (Colorado TC-15)

ffl Irwin AX250L/Accutrak 250 (not QIC-80)

ffl IBM Internal Tape Backup Unit (not QIC-80)

ffl COREtape Light

14. CD-ROM drives 21

14 CD-ROM drives

14.1 Supported

ffl SCSI CD-ROM drives

(From the CD-ROM HOWTO) Any SCSI CD-ROM drive with a block size of 512 or 2048 bytes should work under Linux; this includes the vast majority of CD-ROM drives on the market.

ffl EIDE (ATAPI) CD-ROM drives ffl Aztech CDA268, Orchid CDS-3110, Okano/Wearnes CDD-110, Conrad TXC ffl GoldStar R420 ffl LMS Philips CM 206 ffl Matsushita/Panasonic, Creative Labs, Longshine, Kotobuki (SBPCD) ffl Mitsumi ffl Optics Storage Dolphin 8000AT ffl Sanyo H94A ffl Sony CDU31A/CDU33A ffl Sony CDU-535/CDU-531 ffl Teac CD-55A SuperQuad

14.2 Others

ffl LMS/Philips CM 205/225/202

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/cdrom/lmscd0.3d.tar.gz>

ffl Mitsumi FX001D/F (alternate drivers)

<ftp://ftp.gwdg.de//pub/linux/cdrom/drivers/mitsumi/mcdx-1.0a.tar.gz>

ffl NEC CDR-35D (old)

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/cdrom/linux-neccdr35d.patch>

ffl Sony SCSI multisession CD-XA

<ftp://tsx-11.mit.edu/pub/linux/patches/sony-multi-0.00.tar.gz>

14.3 Notes

PhotoCD (XA) is supported.

All CD-ROM drives should work similarly for reading data. There are various compatibility problems with audio CD playing utilities. (Especially with newer low-end NEC drives.) Some alpha drivers may not have audio support yet.

Early (single speed) NEC CD-ROM drives may have trouble with currently available SCSI controllers.

15. Removable drives 22

15 Removable drives

All SCSI drives should work if the controller is supported, including optical (MO), WORM, floptical, Bernoulli, Zip, SyQuest, PD, and others.

ffl Parallel port Zip drives

<ftp://gear.torque.net/pub/>

Removable drives work like floppies, just fdisk/mkfs and mount the disks. Linux provides drive locking if your drives support it. mtools can also be used if the disks are in MS-DOS format. CD-R drives require special software to work. Read the CD-R Mini-HOWTO. Linux supports both 512 and 1024 bytes/sector disks.

16 Mice

16.1 Supported

ffl Microsoft serial mouse ffl Mouse Systems serial mouse ffl Logitech Mouseman serial mouse ffl Logitech serial mouse ffl ATI XL Inport busmouse ffl C&T 82C710 (QuickPort) (Toshiba, TI Travelmate) ffl Microsoft busmouse ffl Logitech busmouse ffl PS/2 (auxiliary device) mouse

16.2 Others

ffl Sejin J-mouse

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/console/jmouse.1.1.70-jmouse.tar.gz>

ffl MultiMouse - use multiple mouse devices as single mouse

<ftp://sunsite.unc.edu/pub/Linux/system/Misc/MultiMouse-1.0.tgz>

17. Modems 23

16.3 Notes

Touchpad devices like Alps Glidepoint also work, so long they’re compatible with another mouse protocol. Newer Logitech mice (except the Mouseman) use the Microsoft protocol and all three buttons do work. Eventhough Microsoft’s mice have only two buttons, the protocol allows three buttons. The mouse port on the ATI Graphics Ultra and Ultra Pro use the Logitech busmouse protocol. (See the Busmouse HOWTO for details.)

17 Modems

All internal modems or external modems connected to the serial port.

A small number of modems come with DOS software that downloads the control program at runtime. These can normally be used by loading the program under DOS and doing a warm boot. Such modems are probably best avoided as you won’t be able to use them with non PC hardware in the future. All PCMCIA modems should work with the PCMCIA drivers. Fax modems need appropriated fax software to operate.

ffl Digicom Connection 96+/14.4+ - DSP code downloading program

<ftp://sunsite.unc.edu/pub/Linux/system/Serial/smdl-linux.1.02.tar.gz>

ffl ZyXEL U-1496 series - ZyXEL 1.4, modem/fax/voice control program

<ftp://sunsite.unc.edu/pub/Linux/system/Serial/ZyXEL-1.4.tar.gz>

18 Printers/Plotters

All printers and plotters connected to the parallel or serial port should work.

ffl HP LaserJet 4 series - free-lj4, printing modes control program

<ftp://sunsite.unc.edu/pub/Linux/system/Printing/free-lj4-1.1p1.tar.gz>

ffl BiTronics parallel port interface

<ftp://sunsite.unc.edu/pub/Linux/kernel/misc/bt-ALPHA-0.0.1.tar.gz>

18.1 Ghostscript

Many Linux programs output PostScript files. Non-PostScript printers can emulate PostScript Level 2 using Ghostscript.

ffl Ghostscript

<ftp://ftp.cs.wisc.edu/pub/ghost/aladdin/>

18. Printers/Plotters 24

18.1.1 Ghostscript supported printers

ffl Apple Imagewriter ffl C. Itoh M8510 ffl Canon BubbleJet BJ10e, BJ200 ffl Canon LBP-8II, LIPS III ffl DEC LA50/70/75/75plus ffl DEC LN03, LJ250 ffl Epson 9 pin, 24 pin, LQ series, Stylus, AP3250 ffl HP 2563B ffl HP DesignJet 650C ffl HP DeskJet/Plus/500 ffl HP DeskJet 500C/520C/550C/1200C color ffl HP LaserJet/Plus/II/III/4 ffl HP PaintJet/XL/XL300 color ffl IBM Jetprinter color ffl IBM Proprinter ffl Imagen ImPress ffl Mitsubishi CP50 color ffl NEC P6/P6+/P60 ffl Okidata MicroLine 182 ffl Ricoh 4081 ffl SPARCprinter ffl StarJet 48 inkjet printer ffl Tektronix 4693d color 2/4/8 bit ffl Tektronix 4695/4696 inkjet plotter ffl Xerox XES printers (2700, 3700, 4045, etc.)

18.1.2 Others

ffl Canon BJC600 and Epson ESC/P color printers

<ftp://petole.imag.fr/pub/postscript/>

19. Scanners 25

19 Scanners

ffl A4 Tech AC 4096

<ftp://ftp.informatik.hu-berlin.de/pub/local/linux/ac4096.tgz>

ffl Epson GT6000

<ftp://sunsite.unc.edu/pub/Linux/apps/graphics/scanners/ppic0.5.tar.gz>

ffl Fujitsu SCSI-2 scanners

contact Dr. G.W. Wettstein <greg%wind.UUCP@plains.nodak.edu>

ffl Genius GS-B105G

<ftp://tsx-11.mit.edu/pub/linux/ALPHA/scanner/gs105-0.0.1.tar.gz>

ffl Genius GeniScan GS4500 handheld scanner

<ftp://tsx-11.mit.edu/pub/linux/ALPHA/scanner/gs4500-1.3.tar.gz>

ffl HP ScanJet, ScanJet Plus

<ftp://ftp.ctrl-c.liu.se/unix/linux/wingel/>

ffl HP ScanJet II series SCSI

<ftp://sunsite.unc.edu/pub/Linux/apps/graphics/scanners/hpscanpbm-0.3a.tar.gz>

ffl HP ScanJet family (including ScanJet 3c)

<http://www.tummy.com/xvscan/>

ffl Logitech Scanman 32 / 256

<ftp://tsx-11.mit.edu/pub/linux/ALPHA/scanner/logiscan-0.0.2.tar.gz>

ffl Mustek M105 handheld scanner with GI1904 interface

<ftp://tsx-11.mit.edu/pub/linux/ALPHA/scanner/scan-driver-0.1.8.tar.gz>

ffl Mustek Paragon 6000CX

<ftp://sunsite.unc.edu/pub/Linux/apps/graphics/scanners/muscan-1.1.5.taz>

ffl Nikon Coolscan SCSI 35mm film scanner

<ftp://sunsite.unc.edu/pub/Linux/apps/graphics/scanners/>

ffl UMAX SCSI scanners

contact Craig Johnston <mkshenk@u.washington.edu>

20 Other hardware

20.1 VESA Power Savings Protocol (DPMS) monitors

Support for power savings is included in the Linux kernel. Just use setterm to enable support.

20. Other hardware 26

20.2 Joysticks

ffl Joystick driver

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/console/joystick-0.7.3.tgz>

ffl Joystick driver (module)

<ftp://sunsite.unc.edu/pub/Linux/kernel/patches/console/joyfixed.tgz>

20.3 Video capture boards

ffl FAST Screen Machine II

<ftp://sunsite.unc.edu/pub/Linux/apps/video/ScreenMachineII.1.2.tgz>

ffl ImageNation Cortex I

<ftp://sunsite.unc.edu/pub/Linux/apps/video/cortex.drv.0.1.tgz>

ffl ImageNation CX100

<ftp://sunsite.unc.edu/pub/Linux/apps/video/cxdrv-0.1beta.tar.gz>

ffl Pro Movie Studio

<ftp://sunsite.unc.edu/pub/Linux/apps/video/PMS-grabber.2.0.tgz>

ffl Quanta WinVision video capture card

<ftp://sunsite.unc.edu/pub/Linux/apps/video/fgrabber-1.0.tgz>

ffl Video Blaster, Rombo Media Pro+

<ftp://sunsite.unc.edu/pub/Linux/apps/video/vid src.gz>

ffl VT1500 TV cards

<ftp://sunsite.unc.edu/pub/Linux/apps/video/vt1500-1.0.5.tar.gz>

20.4 UPS

ffl APC SmartUPS

<ftp://sunsite.unc.edu/pub/Linux/system/UPS/apcd-0.1.tar.gz>

ffl UPS’s with RS-232 monitoring port (unipower package)

<ftp://sunsite.unc.edu/pub/Linux/system/UPS/unipower-1.0.0.tgz>

ffl various other UPS’s are supported, read the UPS HOWTO

20.5 Data acquisition

The Linux Lab Project site collects drivers for hardware dealing with data acquisition, they also maintain some mailing lists dealing with the subject. I have no experience with data acquisition so please check the site for more details.

21. Related sources of information 27

ffl Linux Lab Project

<ftp://koala.chemie.fu-berlin.de/pub/linux/LINUX-LAB/>

ffl CED 1401 ffl DBCC CAMAC ffl IEEE-488 (GPIB, HPIB) boards ffl Keithley DAS-1200 ffl National Instruments AT-MIO-16F / Lab-PC+ ffl Analog Devices RTI-800/815 ADC/DAC board contact Paul Gortmaker <gpg109@anu.edu.au>

20.6 Miscellaneous

ffl Maralu chip-card reader/writer

<ftp://ftp.thp.uni-koeln.de/pub/linux/chip/>

ffl Mattel Powerglove

<ftp://sunsite.unc.edu/pub/Linux/apps/linux-powerglove.tgz>

ffl AIMS Labs RadioTrack FM radio card

<ftp://sunsite.unc.edu/pub/Linux/apps/sound/radiotrack-1.1.tgz>

ffl Reveal FM Radio card

<ftp://magoo.uwsuper.edu/pub/fm-radio/>

ffl Videotext cards

<ftp://sunsite.unc.edu/pub/Linux/apps/video/videoteXt-0.5.tar.gz>

21 Related sources of information

ffl Cameron Spitzer’s hardware FAQ archive

<ftp://rahul.net/pub/cameron/PC-info/>

ffl Computer Hardware and Software Vendor Phone Numbers

<http://mtmis1.mis.semi.harris.com/comp ph1.html>

ffl Guide to Computer Vendors

<http://www.ronin.com/SBA/>

ffl System Optimization Information

<http://www.dfw.net/~sdw/>

22. Acknowledgments 28

22 Acknowledgments

Thanks to all the authors and contributors of other HOWTO’s, many things here are shamelessly stolen from their works; to Zane Healy and Ed Carp, the original authors of this list; and to everyone else who sent in updates and feedbacks. Special thanks to Eric Boerner and lilo (the person, not the program) for the sanity checks. And thanks to Dan Quinlan for the original SGML conversion.

23. Appendix A. S3 cards supported by XFree86 3.1.2. 29

23 Appendix A. S3 cards supported by XFree86 3.1.2.

CHIPSET RAMDAC CLOCKCHIP BPP CARD

801/805 AT&T 20C490 16 Actix GE 32 Orchid Fahrenheit 1280+ 801/805 AT&T 20C490 ICD2061A 16 STB PowerGraph X.24 805 S3 GENDAC 16 Miro 10SD VLB/PCI SPEA Mirage VLB 805 SS2410 ICD2061A 8 Diamond Stealth 24 VLB 801/805 AT&T 20C490 Ch8391 16 JAX 8231, SPEA Mirage 928 AT&T 20C490 16 Actix Ultra 928 Sierra SC15025 ICD2061A 32 ELSA Winner 1000 ISA/VLB/EISA 928 Bt485 ICD2061A 32 STB Pegasus VL 928 Bt485 SC11412 16 SPEA Mercury VLB 928 Bt485 ICD2061A 32 #9 GXE Level 10/11/12 928 Ti3020 ICD2061A 32 #9 GXE Level 14/16 864 AT&T 20C498 ICS2494 32 Miro 20SD (BIOS 1.x) 864 AT&T 20C498/ ICD2061A/ 32 ELSA Winner 1000 PRO VLB/PCI STG1700 ICS9161 MIRO 20SD (BIOS 2.x) 864 STG1700 ICD2061A 32 Actix GE 64 VLB 864 AT&T 20C498/ ICS2595 16 SPEA Mirage P64 DRAM (BIOS 3.x) AT&T 21C498 864 S3 86C716 SDAC 32 ELSA Winner 1000 PRO Miro 20SD (BIOS 3.x) SPEA Mirage P64 DRAM (BIOS 4.x) Diamond Stealth 64 DRAM 864 ICS5342 ICS5342 32 Diamond Stealth 64 DRAM (some) 864 AT&T 20C498-13 ICD2061A 32 #9 GXE64 PCI 964 AT&T 20C505 ICD2061A 32 Miro Crystal 20SV PCI 964 Bt485 ICD2061A 32 Diamond Stealth 64 964 Bt9485 ICS9161A 32 SPEA Mercury 64 964 Ti3020 ICD2061A 8 ELSA Winner 2000 PRO PCI 964 Ti3025 Ti3025 32 #9 GXE64 Pro VLB/PCI Miro Crystal 40SV 964 IBM RGB 32 Hercules Terminator 64 868 S3 86C716 SDAC 32 ELSA Winner 1000AVI 968 TVP3026 32 ELSA Winner 2000PRO/X Diamond Stealth 64 Video VRAM 968 IBM RGB 32 Genoa VideoBlitz III AVI Hercules Terminator Pro 64 STB Velocity 64V #9 FX Motion 771 732 (Trio32) 32 Diamond Stealth 64 DRAM SE (all Trio32 based cards) 764 (Trio64) 32 SPEA Mirage P64 (BIOS 5.x) Diamond Stealth 64 DRAM #9 FX Vision 330 STB PowerGraph 64 (all Trio64 based cards)

24 Appendix B. Supported PCMCIA cards

These cards are supported by David Hinds’ PCMCIA package and this list is taken from his web page.

24.1 Ethernet cards

ffl 3Com 3c589, 3c589B ffl Accton EN2212 EtherCard ffl CNet CN30BC Ethernet ffl D-Link DE-650 ffl EFA InfoExpress SPT EFA 205 10baseT ffl EP-210 Ethernet ffl Farallon Etherwave ffl GVC NIC-2000P Ethernet Combo ffl HYPERTEC HyperEnet ffl IBM CreditCard Ethernet Adapter ffl IC-Card Ethernet ffl Katron PE-520 Ethernet ffl Kingston KNE-PCM/M ffl LANEED Ethernet ffl Linksys EtherCard ffl Maxtech PCN2000 Ethernet ffl Network General “Sniffer” ffl New Media Ethernet ffl Novell/National NE4100 InfoMover ffl Proteon Ethernet ffl PreMax PE-200 Ethernet ffl RPTI EP400 Ethernet ffl Socket Communications Socket EA LAN Adapter ffl Thomas-Conrad Ethernet ffl Volktek Ethernet

24.2 Modem cards

ffl All modem cards should work

24.3 Memory cards

ffl New Media SRAM ffl Epson 2MB SRAM ffl Intel Series 2 and Series 2+ Flash

24.4 SCSI adapters

ffl Qlogic FastSCSI PCMCIA ffl New Media Bus Toaster SCSI ffl Adaptec APA-1460 SlimSCSI

24.5 Unsupported

ffl Xircom ethernet and ethernet/modem cards ffl Canon/Compaq PCMCIA floppy drive