The work required after drilling a successful well to make the well ready for production.