A method of preparing a well for production in which no production casing or liner is set opposite the producing formation, so reservoir fluids can flow unrestricted into the open wellbore.