To place a cement plug or mechanical plug in a well as a means of isolating oil bearing zones from non-oil bearing zones below the plug.