InS_StArT
MADGEODI.COM
1.0,ROUTE.COM,MDGDOS02.BIN
^Madge Smart 16/4 PC Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 AT Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 MC Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 MC32 Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 EISA Ringnode,MADGEODI.COM,0E0
^Madge Smart 16/4 EISA Mk II Ringnode,MADGEODI.COM,0E0
?This board can be used with source routing. If your network is using source routing, load the ROUTE.COM file after the MADGEODI.COM file
!OIE0(PORT) Base I/O Port
A20
1A20
2A20
3A20
!O00M(SLOT) Slot location
1
2
3
4
5
6
7
8
!OIEM(FRAME) Frame Type
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIEM(NODE ADDRESS) Node Address
0
7FFFFFFFFFFF
!OIEM(MAX FRAME SIZE) Maximum frame size
?Select the maximum packet size for your network. The packet sizes include protocol headers and represent 1/2K, 1K, 2K and 4K frames, respectively.  Default: 4K.
626
1138
2162
4210
$OIEM(TRANSMIT BUFFER SIZE) Transmit Buffer Size
?Select a transmit buffer size greater than the maximum packet size. A value of twice the packet size is recommended. Default: 8500.
630
30000
$OIEM(RECEIVE BUFFER SIZE) Receive Buffer Size
?Select a transmit buffer size greater than the maximum packet size. A value of twice the packet size is recommended. Default: 8500.
630
30000
InS_EnD
