A,I,128,Ascii (Non-Binary)
C,I,128,Xmodem-CRC (CRC)
F,I,1024,1K-Xmodem-G (Full flow)
G,S,1024,Ymodem-G (DOOR {doornum} only)
K,S,90,Kermit (DOOR {doornum} only)
O,I,1024,1K-Xmodem (Old Ymodem)
W,S,128,WXmodem (DOOR {doornum} only)
X,I,128,Xmodem (Checksum)
Y,S,1024,Ymodem Batch (DOOR {doornum} only)
Z,S,1024,Zmodem (DOOR {doornum} only)
N,I,0,None
