NEXTSTEP for Intel Processors
Tested Compatible System

Title:	Deskpro 5120 
Last Updated:		October 11 1995
Effective Date:	October 10th 1995
Tested With:		3.3

Product Vendor:

Explanation of Compatibility Testing 
NEXTSTEP Compatible systems are tested by third parties using a test procedure developed by NeXT.  NeXT approves the use of the "NEXTSTEP Compatible" designation for these systems based on the completeness of the test results submitted by these NeXT-trained 3rd parties.
 
For more detailed information on the NICE program, please refer to NeXTanswers document 1903_Compatible_Systems_Tested_With_NEXTSTEP.rtf

Note: NeXT accepts no support responsibilities or liability whatsoever for any system authorized to use the "NEXTSTEP Compatible" designation, nor does NeXT represent that their test procedures or training--even if followed exactly by the 3rd party performing the test work--are in any way complete or exhaustive. Known or unknown errors may be present in configurations which are designated as "NEXTSTEP Compatible" which could adversely affect the operation of these systems.  Support for compatible systems may be provided by the PC vendor or System integrator.  

Tested Components:
Compaq reports testing a system configuration consisting of the following components:
System CPU Board(s)
	CPU:		Intel Pentium, 120 MHz
	RAM:		32MB maximum tested
	ISA slots:		2 and 2 Combo with PCI
	PCI slots:		2 in Combo with ISA
	BIOS name:	Compaq
	Jumper/Switch Settings:
	 All jumpers in factory default position.	

IDE Controller(s)
	on-board

SCSI Controller(s)
	Manufacturer:	Compaq
	Model name:	Compaq 6260
	Revision:		A
	BIOS Rev. #:	Unknown
	Interface Type:	ISA
	Jumper/Switch Settings:
	SW1 - OFF	ROM Disable
	SW2 - OFF	   "	"
	SW3 - ON	Addr  0x140
	SW4 - ON	INT 10
	SW5 - ON	  "     "
	SW6 - OFF	Disconnect Enabled
	SW7 - OFF	Sync Enabled
	SW8 - OFF	Parity Enabled

CD-ROM Drive(s)
	Manufacturer:	Sony
	Model name:	Compaq Quadspeed
	Model number:	CDU76E	
	Revision:		1.0c
	Interface Type:	IDE
	SCSI ID:		n/a
	Jumper/Switch Settings:
	All jumpers in factory default position.

Hard Drive(s)
	Manufacturer:	Western Digital
	Model name:	Caviar 31000
	Model number:	WDC AC31000F	
	Revision:		22.20H30
	Size:			1082MB
	Interface:		IDE
	SCSI ID:		n/a

	Manufacturer:	Micropolis
	Model name:	2105
	Model number:	COMPAQ 2105	
	Revision:		15E3
	Size:			560MB
	Interface:		SCSI
	Jumper/Switch Settings:
	All jumpers in factory default position.

Floppy Drive(s)
	Manufacturer:	TEAC
	Model name:	FD-235HG
	Model number:	6325-U
	Jumper/Switch Settings:
	All jumpers in factory default position.
	
Graphics Adaptor(s)
	Manufacturer:	Compaq	
	Model name:	Qvision 1280/P 		
	Video RAM:	1MB
	RAM Type:	VRAM
	Interface:		Integrated PCI
	BIOS Rev. #:	12/01/94
	Jumper/Switch Settings:
	n/a

Serial Port(s)
	Ports:	1
	UART:	16550A compatible

Parallel Port(s)
	on-board, LPT1
	
Keyboard(s)
	Manufacturer:	Compaq
	Model name:	RT101
	Interface:		PS/2
	# of keys:		101
	Jumper/Switch Settings:
	n/a

Mice and Other Pointing Devices
	Manufacturer:	Compaq
	Model name:	M-S34
	Interface:		PS/2
	Jumper/Switch Settings:
	n/a

LAN Adaptor(s)
	Manufacturer:	AMD
	Model name:	Integrated Netflex-L
	Interface:		PCI
	Connectors:	AUI, TP*
	Jumper/Switch Settings:
	n/a

Sound Card(s)
	Manufacturer:	n/a (no sound installed)	
	Jumper/Switch Settings:
	n/a

Monitor(s)
	Manufacturer:	Compaq 
	Model name:	Qvision 200
	Size:			20 inches
	Max resolution:	1024 width x 1280 height @76Hz
	Jumper/Switch Settings:
	n/a

Note that only the specific components listed were tested.

Setup and Installation
Hardware Setup:
	See above for individual setup instructions for each adaptor.

CMOS settings:
To Access:
Press F10
Settings:
To Access:      	Press F10 when cursor jumps over to the right of the screen.  If NeXT is loaded then select partition 1.

INSPECT - Version PC10.06C
===========================

----------------------------------------------------------------------------
System : 

Date . . . . . . . . . . . . . .  9/29/95
Time . . . . . . . . . . . . . .  12:43:20

Product  . . . . . . . . . . . .  Compaq Deskpro 5120

Machine ID
  From System Board  . . . . . .  230

Processor  . . . . . . . . . . .  Pentium at 120 MHz
CPU ID . . . . . . . . . . . . .  0525

Numeric Coprocessor  . . . . . .  Integrated 387-Compatible

Secondary Cache  . . . . . . . .  256K

Expansion Bus  . . . . . . . . .  ISA, PCI

Asset tag  . . . . . . . . . . .  D527HSE3D363

CPU Mode . . . . . . . . . . . .  Real Mode

Current System Speed . . . . . .  High

System board revision level  . .  A

System serial number . . . . . .  D527HSE3D363

Temperature  . . . . . . . . . .  Caution

Compaq Deskpro 5120 is a trademark of Compaq Computer Corporation.

----------------------------------------------------------------------------
ROM : 

System ROM
    Revision . . . . . . . . . .  05/10/95
      Family . . . . . . . . . .  486G
    Flashable  . . . . . . . . .  Yes
    Socketed . . . . . . . . . .  No

Video Controller ROM
    Revision . . . . . . . . . .  12/01/94
      Family . . . . . . . . . .  V1

Keyboard Controller ROM
    Revision . . . . . . . . . .  C.7 06/14/91
      Family . . . . . . . . . .  K

Option ROMs  . . . . . . . . . .  C0000 - C7FFF 

----------------------------------------------------------------------------
Keyboard : 

Keyboard . . . . . . . . . . . .  Enhanced

----------------------------------------------------------------------------
System Ports : 

LPT Ports  . . . . . . . . . . .  LPT1 (Address 378)

COM Ports  . . . . . . . . . . .  COM1 (Address 3F8)

----------------------------------------------------------------------------
System Storage : 

SCSI Controller, Base Address 0x140

  Device . . . . . . . . . . . .  Compaq 535 MB SCSI Disk
  SCSI ID  . . . . . . . . . . .  0
  Revision . . . . . . . . . . .  15E3
  Model Number . . . . . . . . .  COMPAQ  2105
  Serial Number  . . . . . . . .  3042215540
  Drive capacity (blocks)  . . .  1090999
  Drive geometry (Cyl, Hds, Sec)  532, 64, 32

Embedded IDE Controller, Base Address 0x1f0

  Device . . . . . . . . . . . .  Compaq QuadSpeed CD-ROM
  Drive position . . . . . . . .  2
  Revision . . . . . . . . . . .  1.0c
  Model Number . . . . . . . . .  SONY    CD-ROM CDU76E-Q

Diskette Drive A . . . . . . . .  1.44 Megabyte (3.5 inch)
 
Drive Controller 1
  Standard Interface . . . . . .  Primary
  Hard Drive 1 . . . . . . . . .  Type  65 (1082.8 Megabyte)
  Serial Number  . . . . . . . .  WD-WT2721242035
  Firmware Revision 1  . . . . .  22.20H30
  Model Number . . . . . . . . .  WDC AC31000F
  1:1 Interleave Supported . . .  Yes
  Cylinders  . . . . . . . . . .  2098
  Heads  . . . . . . . . . . . .  16
  Sectors per Track  . . . . . .  63
  IntelliSafe Hard Drive Status.  OK

----------------------------------------------------------------------------
Graphics : 

Graphics Mode  . . . . . . . . .  12 (640 x 480 Graphics)

Primary Monitor attached to  . .  Compaq QVision 1280/P Graphics Controller
                                  with Video Graphics Color Monitor

Total Video Memory . . . . . . .  1024 Kbytes
Current Monitor  . . . . . . . .  Compaq QVision 200

Monitor serial number  . . . . .  507DA04BA178

----------------------------------------------------------------------------
Memory : 

Memory Boards Identified:
  System Board
   SIMM Bank 1
    SIMM Slot J7 . . . . . . . .     8 Megabytes
    SIMM Slot J8 . . . . . . . .     8 Megabytes
   SIMM Bank 2
    SIMM Slot J10  . . . . . . .     8 Megabytes
    SIMM Slot J11  . . . . . . .     8 Megabytes
   SIMM Bank 3
    SIMM Slot J12  . . . . . . .     0 Megabytes
    SIMM Slot J13  . . . . . . .     0 Megabytes
Total Compaq Memory  . . . . . .    32 Megabytes

Base Memory
  System Total . . . . . . . . .    639 Kbytes
  Amount Free  . . . . . . . . .    558 Kbytes (572112 Bytes)

Extended Memory
  Amount Free  . . . . . . . . .  31744 Kbytes

Expanded Memory
  LIM Driver Support . . . . . .  LIM driver not loaded

Memory Detected at Power-On
  Base Memory  . . . . . . . . .    640 Kbytes
  Extended Memory  . . . . . . .  31744 Kbytes
  Total Memory . . . . . . . . .  32768 Kbytes

----------------------------------------------------------------------------
Network : 

Integrated NetFlex-L ENET
    Network Type  . . . . . . . . Ethernet
    IRQ . . . . . . . . . . . . . 5
    IRQ Type  . . . . . . . . . . Level
    Speed . . . . . . . . . . . . 10MBPS
    Media Connector . . . . . . . 10Base-T (RJ-45)
    Network Address . . . . . . . 00805F2C127B

----------------------------------------------------------------------------
Miscellaneous : 

System Configuration Memory
  00 - 0F :    23 00 43 00    12 00 05 29    09 95 26 82    50 80 00 00
  10 - 1F :    40 00 F0 00    03 80 02 00    3C 41 00 00    00 00 00 08
  20 - 2F :    00 00 00 00    7E 29 00 40    00 9A 00 C1    03 00 04 7F
  30 - 3F :    00 3C 19 80    01 10 XX XX    XX XX XX XX    XX XX XX XX

Non-Volatile RAM 
  00 - 0F :    00 01 00 05    25 00 01 00    00 00 00 00    00 10 10 10
  10 - 1F :    01 00 06 00    00 01 00 00    00 00 00 00    3C 00 23 0C
  20 - 2F :    44 35 32 37    48 53 45 33    44 33 36 33    00 00 00 00
  30 - 3F :    32 08 10 C4    3F 00 00 00    00 00 32 08    10 84 3F 00
  40 - 4F :    00 00 00 00    00 00 00 FE    00 00 80 01    00 00 00 7C
  50 - 5F :    00 00 80 01    80 01 00 00    00 3C 00 00    80 01 09 5C
  60 - 6F :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  70 - 7F :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  80 - 8F :    0C 44 35 32    37 48 53 45    33 44 33 36    33 00 00 00
  90 - 9F :    00 1F D9 01    41 43 46 47    00 04 29 01    00 0E 11 AE
  A0 - AF :    07 10 40 00    01 0D 00 01    00 1C 07 03    00 87 78 03
  B0 - BF :    02 78 07 08    00 01 00 14    04 07 F8 03    0B 00 01 00
  C0 - CF :    14 0E 87 F0    01 01 F6 03    03 00 01 00    80 0A 00 01
  D0 - DF :    00 1C 06 02    00 05 F0 03    0E 00 01 00    14 02 9F 20
  E0 - EF :    00 9F A0 00    01 D0 04 08    00 01 00 14    00 03 40 00
  F0 - FF :    0E 00 01 00    18 04 04 8F    00 00 8F 80    00 1F C0 00

BIOS Data Area
  40:0000 :    F8 03 00 00    00 00 00 00    78 03 00 00    00 00 C0 9F
  40:0010 :    27 42 01 7F    02 97 00 00    00 00 26 00    26 00 31 02
  40:0020 :    01 1E 0D 1C    69 17 00 00    00 00 00 00    00 00 00 00
  40:0030 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:0040 :    E1 00 0C 13    26 01 00 A2    20 12 50 00    00 A0 00 00
  40:0050 :    00 21 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:0060 :    00 00 00 D4    03 29 30 12    05 59 8F 00    E0 B6 0C 00
  40:0070 :    00 00 00 12    00 01 00 00    14 14 14 14    01 01 01 01
  40:0080 :    1E 00 3E 00    1D 10 00 60    F9 11 0B 01    50 00 00 05
  40:0090 :    07 00 00 00    00 00 10 00    00 00 00 00    00 00 00 00
  40:00A0 :    00 00 00 00    00 00 00 00    22 00 00 C0    00 00 00 00
  40:00B0 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:00C0 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:00D0 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:00E0 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00
  40:00F0 :    00 00 00 00    00 00 00 00    00 00 00 00    00 00 00 00

Interrupt Vector Table (including INSPECT)
  00 - 03 :    2DA2:0555      0070:06F4      0DBB:0016      0070:06F4   
  04 - 07 :    0070:06F4      F000:FF54      F000:93CC      F000:9BD0   
  08 - 0B :    0DBB:003C      0DBB:0045      F000:9BD0      F000:9BD0   
  0C - 0F :    F000:9BD0      F000:9BD0      0DBB:00B7      0070:06F4   
  10 - 13 :    1724:34CE      F000:F84D      F000:F841      0070:0774   
  14 - 17 :    F000:E739      0070:084A      F000:E82E      F000:EFD2   
  18 - 1B :    F000:C883      0070:07FB      F000:FE6E      0070:06EE   
  1C - 1F :    F000:FF53      F000:F0A4      0000:0522      C000:4FE3   
  20 - 23 :    0019:40CC      0019:40F8      0E30:0439      0019:40D2   
  24 - 27 :    8F59:43F6      0019:42E5      0019:436C      0019:A1CC   
  28 - 2B :    0019:40D2      0070:0762      0019:40D2      0019:40D2   
  2C - 2F :    0019:40D2      0019:40D2      0019:40D2      1003:25C9   
  30 - 33 :    1940:D3EA      F000:9B00      0019:40D2      1003:0A4E   
  34 - 37 :    0019:40D2      0019:40D2      0019:40D2      0019:40D2   
  38 - 3B :    0019:40D2      0019:40D2      0019:40D2      0019:40D2   
  3C - 3F :    0019:40D2      0019:40D2      0019:40D2      3D82:04FB   
  40 - 43 :    F000:EC59      F000:E801      F000:F065      C000:2B72   
  44 - 47 :    F000:9BD0      F000:9BD0      F000:E401      F000:9BD0   
  48 - 4B :    1425:00F3      F000:9BD0      F000:9BD0      F000:9BD0   
  4C - 4F :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  50 - 53 :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  54 - 57 :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  58 - 5B :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  5C - 5F :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  60 - 63 :    0000:0000      0000:0000      0000:0000      0000:0000   
  64 - 67 :    0000:0000      0000:0000      0000:0000      0000:0000   
  68 - 6B :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  6C - 6F :    F000:9BD0      F000:9BD0      F000:9BD0      F000:9BD0   
  70 - 73 :    0DBB:0052      F000:9C1F      F000:9BD0      F000:9BD0   
  74 - 77 :    1003:2774      F000:9C28      0DBB:0117      F000:9BD0   
  78 - 7B :    0000:0000      0000:0000      0000:0000      0000:0000   
  7C - 7F :    0000:0000      0000:0000      0000:0000      0000:0000   
  80 - 83 :    0000:0000      0000:0000      0000:0000      0000:0000   
  84 - 87 :    0000:0000      0000:0000      0000:0000      0000:0000   
  88 - 8B :    0000:0000      0000:0000      0000:0000      0000:0000   
  8C - 8F :    0000:0000      0000:0000      0000:0000      0000:0000   
  90 - 93 :    0000:0000      0000:0000      0000:0000      0000:0000   
  94 - 97 :    0000:0000      0000:0000      0000:0000      0000:0000   
  98 - 9B :    0000:0000      0000:0000      0000:0000      0000:0000   
  9C - 9F :    0000:0000      0000:0000      0000:0000      0000:0000   
  A0 - A3 :    0000:0000      0000:0000      0000:0000      0000:0000   
  A4 - A7 :    0000:0000      0000:0000      0000:0000      0000:0000   
  A8 - AB :    0000:0000      0000:0000      0000:0000      0000:0000   
  AC - AF :    0000:0000      0000:0000      0000:0000      0000:0000   
  B0 - B3 :    0000:0000      0000:0000      0000:0000      0000:0000   
  B4 - B7 :    0000:0000      0000:0000      0000:0000      0000:0000   
  B8 - BB :    0000:0000      0000:0000      0000:0000      0000:0000   
  BC - BF :    0000:0000      0000:0000      0000:0000      0000:0000   
  C0 - C3 :    0000:0000      0001:0000      0000:0000      0000:0000   
  C4 - C7 :    0000:0000      0000:0000      0000:0000      0000:0000   
  C8 - CB :    0000:0000      0000:0000      0000:0000      0000:0000   
  CC - CF :    0000:0000      0000:0000      0000:0000      0000:0000   
  D0 - D3 :    0000:0000      0000:0000      0000:0000      0000:0000   
  D4 - D7 :    0000:0000      0000:0000      0000:0000      0000:0000   
  D8 - DB :    0000:0000      0000:0000      0001:0000      0000:0246   
  DC - DF :    0003:27DA      000E:93DE      0000:07C8      0000:0090   
  E0 - E3 :    000E:2000      000E:07F8      000E:0004      000C:0731   
  E4 - E7 :    F88B:022A      EF6C:007C      0082:F000      6A2D:0090   
  E8 - EB :    D9B4:0090      697D:D9C5      0048:F88B      0000:F88B   
  EC - EF :    E3F9:B35E      0007:F000      19BC:03D4      1003:0311   
  F0 - F3 :    5D88:03C9      0040:0000      C000:5C7C      58B4:0003   
  F4 - F7 :    C000:0022      0022:03D4      0003:0000      0D25:56E7   
  F8 - FB :    0040:0040      8F04:0246      0003:0080      007C:0000   
  FC - FF :    0000:4227      0000:012C      EC3A:0030      0246:F000   

PCI Devices Information
  Signature  . . . . . . . . . .  PCI
  Config Mechanism #1  . . . . .  Supported
  Config Mechanism #2  . . . . .  Not Supported
  Spec Cycle for Config #1 . . .  Supported
  Spec Cycle for Config #2 . . .  Not Supported
  BIOS Interface Version . . . .  2.10
  Last PCI Bus Number  . . . . .  0
  Number of PCI Devices  . . . .  2

  Bus Number . . . . . . . . . .  0
  Device Number  . . . . . . . .  10
  Function Number  . . . . . . .  00h
  Slot Number  . . . . . . . . .  0
  Vendor ID  . . . . . . . . . .  0E11h
  Device ID  . . . . . . . . . .  3033h
  Revision ID  . . . . . . . . .  12h
  Device Type  . . . . . . . . .  VGA Compatible Controller
  Programming Interface  . . . .  00h
  Expansion ROM Base Address . .  FF000000h
  IRQ Line . . . . . . . . . . .  15
  IRQ Pin  . . . . . . . . . . .  INTA#
  Memory Address Base  . . . . .  40000000h
  Memory Address Length  . . . .  1000000h 

  Bus Number . . . . . . . . . .  0
  Device Number  . . . . . . . .  11
  Function Number  . . . . . . .  00h
  Slot Number  . . . . . . . . .  0
  Vendor ID  . . . . . . . . . .  1022h
  Device ID  . . . . . . . . . .  2000h
  Revision ID  . . . . . . . . .  02h
  Device Type  . . . . . . . . .  Ethernet Controller
  Programming Interface  . . . .  00h
  Expansion ROM Base Address . .  0h
  IRQ Line . . . . . . . . . . .  5
  IRQ Pin  . . . . . . . . . . .  INTA#
  IO Address Base  . . . . . . .  1000h
  IO Address Length  . . . . . .  20h

---------------------------------------------------------------------------- 

ECU settings (EISA-bus systems only):
n/a 
	
Special installation instructions:

Driver settings:
Use Configure.app to load and configure the following drivers:
Display 
	Qvision
Pointing Device:
	PS2 Mouse
Network 
	AMDPCnet32NetworkDriver
SCSI 
	AIC6X60
Audio 
	none
Other
	EIDE/ATAPI controller
	SerialPorts
	Floppy Disk
	PS2 Keyboard
	PCIBus
	EISABus
	Parallel port
					
Known Problems
This system was tested with 1MB of Video RAM.  The only video modes supported are:
Width	Height 	Refresh 	Colorspace
768		1024	66Hz	256/8
768		1024	66Hz	BW:8
768		1024	60Hz	256/8
768		1024	60Hz	BW:8

600		800		72Hz	555/16
600		800		60Hz	555/16

choosing a video mode other than the ones listed will cause a system panic during boot-up.
If you do set the video mode to an unsupported mode, type "config=hd( )Default" at the boot: prompt to start the system up in 640 x 480 @60Hz BW:2 mode. 

See Also: (None)