NEXTSTEP for Intel Processors
Tested Compatible System

Title:	Andromeda/133 
Last Updated:	December 13 1995
Tested with:		3.3

Product Vendor:
Applied Instruments
47757 Warm Springs Blvd.
Fremont, CA  94539
Tel: (510) 490-7117
Fax: (510) 490-7198

Explanation of Compatibility Testing 
NEXTSTEP Compatible systems are tested by third parties using a test procedure developed by NeXT. NeXT approves the use of the "NEXTSTEP Compatible" designation for these systems based on the completeness of the test results submitted by these NeXT-trained 3rd parties.
 
For more detailed information on the NICE program, please refer to NeXTanswers document 1903_Compatible_Systems_Tested_With_NEXTSTEP.rtf

Note:	NeXT accepts no support responsibilities or liability whatsoever for any system authorized to use the "NEXTSTEP Compatible" designation, nor does NeXT represent that their test procedures or training--even if followed exactly by the 3rd party performing the test work--are in any way complete or exhaustive. Known or unknown errors may be present in configurations which are designated as "NEXTSTEP Compatible" which could adversely affect the operation of these systems. Support for compatible systems may be provided by the PC vendor or System integrator. 

Tested Components:
Applied Instruments reports testing a system configuration consisting of the following components:
Summary information only. Contact Applied Instruments for more specific configuration information

System CPU Board(s)
	CPU:		Intel Pentium, 133 MHzMHz
	RAM:		64 MBMB maximum tested
	ISA slots:		4 (plus one slot in combo with PCI)
	PCI slots:		3 (plus one slot in combo with ISA)

SCSI Controller(s)
	Manufacturer:	Adaptec
	Model name:	Ultra Wide SCSI Master
	Interface:		PCI

CD-ROM Drive(s)
	Manufacturer:	n/a

Hard Drive(s)
	Manufacturer:	Quantum
	Interface:		Synchronous Wide SCSI-2
	Size:		2.05GB

Graphics Adaptor(s)
	Manufacturer:	ATI 
	Model name:	Graphics Pro Turbo 
	Video RAM:	2MB
	RAM Type:	VRAM, 70ns
	Interface:		PCI

Serial Port(s)
	Ports:	2
	UART:	16550A

Parallel Port(s)
	on-board, LPT1

Keyboard(s)
	Manufacturer:	NMB
	Model name:	Right Touch
	Interface:		AT (with AT to PS/2 adapter cable)
	# of keys:		101

Mice and Other Pointing Devices
	Manufacturer:	Microsoft
	Model name:	Mouse
	Interface:		PS/2 (Mini Din)

LAN Adaptor(s)
	Manufacturer:	Cogent
	Model name:	eMaster+
	Interface:		PCI
	Connectors:	AUI, *BNC, *TP
	* Adaptor tested with this connector

Sound Card(s)
	Manufacturer:	n/a 

Monitor(s)
	Manufacturer:		Sampo 
	Model name:		AlphaScan 17GX
	Size:			17" Diagonal
	Max resolution:	1600x1200x60

Note that only the specific components listed were tested.

Setup and Installation
Hardware Setup:
	See above for individual setup instructions for each adaptor.

CMOS settings:
To Access:
 press <F1> when prompted during boot
Settings:
Use Factory defaults 

ECU settings (EISA-bus systems only):
n/a 
	
Special installation instructions:
1.  FTG Light Pen Driver requires use of Serial Port driver version 3.33, available as Next Answer #1942.
2.  Must use latest version of Adaptec AHA-2940 Driver at installation time.  If necessary, add Auto Detect ID 0x81789004 per Next Answer #1760.

Driver settings:
Use Configure.app to load and configure the following drivers:
Display
	ATIMach64DisplayDriver
Pointing Device 
	PS2Mouse
	FTGSerialLightPen
Network 
	CogentEM960NetworkDriver
SCSI 
	Adaptec2940SCSIDriver
Other
	Floppy Disk
	PS2Keyboard
	PCIBus
	EISABus
	ISASerialPort, #1
	ISASerialPort, #2
	Serial PortServer
	ParallelPort

Known Problems

See Also:	(None)