CPU

On-Chip Cache

8--64 KBytes (Typical) Secondary

Cache

32--256 KBytes (Typical)

Main Memory

1--64 MBytes (Typical)

Increasing Memory Latency