)

N

RZ ( 1 ) UNIX Programmer’s Manual RZ ( 1

AME rx, rb, rz – XMODEM, YMODEM, ZMODEM (Batch) file receive

SYNOPSIS

rz [– +abepqtuvy] r rb [– +abqtuvy] x [– abceqtuv] file [ gz file ... –][v]rzCOMMAND

DESCRIPTION This program uses error correcting protocols to receive files over a dial-in serial port from a variety of l programs running under PC-DOS, CP/M, and other operating systems. It is invoked from a shel

Unix, prompt manually, or automatically as a result of an "sz file ..." command given to the calling program.

n T Rz is not intended be called from cu(1), or other communications programs. Unix flavors of Ome echnology’s Professional-YAM communications software are available for dial-out applications. ® y t Rz (Receive ZMODEM) receives files with the ZMODEM batch protocol. Pathnames are supplied b he sending program, and directories are made if necessary (and possible). Normally, the "rz" command - t is automatically issued by the calling ZMODEM program, but some defective ZMODEM implementa ions may require starting rz the old fashioned way. Rz does not support ZMODEM Crash Recovery, a compression, and other ZMODEM features. Unix flavors of Professional-YAM may be linked to "rz" nd used in place of this program to support these ZMODEM features.

s ( Rb receives file(s) with YMODEM, accepting either standard 128 byte sectors or 1024 byte sector YAM sb -k option). The user should determine when the 1024 byte block length actually improves

I throughput without causing lost data or even system crashes.

f True YMODEM (Omen Technology trademark) file information (file length, etc.) is received, the file n length controls the number of bytes written to the output dataset, and the modify time and file mode (iff on zero) are set accordingly.

If no True YMODEM file information is received, slashes in the pathname are changed to underscore, C and any trailing period in the pathname is eliminated. This conversion is useful for files received from P/M systems. With YMODEM, each file name is converted to lower case unless it contains one or

R more lower case letters.

x receives a single file with XMODEM or XMODEM-1k protocol. The user should determine when - p the 1024 byte block length actually improves throughput without causing problems. The user must sup ly the file name to both sending and receiving programs. Up to 1023 garbage characters may be

G added to the received file.

z is a shell script which calls sz to command Pro-YAM or ZCOMM to transmit the specified files. E Pathnames used with gz must be escaped if they have special significance to the Unix shell. XAMPLE: gz "-a C:∗.c D:∗.h"

Rz may be invoked as rzCOMMAND (with an optional leading – as generated by login(1)). For each e t received file, rz will pipe the file to ‘‘COMMAND filename’’ where filename is the name of th ransmitted file with the file contents as standard input.

7th Edition OMEN

) RZ ( 1 ) UNIX Programmer’s Manual RZ ( 1

Each file transfer is acknowledged when COMMAND exits with 0 status. A non zero exit status ter-

A minates transfers.

typical use for this form is rzrmail which calls rmail(1) to post mail to the user specified by the transmitted file name. For example, sending the file "caf" from a PC-DOS system to rzrmail on a Unix

O system would result in the contents of the DOS file "caf" being mailed to user "caf".

n some systems, the login directory must contain a link to COMMAND as login sets SHELL=rsh w Unix hich disallows absolute pathnames. If invoked with a leading ‘‘v’’, rz will report progress to /tmp/rzlog. The following entry works for SYS III/V:

Unix rzrmail::5:1::/bin:/usr/local/rzrmail e p If the SHELL environment variable includes rsh or rksh (restricted shell), rz will not accept absolut athnames or references to a parent directory, will not modify an existing file, and removes any files

I received in error.

f rz is invoked with stdout and stderr to different datasets, Verbose is set to 2, causing frame by frame

T progress reports to stderr. This may be disabled with the q option.

he meanings of the available options are:

a Convert files to conventions by stripping carriage returns and all characters beginning with t Unix he first Control Z (CP/M end of file). . c b Binary (tell it like it is) file transfer override

Request 16 bit CRC. XMODEM file transfers default to 8 bit checksum. YMODEM and D ZMODEM normally use 16 bit CRC.

Output file data to /dev/null; for testing. (Unix only) d e Force sender to escape all control characters; normally XON, XOFF, DLE, CR-@-CR, an Ctrl-X are escaped.

p (ZMODEM) Protect: skip file if destination file exists. t q Quiet suppresses verbosity. tim Change timeout to tim tenths of seconds. v Verbose causes a list of file names to be appended to /tmp/rzlog . More v’s generate more y output.

Yes, clobber any existing files with the same name.

EXAMPLES (Pro-YAM command) P <ALT-2> ro-YAM Command: sz ∗.h ∗.c ) (This automatically invokes rz on the connected system. O SEE ALS ZMODEM.DOC, YMODEM.DOC, Professional-YAM, crc(omen), sz(omen), usq(omen), undos(omen)

NOTES

Compile time options required for various operating systems are described in the source file.

ZMODEM’s support of XOFF/XON flow control allows proper operation in many environments that do . T not support XMODEM uploads. Unfortunately, not all timesharing systems support input flow control he TTY input buffering on some systems may not adequately buffer long blocks or streaming input at s high speed. You should suspect this problem when you can’t send data to the Unix system at high peeds using ZMODEM, but YMODEM-1k or XMODEM-1k, when YMODEM with 128 byte blocks

T works properly.

he DSZ or Pro-YAM zmodem l numeric parameter may be set to a value between 64 and 1024 to

7th Edition OMEN

) RZ ( 1 ) UNIX Programmer’s Manual RZ ( 1

limit the burst length ("zmodem pl128"). Although this compromises ZMODEM’s throughput,

I ZMODEM’s superior reliability remains intact.

f a program that does not properly implement the specified file transfer protocol causes rz to "hang" . E the port after a failed transfer, either wait for rz to time out or keyboard a dozen Ctrl-X characters very reported instance of this problem has been corrected by using ZCOMM, Pro-YAM, DSZ, or other

M program with a correct implementation of the specified protocol.

any programs claiming to support YMODEM only support XMODEM with 1k blocks, and they often

I don’t get that quite right.

n the case of a few poorly designed microcomputers, sending serial data to a tty port at sustained high l b speeds has been known to cause lockups, system halts, kernel panics, and occasional antisocia ehaviour. This problem is not unique to rz; CRT terminals with block mode transmission and line t noise have the same effect. When experimenting with high speed input to a system, consider rebooting he system if the file transfers are not successful, especially if the personality of the system appears

T altered.

he Unix "ulimit" parameter must be set high enough to permit large file transfers to Unix. - g 32 bit CRC code courtesy Gary S. Brown. Directory creation code from John Gilmore’s PD TAR pro ram.

BUGS

Rz is not intended be called from cu(1), or other communications programs. Unix flavors of Omen

R Technology’s Professional-YAM communications software are available for dial-out applications.

z does not support ZMODEM Crash Recovery and many other ZMODEM features. Unix flavors of

P Professional-YAM may be linked to "rz" to support these features.

athnames are restricted to 127 characters. In XMODEM single file mode, the pathname given on the m command line is still processed as described above. The ASCII option´s CR/LF to NL translation erely deletes CR´s; undos(omen) performs a more intelligent translation.

VMS VERSION The VMS version does not set the file time. . T VMS C Standard I/O and RMS may interact to modify file contents unexpectedly

he VMS version does not support invocation as rzCOMMAND . The current VMS version does not

A support XMODEM, XMODEM-1k, or YMODEM.

ccording to the VMS documentation, the buffered input routine used on the VMS version of rz intro- s duces a delay of up to one second for each protocol transaction. This delay may be significant for very hort files. Removing the "#define BUFREAD" line from rz.c will eliminate this delay at the expense

F of increased CPU utilization.

or high speed operation, try increasing the SYSGEN parameter TTYiTYPAHDSZ to 256. - t The VMS version causes DCL to generate a random off the wall error message under some error condi ions; this is a result of the incompatibility of the VMS "exit" function with the Unix/MSDOS standard.

7th Edition OMEN

)

Z

RZ ( 1 ) UNIX Programmer’s Manual RZ ( 1

MODEM CAPABILITIES Rz supports incoming ZMODEM binary (-b), ASCII (-a), protect (-p), clobber (-y), and append (-+)

T requests. Other options sent by the sender are ignored. The default is protect (-p) and binary (-b). he Unix versions support ZMODEM command execution.

FILES

rz.c, crctab.c, rbsb.c, zm.c, zmodem.h Unix source files. . / rz.c, crctab.c, vrzsz.c, zm.c, zmodem.h, vmodem.h, vvmodem.c, VMS source files tmp/rzlog stores debugging output generated with -vv option (rzlog on VMS).

4

i

7th Edition OMEN

i ii