Export

After clicking the Export menu item an Save Panel appears and a filename can be selected for exporting. The Export Save Panel contains switches for selecting the export mode:

The first radio button defines which buffer should be exported. If Current Buffer  is selected only the current buffer will be exported. The All Buffer  mode exports all buffers and appends the buffer numbers to the filenames.

The second radio button lets you select the order in which  the data will be exported. There is also the possibillity to export either the X or Y value only.

The third radio button is used to enable/disable comment and axis text exporting.

With the last radio button the line-end-character can be defined. Lf  is the normal mode and Cr/Lf  is only needed for PC's or other low level computers.