Default VGA/Generic SVGA Display
,

, Display Devices

This device driver is for ISA, EISA, VL and PCI Bus systems.

This graphics driver is designed to support on-board VGA and generic SVGA implementations. 

For VGA, the display resolution is fixed at 640x480 in two bits per pixel depth. This mode is available for all display adapters.

Generic SVGA driver provides a fixed display resolution of 800x600 in two bits per pixel depth. The driver does so by emulating VESA display mode 0x6A which is often implemented in the video BIOS. It is expected that all VESA-compliant video BIOS manufacturers will implement this mode.

Both these display modes are designed to provide a default display mode only. You should use a supported local bus based display adapter for better performance.

Known Bugs:  Console support is not implemented for Generic SVGA (800x600) display adapters.

Warning:  If you plan to change display adapters, be sure to use the Configure application to change the display driver to Default VGA Adapter before you remove the old display adapter (see NeXTanswer 1824 for details on changing display adapters). 

,
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.