3Com EtherLink III ISA Adapter
¬

¬Network Devices

This device driver is designed to run on an Intel-based computer running OPENSTEP for Mach Release 4.1.

Supported Hardware 
	3Com EtherLink III 3C509 ISA		(AUI, BNC)
	3Com EtherLink III 3C509-TP ISA		(AUI, RJ-45)
	3Com EtherLink III 3C509-Combo	ISA	(AUI, BNC, RJ-45)

Installing the Adaptor 
· 	Install the adapter in the system and configure its Port Address using 3Com's 3C509.EXE utility.  Use this value in the configuration steps below.  Refer to the 3Com EtherLink III User's Guide for complete information.

Configuration 
·  	Log in as root and run Configure to add the adapter to the system.  
· 	Click on the Network Devices icon at the top of Configure's "Summary of Devices" window.  In the Add Network Devices panel that opens, select the radio button labeled "Show All Installed Drivers" if it is not already highlighted.  
· 	Select "3Com EtherLink III ISA Adapter" from the list, and click Add. 
·  	Choose a Port Address and IRQ Level that do not conflict with other devices on the system.  
·  	Select the Connector type.
·  	Click Done, then click Save, then quit Configure.

¬
	
See also

·	"Add a Device" in Configure's on-line help.

·	See NeXTanswer 1824 for general information on installing and configuring device drivers.