SGI Desktop Audio Hardware
Performance Specifications
(Typical)

 Indigo
 Indigo2
 Indy

Compiled by Amit Shoham 10/93

Send comments etc. to: Ted Marsh tm@esd.sgi.com

NOTE: All specifications subject to change without notice

                                    FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        5kOhm nominal
  Amplitude at Full Scale:
        1Vpp to 10Vpp
  Level Control:
        2 independent digitally
        controlled analog attenuators
  Analog to Digital Converter:
        16 bit, Delta Sigma
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.
        64x oversampling

 ANALOG STEREO LINE LEVEL INPUTS

 Frequency Response:
      +/- 0.43dB 20Hz to 20kHz
 Total Harmonic Distortion + Noise:
      At 1kHz: 0.0027%  20Hz to 20kHz maximum: 0.0057%
      (max occurs at 22.3Hz)
 Residual Noise, Unweighted:
       -90.77dB
 Residual Noise, A weighted:
       -93.73dB
 Interchannel Isolation:
       1kHz: -74.42dB
      10kHz: -55.49dB
      20kHz: -49.34dB

10 100 1k 10k 30k

FREQ(Hz)

FLTLVL(%FS)

0.0 .00100

.00200

.00300

.00400

.00500

.00600

.00700

.00800

.00900

.01000

FLTLVL(%FS)

INDIGO:ADC_THD+N & vs 14 AUG 92 16:30:50

TEST CONDITIONS

Unless otherwise stated, all
parameters are measured under
the following conditions:

Analog Test Signal Level:
      1Vrms
Test Signal Output Impedance:
      600 Ohms
Sampling Rate:
      48kHz
Measurement Bandwidth:
      17Hz to 22kHz, Unweighted

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

A-D frequency response & vs 14 AUG 92 16:30:39

                           INDIGO AUDIO
                            PERFORMANCE

ANALOG STEREO LINE LEVEL OUTPUTS

Frequency Response:
     +/- 0.30dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.0059%  20Hz to 20kHz maximum: 0.0270%
     (max occurs at 10.19kHz)
Residual Noise, Unweighted:
      -87.52dB
Residual Noise, A weighted:
      -91.04dB
Interchannel Isolation:
      1kHz: -74.90dB
     10kHz: -63.75dB
     20kHz: -59.74dB

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

D-A Frequency Response & vs 11 AUG 92 14:26:32

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1 THD+N(%)

INDIGO:DAC_THD+N DA-THD & vs 11 AUG 92 14:26:47

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-130.0

-120.0

-110.0

-100.0

-90.00

-80.00

-70.00

-60.00

-50.00

-40.00

-30.00

-20.00

-10.00 0.0 AMP1(dBr)

D-A Noise SpectrumDA-RNP & vs 11 AUG 92 14:29:09

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        600 Ohms nominal
  Amplitude at Full Scale:
        6.0Vpp
  Digital Output Filter:
        Linear Phase FIR
        16 bit in, 18 bit out
  Digital to Analog Converter:
        18 bit
        8x oversampling
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.

TOTAL HARMONIC DISTORTION + NOISE

                                          FREQUENCY RESPONSE

                                                                    RESIDUAL NOISE

                                                  TEST CONDITIONS

                                                  Unless otherwise stated, all
                                                  parameters are measured under
                                                  the following conditions:

                                                  Digital Test Signal Level:
                                                        100% of full scale
                                                  Output Destination Impedance:
                                                        5 kOhms
                                                  Sampling Rate:
                                                        48kHz
                                                  Measurement Bandwidth:
                                                        17Hz to 22kHz, Unweighted

                             INDIGO AUDIO
                              PERFORMANCE

   PHYSICAL SPECIFICATIONS

   Connector:
         Single-ended 3.5mm stereo
         phone
   Impedance:
         2kOhm
   Amplitude at Full Scale:
         0.25Vpp to 2.5Vpp
   Microphone Power Supply:
         +3V DC, 1mA max

                                        FREQUENCY RESPONSE

  TOTAL HARMONIC DISTORTION + NOISE

10 100 1k 10k 30k

FREQ(Hz)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

MIC freq. responseMIC-FRESP vs 14 AUG 92 17:00:13

10 100 1k 10k 30k

FREQ(Hz)

0.0 .00100

.00200

.00300

.00400

.00500

.00600

.00700

.00800

.00900

.01000

FLTLVL(%FS)

MIC THD+NMC-THD vs 14 AUG 92 17:00:28

                                                          TEST CONDITIONS

                                                          Unless otherwise stated, all
                                                          parameters are measured under
                                                          the following conditions:

                                                          Analog Test Signal Level:
                                                                0.75Vrms
                                                          Test Signal Output Impedance:
                                                                600 Ohms
                                                          Sampling Rate:
                                                                48kHz
                                                          Measurement Bandwidth:
                                                                17Hz to 22kHz, Unweighted

MICROPHONE INPUT

Frequency Response:
     +/- 0.47dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.0030%  20Hz to 20kHz maximum: 0.0102%
     (max occurs at 22.3Hz)
Residual Noise, Unweighted:
      -90.54dB
Residual Noise, A weighted:
      -93.51dB

                          INDIGO AUDIO
                           PERFORMANCE

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Headphone Impedance:
        16 Ohms
  Headphone Level:
        200mW into 32 Ohm load
  Headphone and Speaker Level Control:
        2 independent digitally
        controlled analog attenuators
  Speaker:
        2.6" diameter dynamic
  Speaker Sound Pressure Level:
        88dB/W
  Speaker Output Level:
        3W max, 1.5W nominal

                                     FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

Headphone freq. response & vs 14 AUG 92 16:49:10

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1

0.5 THD+N(%)

Headphone THD+NHP-THD & vs 14 AUG 92 16:49:19

                                                       TEST CONDITIONS

                                                       Unless otherwise stated, all
                                                       parameters are measured under
                                                       the following conditions:

                                                       Digital Test Signal Level:
                                                             100% of full scale
                                                       Output Destination Impedance:
                                                             150 Ohms
                                                       Sampling Rate:
                                                             48kHz
                                                       Measurement Bandwidth:
                                                             17Hz to 22kHz, Unweighted

STEREO HEADPHONE OUTPUT

Frequency Response:
     +/- 0.78dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.0744%  20Hz to 20kHz maximum: 0.3809%
     (max occurs at 6.94kHz)
Residual Noise, Unweighted:
      -89.77dB
Residual Noise, A weighted:
      -94.55dB
Interchannel Isolation:
      1kHz: -50.06dB
     10kHz: -39.07dB
     20kHz: -35.09dB

                          INDIGO AUDIO
                           PERFORMANCE

                                     FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        20kOhm nominal
  Amplitude at Full Scale:
        0.63Vpp to 8.4Vpp
  Level Control:
2       2 independent digitally
       controlled amplifiers,
       internal to codecs
  Analog to Digital Converter:
        16 bit, Delta-Sigma
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.

 ANALOG STEREO LINE LEVEL INPUTS

 Frequency Response:
      +/- 0.81dB 20Hz to 20kHz
 Total Harmonic Distortion + Noise:
      At 1kHz: <0.006%  20Hz to 20kHz maximum: <0.007%
 Residual Noise, Unweighted:
       -86dB
 Residual Noise, A weighted:
       -88dB
 Interchannel Isolation:
       1kHz: -82dB
      10kHz: -72dB
      20kHz: -67dB

                                                         TEST CONDITIONS

                                                         Unless otherwise stated, all
                                                         parameters are measured under
                                                         the following conditions:

                                                         Analog Test Signal Level:
                                                               1Vrms
                                                         Test Signal Output Impedance:
                                                               600 Ohms
                                                         Sampling Rate:
                                                               48kHz
                                                         Measurement Bandwidth:
                                                               17Hz to 22kHz, Unweighted

                          INDIGO2 AUDIO
                            PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

A-D frequency response & vs 22 OCT 93 14:34:22

10 100 1k 10k 30k

FREQ(Hz)

FLTLVL(%FS)

0.0 .00100

.00200

.00300

.00400

.00500

.00600

.00700

.00800

.00900

.01000

FLTLVL(%FS)

INDIGO:ADC_THD+N & vs 22 OCT 93 14:35:01

 ANALOG STEREO LINE LEVEL OUTPUTS

 Frequency Response:
      +/- 1.2dB 20Hz to 20kHz
 Total Harmonic Distortion + Noise:
      <0.02%  20Hz to 20kHz
 Residual Noise, Unweighted:
       -81dB
 Residual Noise, A weighted:
       -85dB
 Interchannel Isolation:
       1kHz: -80dB
      10kHz: -75dB
      20kHz: -71dB

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        600 Ohms nominal
  Amplitude at Full Scale:
        4.7Vpp
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.

TOTAL HARMONIC DISTORTION + NOISE

                                          FREQUENCY RESPONSE

                                                                    RESIDUAL NOISE

                                                  TEST CONDITIONS

                                                  Unless otherwise stated, all
                                                  parameters are measured under
                                                  the following conditions:

                                                  Digital Test Signal Level:
                                                        100% of full scale
                                                  Output Destination Impedance:
                                                        5 kOhms
                                                  Sampling Rate:
                                                        48kHz
                                                  Measurement Bandwidth:
                                                        17Hz to 22kHz, Unweighted

                           INDIGO2 AUDIO
                             PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

D-A Frequency Response & vs 22 OCT 93 14:40:26

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1

1 THD+N(%)

INDIGO:DAC_THD+N DA-THD & vs 22 OCT 93 14:40:48

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-130.0

-120.0

-110.0

-100.0

-90.00

-80.00

-70.00

-60.00

-50.00

-40.00

-30.00

-20.00

-10.00 0.0 AMP1(dBr)

D-A Noise SpectrumDA-RNP & vs 22 OCT 93 14:43:02

PHYSICAL SPECIFICATIONS

Connector:
      Single-ended 3.5mm stereo
      phone
Impedance:
      1.5kOhm
Amplitude at Full Scale:
      0.063Vpp to 0.84Vpp
Microphone Power Supply:
      +3V DC, 1mA max

                                      FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

                                                          TEST CONDITIONS

                                                          Unless otherwise stated, all
                                                          parameters are measured under
                                                          the following conditions:

                                                          Analog Test Signal Level:
                                                                0.1 Vrms
                                                          Test Signal Output Impedance:
                                                                600 Ohms
                                                          Sampling Rate:
                                                                48kHz
                                                          Measurement Bandwidth:
                                                                17Hz to 22kHz, Unweighted

MICROPHONE INPUT

Frequency Response:
     +/- 0.66dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.0053%  20Hz to 20kHz maximum: 0.0067%
     (max occurs at 17.5kHz)
Residual Noise, Unweighted:
      -86dB
Residual Noise, A weighted:
      -89dB

                          INDIGO2 AUDIO
                            PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

MIC freq. responseMC-FRES vs 22 OCT 93 14:50:14

10 100 1k 10k 30k

FREQ(Hz)

0.0 .00100

.00200

.00300

.00400

.00500

.00600

.00700

.00800

.00900

.01000

FLTLVL(%FS)

MIC THD+NMC-THD vs 22 OCT 93 14:50:30

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Headphone Impedance:
        10 Ohms
  Headphone Level:
        57mW into 32 Ohm load
  Headphone and Speaker Level Control:
        2 independent digitally
        controlled analog attenuators
  Speaker
        70mm x 40mm
  Speaker Sound Pressure Level:
        80dB @ 1W, 1 meter

                                     FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

                                                        TEST CONDITIONS

                                                        Unless otherwise stated, all
                                                        parameters are measured under
                                                        the following conditions:

                                                        Digital Test Signal Level:
                                                              100% of full scale
                                                        Output Destination Impedance:
                                                              150 Ohms
                                                        Sampling Rate:
                                                              48kHz
                                                        Measurement Bandwidth:
                                                              17Hz to 22kHz, Unweighted

STEREO HEADPHONE OUTPUT

Frequency Response:
     +/- 2.3dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.02%  20Hz to 20kHz maximum: 0.3%
     (max occurs at 19.3kHz)
Residual Noise, Unweighted:
      -88dB
Residual Noise, A weighted:
      -90dB
Interchannel Isolation:
      1kHz: -87dB
     10kHz: -76dB
     20kHz: -73dB

                          INDIGO2 AUDIO
                            PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

Headphone freq. response & vs 22 OCT 93 14:44:57

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1

0.5 THD+N(%)

Headphone THD+NHP-THD & vs 22 OCT 93 14:45:11

                                    FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        10kOhm nominal
  Amplitude at Full Scale:
        0.63Vpp to 8.4Vpp
  Level Control:
        2 independent digitally
        controlled amplifiers,
        internal to codecs
  Analog to Digital Converter:
        16 bit, Delta Sigma
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.

 ANALOG STEREO LINE LEVEL INPUTS

 Frequency Response:
      +/- 0.62dB 20Hz to 20kHz
 Total Harmonic Distortion + Noise:
      At 1kHz: 0.0063%  20Hz to 20kHz maximum: <0.009%
 Residual Noise, Unweighted:
       -84dB
 Residual Noise, A weighted:
       -87dB
 Interchannel Isolation:
       1kHz: -80dB
      10kHz: -73dB
      20kHz: -68dB

                                                        TEST CONDITIONS

                                                        Unless otherwise stated, all
                                                        parameters are measured under
                                                        the following conditions:

                                                        Analog Test Signal Level:
                                                              1Vrms
                                                        Test Signal Output Impedance:
                                                              600 Ohms
                                                        Sampling Rate:
                                                              48kHz
                                                        Measurement Bandwidth:
                                                              17Hz to 22kHz, Unweighted

                             INDY AUDIO
                            PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

A-D frequency response & vs 02 SEP 93 17:18:29

10 100 1k 10k 30k

FREQ(Hz)

FLTLVL(%FS)

0.0 .00100

.00200

.00300

.00400

.00500

.00600

.00700

.00800

.00900

.01000

FLTLVL(%FS)

INDIGO:ADC_THD+N & vs 02 SEP 93 17:18:49

 ANALOG STEREO LINE LEVEL OUTPUTS

 Frequency Response:
      +/- 0.88dB 20Hz to 20kHz
 Total Harmonic Distortion + Noise:
      <0.02%  20Hz to 20kHz
 Residual Noise, Unweighted:
       -83dB
 Residual Noise, A weighted:
       -86dB
 Interchannel Isolation:
       1kHz: -82dB
      10kHz: -68dB
      20kHz: -64dB

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Impedance:
        600 Ohms nominal
  Amplitude at Full Scale:
        4.7Vpp
  Sampling Rates:
        32kHz, 44.1kHz, 48kHz,
        serial digital input rate,
        divisors of above rates.

TOTAL HARMONIC DISTORTION + NOISE

                                          FREQUENCY RESPONSE

                                                                    RESIDUAL NOISE

                                                  TEST CONDITIONS

                                                  Unless otherwise stated, all
                                                  parameters are measured under
                                                  the following conditions:

                                                  Digital Test Signal Level:
                                                        100% of full scale
                                                  Output Destination Impedance:
                                                        5 kOhms
                                                  Sampling Rate:
                                                        48kHz
                                                  Measurement Bandwidth:
                                                        17Hz to 22kHz, Unweighted

                              INDY AUDIO
                             PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

D-A Frequency Response & vs 02 SEP 93 17:24:17

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1

1 THD+N(%)

INDIGO:DAC_THD+N DA-THD & vs 02 SEP 93 17:24:31

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-130.0

-120.0

-110.0

-100.0

-90.00

-80.00

-70.00

-60.00

-50.00

-40.00

-30.00

-20.00

-10.00 0.0 AMP1(dBr)

D-A Noise SpectrumDA-RNP & vs 02 SEP 93 17:26:39

PHYSICAL SPECIFICATIONS

Connector:
      Single-ended 3.5mm stereo
      phone
Impedance:
      2kOhm
Amplitude at Full Scale:
      0.063Vpp to 0.84Vpp
Microphone Power Supply:
      +3V DC, 1mA max

                                      FREQUENCY RESPONSE

                                                          TEST CONDITIONS

                                                          Unless otherwise stated, all
                                                          parameters are measured under
                                                          the following conditions:

                                                          Analog Test Signal Level:
                                                                0.1Vrms
                                                          Test Signal Output Impedance:
                                                                600 Ohms
                                                          Sampling Rate:
                                                                48kHz
                                                          Measurement Bandwidth:
                                                                17Hz to 22kHz, Unweighted

MICROPHONE INPUT

Frequency Response:
     +/- 0.38dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.01%  20Hz to 20kHz maximum: 0.013%
     (max occurs at 17.5kHz)
Residual Noise, Unweighted:
      -80dB
Residual Noise, A weighted:
      -83dB

                             INDY AUDIO
                            PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

MIC freq. responseMC-FRES vs 02 SEP 93 17:30:27

  PHYSICAL SPECIFICATIONS

  Connector:
        Single-ended 3.5mm stereo
        phone
  Headphone Impedance:
        10 Ohms
  Headphone Level:
        57mW into 32 Ohm load
  Headphone and Speaker Level Control:
        2 independent digitally
        controlled analog attenuators
  Speaker
        70mm x 40mm
  Speaker Sound Pressure Level:
        80dB @ 1W, 1 meter

                                     FREQUENCY RESPONSE

TOTAL HARMONIC DISTORTION + NOISE

                                                        TEST CONDITIONS

                                                        Unless otherwise stated, all
                                                        parameters are measured under
                                                        the following conditions:

                                                        Digital Test Signal Level:
                                                              100% of full scale
                                                        Output Destination Impedance:
                                                              150 Ohms
                                                        Sampling Rate:
                                                              48kHz
                                                        Measurement Bandwidth:
                                                              17Hz to 22kHz, Unweighted

STEREO HEADPHONE OUTPUT

Frequency Response:
     +/- 3.3dB 20Hz to 20kHz
Total Harmonic Distortion + Noise:
     At 1kHz: 0.06%  20Hz to 20kHz maximum: 0.25%
     (max occurs at 19.3kHz)
Residual Noise, Unweighted:
      -90dB
Residual Noise, A weighted:
      -93dB
Interchannel Isolation:
      1kHz: -80dB
     10kHz: -61dB
     20kHz: -56dB

                              INDY AUDIO
                             PERFORMANCE

10 100 1k 10k 30k

FREQ(Hz)

AMP2(dBr)

-10.00

-8.000

-6.000

-4.000

-2.000 0.0 2.0000

4.0000

6.0000

8.0000

10.000

AMP1(dBr)

Headphone freq. response & vs 02 SEP 93 17:36:32

10 100 1k 10k 30k

GENFRQ(Hz)

THD+N(%)

0.001

0.010

0.1

0.5 THD+N(%)

Headphone THD+NHP-THD & vs 02 SEP 93 17:37:00

DIGITAL COAXIAL SERIAL INPUT/OUTPUT

Connector:
      Single ended 3.5mm stereo phone
Input Impedance:
      75 Ohms, transformer coupled
Input Level:
      0.5Vpp nominal
Input Sample Rates:
      30kHz to 50kHz
Output Impedance:
      75 Ohms, transformer coupled
Output Level:
      0.5Vpp into 75 Ohm load
Output Sample Rates:
      32kHz, 44.1kHz, 48kHz,
      serial input sample rate,
      divisors of above rates.
Resolution:
      Supports up to 24 bits per sample
Coding:
      AES-3, IEC-958