NEWLINE	equ	-2
HT	equ	09h
LF	equ	0ah
CR	equ	0dh
LINENEW	equ	CR+LF*256	;the way a newline is stored in memory.
