*
* Printer Definition for EPSON FX80
*
*--------------------------------------------------------------------
* The following options are set immediately.  They are not activated
* by parameters.
*--------------------------------------------------------------------
DOT                     * DOT LETTER LASER
TOPMARGIN 0
BOTMARGIN 0
LINELEN 80
LINESPAGE 58              * Printable lines per page
*MICSPACE 27 65 9         * SET MICRO SPACING to n 72nds of an inch
*FORMLEN 27 67 66         * set form length in lines  66 = 66 lines
*FORMLENI 27 67 0 11      * Set form length in inches 11 = inches
FFEED 12                * Form Feed Character
*--------------------------------------------------------------------
* The following parameters are activated by parameters
*--------------------------------------------------------------------
COMPON 15               * set compressed print
COMPOFF 18
EXPAND 27 87 1          * SET EXPANDED PRINT
EXPANDOFF 27 87 0
EMPH 27 69
EMPHOFF 27 70
DOUBLE 27 71               * double strike (nlq) printing
DOUBLEOFF 27 72
*NLQ 27 73 2
*NLQOFF 27 73 0
*DLFONT 27 37 1 0         * Download font off
*DLFONTOFF 27 37 0 0
PERFSKIP  27 78 4        * set number lines to skip over perfs (4)
PERFSKIPOFF 27 79
ONEDIR 27 85 1           * print in only 1 direction
ONEDIROFF 27 85 0
8LPI 27 48
6LPI 27 50
*CHARSET 27 54            * Select char set 2   27 55 = char set 1
*CHARSETOFF 27 55
12CPI 27 77              * 12 characters per inch
12CPIOFF 27 80
