DA Byte_Param     Data_Bits                 Data bits
PA Char_Param     Parity                    Parity
ST Byte_Param     Stop_Bits                 Stop bits
BA Word_Param     Baud_Rate                 Baud rate
PO Byte_Param     Comm_Port                 Serial port
BS String_Param   BS_String                 Backspace key sends
DE String_Param   Ctrl_BS_String            Ctrl-Backspace key sends
TE Terminal_Param Terminal_To_Emulate       Terminal to emulate
LO Boolean_Param  Logging_On                Perform logging to log file
LF Boolean_Param  Add_Lf                    Add line feeds to incoming CRs
MI String_Param   Modem_Init                Initialization string
MD String_Param   Modem_Dial                Dialing command
MC String_Param   Modem_Connect             Connect message
MN String_Param   Modem_No_Carrier          No Carrier message
MB String_Param   Modem_Busy                Busy message
ME String_Param   Modem_Escape              Escape string
MT PosInt_Param   Modem_Escape_Time         Escape delay (ms)
MH String_Param   Modem_Hang_Up             Hang Up string
MO LongInt_Param  Modem_Time_Out            Dialing timeout (secs)
MR LongInt_Param  Modem_Redial_Delay        Redial time (secs)
SM Boolean_Param  Silent_Mode               Silent (mute) mode on
PM Boolean_Param  Play_Music_On             Play music in ANSI/BBS mode
LE Boolean_Param  Local_Echo                Local echo on
FC Char_Param     FK_CR                     Function key carriage return
FD Char_Param     FK_Delay                  Function key delay
FW Char_Param     FK_Wait_For               Function key await string
TT Transfer_Param Default_Transfer_Type     Default file transfer type
SD String_Param   Screen_Dump_Name          Text mode screen dump file
GD Integer_Param  GMT_Difference            # hours local time lags GMT
TB PosInt_Param   Transfer_Bells            # bells after transfer
MA String_Param   Modem_Answer              Answer phone string
MS String_Param   Modem_Host_Set            Host mode modem setup string
FM Char_Param     FK_Ctrl_Mark              Function key control character
TM VidMode_Param  New_Text_Mode             Video mode
CF Color_Param    New_ForeGround_Color      Foreground color
CB BColor_Param   New_BackGround_Color      Background color
CT Color_Param    New_Menu_Text_Color       Menu text color
CM Color_Param    New_Menu_Frame_Color      Menu frame color
MW PosInt_Param   Modem_Command_Delay       Intercharacter delay (ms)
BP Boolean_Param  CompuServe_B_On           Do CompuServe B protocol
EB Boolean_Param  Mahoney_On                Do EXEC PC BBS commands
DP Char_Param     Default_Prefix            Default dialing prefix character
BB PosInt_Param   Max_Review_Length         Review buffer size
XM Boolean_Param  Exploding_Menus           Use exploding menus
CH Boolean_Param  Modem_Carrier_High        Carrier line always high
XB PosInt_Param   Max_Write_Buffer          File transfer buffer size
AB Boolean_Param  Host_Auto_Baud            Detect caller speed from modem
VB BColor_Param   VT100_BackGround_Color    VT100 background color
VF Color_Param    VT100_ForeGround_Color    VT100 foreground color
VE Color_Param    VT100_Bold_Color          VT100 bold color
VU Color_Param    VT100_Underline_Color     VT100 underline color
KC KCheck_Param   Kermit_Chk_Type           Block check type
KD Boolean_Param  Kermit_Debug              Kermit debug mode
KE SpecChar_Param Kermit_EOL                End of block character
KH SpecChar_Param Kermit_Header_Char        Block header character
KN PosInt_Param   Kermit_Npad               Number of pad characters
KP SpecChar_Param Kermit_Pad_Char           Pad character
KQ SpecChar_Param Kermit_Quote_Char         Control quote character
KR SpecChar_Param Kermit_Repeat_Char        Repeat quote character
KS PosInt_Param   Kermit_Init_Packet_Size   Maximum short block size
KT PosInt_Param   Kermit_TimeOut            Timeout in seconds
KW PosInt_Param   Kermit_Delay_Time         Delay before sending (secs)
K8 SpecChar_Param Kermit_Quote_8_Char       Eighth-bit quoting character
DT Char_Param     Default_Postfix           Default dialing postfix character
WS Boolean_Param  Write_Screen_Memory_Par   Write directly to video memory
BD Boolean_Param  Alter_Baud_Rate           Match speed of called system
EC Boolean_Param  Exact_Capture             Exact capture
FS Char_Param     FK_Script_Ch              Function key command character
XS Boolean_Param  Check_CTS                 Check Clear To Send
XD Boolean_Param  Check_DSR                 Check Data Set Ready
MX String_Param   Modem_Host_UnSet          Host mode termination string
MF String_Param   Modem_Dial_End            Dialing command postfix
HW Boolean_Param  Hard_Wired                Hard-wired connection
BL PosInt_Param   Break_Length              Break length in 1/100 seconds
DD Path_Param     Download_Dir_Path         Download directory
GW PosInt_Param   Gossip_Window_Size        Gossip mode top window size
GL Boolean_Param  Gossip_Line_Mode          Use gossip line mode
SG String_Param   Graphics_Dump_Name        Graphics mode screen dump file
SP Char_Param     Script_Parameter_Marker   Script parameter marker
KL PosInt_Param   Kermit_Window_Size        Sliding windows size
DR Boolean_Param  Drop_Dtr_At_End           Drop DTR at end
CJ Boolean_Param  Close_Comm_For_Dos        Close serial port on jump to DOS
US Boolean_Param  Use_Short_Dial_Menu       Use short dialing menu
WR Boolean_Param  Wait_For_Retrace_Par      Wait for retrace when writing to video
EN String_Param   Editor_Name               Editor name
LN String_Param   Browser_Name              File browser name
SS Boolean_Param  Show_Status_Line          Display status line
SE Boolean_Param  Show_Status_Time          Display time on status line
PS String_Param   Printer_Setup             Printer setup string
XO Boolean_Param  Do_Xon_Xoff_Checks        Do XON/XOFF flow control
CS BColor_Param   New_Border_Color          Border color
VS BColor_Param   VT100_Border_Color        VT100 border color
VA String_Param   VT100_Answerback_Message  VT100 answerback message
DY Boolean_Param  Downsize_Ymodem           Allow switch to short blocks
EP Boolean_Param  Evict_Partial_Trans       Evict partially downloaded files
SC PosInt_Param   Script_Learn_Buffer_Size  Script learn buffer size
SL PosInt_Param   Script_Learn_Lines        Script learn lines count
DF Date_Param     Date_Format
TF Time_Param     Time_Format
SF Path_Param     Script_Path               Script directory
EU Boolean_Param  Extended_Keyboard         Allow DOS calls for 101 key keyboards
DS PosInt_Param   Dialing_Dir_Size_Max      Size of dialing directory
FP Path_Param     Function_Key_Path         Function key directory
HD Path_Param     Host_Mode_Download        Host mode download directory
HU Path_Param     Host_Mode_Upload          Host mode upload directory
HB LongInt_Param  Host_Mode_Blank_Time      # seconds to wait before blanking screen
Y0 Boolean_Param  Use_Ymodem_Header         Send block 0 in Xmodem 1K transfer
SO ScrOrder_Param Script_Search_Order
U0 Boolean_Param  Use_Block_Zero            Use block 0 information
EK Boolean_Param  Extended_Keypad           Recognize extended keypad
KA SpecChar_Param Kermit_Handshake_Char     Handshake character
BC Box_Param      Box_Chars                 Box drawing characters
CK PosInt_Param   Command_Key
AM Boolean_Param  Attended_Mode             Run in attended mode
AC PosInt_Param   Ascii_Char_Delay          Intercharacter delay
AL PosInt_Param   Ascii_Line_Delay          Interline delay
AP SpecChar_Param Ascii_Pacing_Char         Pacing character
AS PosInt_Param   Ascii_Line_Size           Maximum text line size
AX Boolean_Param  Ascii_Send_Asis           Byte stream transfer
AE String_Param   Ascii_CR_LF_String
AF Boolean_Param  Ascii_Send_Blank          Send empty line as blank
AZ Boolean_Param  Ascii_Use_CtrlZ           Send <CTRL>Z at end of transfer
AD Boolean_Param  Ascii_Show_Text           Display text during transfer
AT Boolean_Param  Ascii_Translate           Translate incoming characters
IM Boolean_Param  Edit_Insert_Mode          Start editing in insert mode
XC PosInt_Param   Xmodem_Char_Wait          Character wait time
XA PosInt_Param   Xmodem_Ack_Wait           Acknowledgement wait time
XT PosInt_Param   Xmodem_Max_Errors         Maximum allowed errors per block
XH PosInt_Param   Xmodem_Block_Wait         Start of block wait time
AK Boolean_Param  Auto_Load_FunKeys         Auto load function keys
DI Boolean_Param  Use_Dos_Buffer_In         Use DOS function $0A for input
AU String_Param   Host_CTTY_Device          CTTY driver name prefix
YT Boolean_Param  YTerm_On                  Allow YTerm protocol
DO Boolean_Param  Use_Dos_Con_Output        Use DOS console output
SU Boolean_Param  Auto_Unload_Scripts       Auto unload scripts
MG String_Param   Modem_Ring                Ring detect message
DL PosInt_Param   New_Max_Screen_Line       Maximum physical screen length
DC PosInt_Param   New_Max_Screen_Col        Maximum physical screen width
IB PosInt_Param   Async_Buffer_Length       Comm buffer input size
OB PosInt_Param   Async_OBuffer_Length      Comm buffer output size
F0 ExtTrans_Param External_Trans_Def[1]     External file transfer protocol 1
F1 ExtTrans_Param External_Trans_Def[2]     External file transfer protocol 2
F2 ExtTrans_Param External_Trans_Def[3]     External file transfer protocol 3
F3 ExtTrans_Param External_Trans_Def[4]     External file transfer protocol 4
F4 ExtTrans_Param External_Trans_Def[5]     External file transfer protocol 5
F5 ExtTrans_Param External_Trans_Def[6]     External file transfer protocol 6
F6 ExtTrans_Param External_Trans_Def[7]     External file transfer protocol 7
F7 ExtTrans_Param External_Trans_Def[8]     External file transfer protocol 8
F8 ExtTrans_Param External_Trans_Def[9]     External file transfer protocol 9
F9 ExtTrans_Param External_Trans_Def[10]    External file transfer protocol 10
FF Boolean_Param  Auto_Find_FileNames       Auto find file names for transfers
P1 Hexi_Param     Default_Com_Base[1]       Port 1 hardware address
P2 Hexi_Param     Default_Com_Base[2]       Port 2 hardware address
P3 Hexi_Param     Default_Com_Base[3]       Port 3 hardware address
P4 Hexi_Param     Default_Com_Base[4]       Port 4 hardware address
I1 PosInt_Param   Default_Com_Irq[1]        Port 1 interrupt request line
I2 PosInt_Param   Default_Com_Irq[2]        Port 2 interrupt request line
I3 PosInt_Param   Default_Com_Irq[3]        Port 3 interrupt request line
I4 PosInt_Param   Default_Com_Irq[4]        Port 4 interrupt request line
V1 Hexi_Param     Default_Com_Int[1]        Port 1 interrupt vector
V2 Hexi_Param     Default_Com_Int[2]        Port 2 interrupt vector
V3 Hexi_Param     Default_Com_Int[3]        Port 3 interrupt vector
V4 Hexi_Param     Default_Com_Int[4]        Port 4 interrupt vector
T1 String_Param   User_Term_Name[1]         User terminal 1 definition file
T2 String_Param   User_Term_Name[2]         User terminal 2 definition file
T3 String_Param   User_Term_Name[3]         User terminal 3 definition file
SB Color_Param    Status_BackGround_Color   Status line foreground color
SA BColor_Param   Status_ForeGround_Color   Status line background color
SR Boolean_Param  Reverse_Status_Colors     Reverse standard colors for status line
CA Color_Param    New_Menu_Text_Color_2     Secondary menu text color
CC Color_Param    New_Menu_Title_Color      Secondary menu title color
VC Boolean_Param  Auto_Change_Arrows        Do VT100 applic./numeric keypad switch
SH Boolean_Param  Auto_Strip_High_Bit       Strip high bit in terminal mode
ZB PosInt_Param   Zmodem_BlockSize          Block length for Zmodem transfers
FN FileN_Param    FileName                  File name for transfer
FH PosInt_Param   FK_Delay_Time             Function key intercharacter delay (ms)
SZ Boolean_Param  Software_Scroll_Par       Use software scrolling
UP Boolean_Param  Use_Prev_Key_Text         Show previous command in command line mode
TU Boolean_Param  Send_Upper_Case_Only      Translate keyboard input to upper case
KX PosInt_Param   Kermit_Extended_Block     Maximum long block size
T4 String_Param   User_Term_Name[4]         User terminal 4 definition file
T5 String_Param   User_Term_Name[5]         User terminal 5 definition file
HP Host_Param     Privilege                 Host mode privilege
AW Boolean_Param  ATI_Ega_Wonder            ATI EGA Wonder/ATI VIP VGA (TM) card installed
YX Boolean_Param  Honor_XOff_Ymodem         Honor XON/XOFF in Ymodem sends
NL Boolean_Param  New_Line                  Add line feeds to outgoing CRs
WH PosInt_Param   Window_Hold_Time          Time to hold window displays (1/10 secs)
01 Menu_Param                               Serial port hardware settings
02 Ascii_Param                              Ascii transfer parameters
03 Xmodem_Param                             Xmodem/Ymodem transfer parameters
04 ExtTrans_Param                           External protocol definitions
05 VT100_Param                              VT100 settings
06 Key_Param      Command_Key_Name          Command mode key
07 Boolean_Param  Use_Military              Use 24 hour time format
08 String_Param   Date_Format_String        Date format
09 String_Param   Script_Order_String       Script search order
10 Boolean_Param  Ascii_CRLF                Send CR/LF sequence at end of line
11 Menu_Param                               Backspace key sends BS, <CTRL>BS sends DEL
12 Menu_Param                               Backspace key sends DEL, <CTRL>BS sends BS
EG Boolean_Param  Allow_EGA_Graphics        Allow EGA graphics mode
ML Boolean_Param  Modem_Hold_Line           Hold line after abortive dial
VK String_Param   KeyPad_Appl_On_File       Key file for VT100 applic. mode
VN String_Param   KeyPad_Appl_Off_File      Key file for VT100 numeric mode
YF Boolean_Param  Use_Full_Path_Name        Send/receive full path name in Ymodem
KK Boolean_Param  Kermit_AutoDownload       Allow Kermit autodownload
ZA Boolean_Param  Zmodem_AutoDownload       Allow Zmodem autodownload