NT Registry Data added by Novell NT Client v3.5

Changes made to the HKEY_LOCAL_MACHINE key handle are as follows:

hive	CLONE

key	CLONE

subkey	Control

subkey	NetworkProvider

subkey	Order

value	ProviderOrder

value data	NetWareWorkstation	added value data

subkey	Print

subkey	Novell	added subkey

subkey	NDSConnections	added subkey

subkey	NOVELL_INC	added subkey for NDS tree name

subkey	E34-HPIVSIMX-1	added subkey for network queue

subkey Printers

subkey	PRV-SRVCOMM,E34-HPIVSIMX-1	added subkey for pserver & queue name

subkey	PrinterDriverData	added subkey

subkey	Providers

subkey	NetWare Print Services	added subkey

subkey	WOW

value	KnownDLLs

value data	netware.drv	added value data to end of string

subkey	Services

subkey	IpxApi	added subkey

subkey	IpxSpx	added subkey

subkey	LSL	added subkey

subkey	NE20001	added subkey specific to driver

subkey	NetWareAutoReconnect	added subkey

subkey	NetWareWorkstation	added subkey

subkey	NWIP	added subkey

subkey	NWPopUp	added subkey

subkey	OdiLoad	added subkey

subkey	ODINSUP	added subkey

subkey	OdiSourceRouting	added subkey

subkey	OdiVMLID	added subkey

subkey	ResMgr	added subkey

subkey	SpxApi	added subkey

subkey	WinSock

subkey	Parameters

value	Transports

value data	IpxSpx	added value data

hive	SOFTWARE

key	Novell	added key

subkey	Novell key contains many subkeys

key	Microsoft

subkey	Windows NT

subkey	CurrentVersion

subkey	File Manager

subkey	AddOns

value	Novell NetWare Extension	added value

subkey	NetworkCards

subkey	1	one to many subkeys MAY be added

subkey	NWCS	added subkey

subkey	Perflib

subkey	009

value	Counter

value data	NetWare Redirector Stats	added lots of value data

Ioctls/sec

I/O context zone hits/sec

I/O context zone misses/sec

Maximum conncurrent connections

Current connections

Total successful reconnects

Total bytes written/sec

Total bytes read or written/sec

Total IO requests completed/sec

Total asynchronous IO requests/sec

Total NCP's completed/sec

NetWare ODI Stats

Total transmitted packets/sec

Total received packets/sec

No ECB available count

Transmit packet too big count

Transmit packet too small count

Receive buffer overflow count

Receive packet too big count

Receive packet too small count

Total miscellaneous transmit failures

Total miscellaneous receive failures

Transmit retries

Corrupt packets count

Length consistency check failures

Number of bytes transmitted/sec

Number of bytes received/sec

Transmitted packets with group destinations/sec

Received packets with group destinations/sec

Number of adapter resets

Time since adapter last changed operational states

Queued ECB's

NetWare LSL Stats

Total transmit packet requests/sec

Number of requests to obtain an ECB/sec

Number refused requests to obtain an ECB

Number completed AES Events/sec

Number events posponed because of Critical region functions/sec

Number Cancel events that failed

Number ECB's stolen from the Hold Queue/sec

Number of enqueued Send events that have occurred/sec

Total received packets dispatched/sec

Total incoming packets not claimed by any Protocol Stack/sec

value	Help

value data	Displays statistics about the NetWare Redirector	added data

Displays the number of Ioctls/sec issued to the NetWare Redirector

Displays the number of I/O context zone hits/sec for the NetWare Redirector

Displays the number of I/O context zone misses/sec for the NetWare Redirector

Displays the maximum number of conncurrent connections

Displays the number of current connections

Displays the total number of successful reconnects

Displays the total number of failed reconnects

Displays the total number of transport failures

Displays the total number of retries

Displays the total number of retry exhaustions

Displays the total number of server busy packets

Displays the total number of open files"

Displays the total number of bytes read/sec

Displays the total number of bytes written/sec

Displays the total number of bytes read or written/sec

Displays the total number of IO requests completed/sec

Displays the total number of asynchronous IO requests/sec

Displays the total number of NCP's completed/sec

Displays statistics about NetWare ODI

Displays the number of packets successfully transmitted onto the media/sec

Displays the number of packets reported as successfully received without errors/sec. This counter is independent of whether the packet is accepted by a host

Displays the number of times an incoming packet was discarded due to the lack of host receive buffers or the host not wanting the packet

Displays the number of times a send packet was too big for transmission

Displays the number of requested packets for transmission that were normally too small to be transmitted. The packets might still have been sent if the MLID does padding

Displays the number of times the adapter's receive buffer pool was exhausted, which caused subsequent incoming packets to be discarded

Displays the number of times a packet was received that was too large to fit into preallocated receive buffers provided by the host or too large for media definitions

Displays the number of times a packet was received the was too small for media definitions

Displays the number of times a packet failed to transmit for reasons unknown

Displays the number of times a packet failed to be received for reasons unknown

Displays the number of times the MLID retried a transmit operation because of a failure

Displays the number of times the MLID received a packet with corrupt data (for example, CRC errors)

Displays the number of times the MLID received a packet that did not pass the length consistency checks

Displays the number of bytes (including low-level headers) the MLID successfully transmitted onto the media/sec

Displays the number of bytes (including low-level headers) the MLID successfully received/sec

Displays the number of packets the MLID transmitted with a group destination address/sec

Displays the number of packets the MLID received with a group destination address/sec

Displays the number of times the adapter was reset due to an internal failure of a call to the MLID's DriverReset function

Displays the time (platform dependent clock, such as number of ticks) since the adapter last changed operational state, for example, Loaded, DriverShutdown, or DriverReset, etc

Displays the number of transmit ECB's that are queued for the adapter

Displays statistics about NetWare LSL

Displays the total number of packets that requested transmission/sec (whether they were actually transmitted or not)

Displays the total number of get ECB requests/sec

Displays the total number of get ECB requests that failed because of unavailable resources

Displays the number of AES events/sec

Displays the number of events that were postponed because of critical region functions/sec

Displays the number of cancel events that failed

Displays the number of ECB's on the hold queue that were reused before they were removed from the hold queue/sec

Displays the number of enqueued send events that have occurred/sec

Displays the number of packets being received/sec

Displays the number of incoming packets that were not claimed by any protocol stack/sec

hive	SYSTEM

key	CurrentControlSet

subkey	Control

subkey	Lsa

value	Authentication Packages

value data	nwv1_0	added value data

subkey	NetworkProvider

subkey	Order

value	ProviderOrder	added value

subkey	Print

subkey	Providers

subkey	NetWare Print Services	added subkey

subkey	ServiceGroupOrder

value	List

value data	NetWare Services ODI ODI Drivers added data to end of string

subkey	WOW

value	KnownDLLs

value data	netware.drv	added value data to end of string

subkey	Services

subkey	IpxApi	added subkey

subkey	IpxSpx	added subkey

subkey	LSL	added subkey

subkey	NE20001	added subkey specific to ODI driver

subkey	NetWareAutoReconnect	added subkey

subkey	NetWareWorkstation	added subkey

subkey	NWIP	added subkey

subkey	NWPopUp	added subkey

subkey	OdiLoad	added subkey

subkey	ODINSUP	added subkey

subkey	OdiSourceRouting	added subkey

subkey	OdiVMLID	added subkey

subkey	ResMgr	added subkey

subkey	SpxApi	added subkey

subkey	WinSock

subkey	Parameters

value	Transports

value data	IpxSpx	added value data

Changes made to the HKEY_CURRENT_USER key handle are as follows:

hive	Network

key	F	many keys added for all drive mappings

hive	Software

key	NetWare	added key

subkey NDSConnections	added subkey

subkey	F	many subkeys added for NDS drive mappings

subkey Parameters	added key

value	NWLanguage	added value

Changes made to the HKEY_USERS key handle are as follows:

hive	DEFAULT

key	Software

subkey NetWare	added subkey

subkey	Parameters	added subkey

value	NWLanguage	added value

value data	ENGLISH	added value data added

hive	S-1-5-21-82539751-1635331623-1097073633-1000	Security ID numbers will vary!

key	Network

subkey	F	many subkeys added for all drive mappings

key	Software

subkey NetWare	added subkey

subkey NDSConnections	added subkey

subkey	F	many subkeys added for NDS drive mappings

subkey Parameters	added key

value	NWLanguage	added value