InS_StArT
NI9210.COM
1.0
^Racal InterLan MCA/NI9210 Ethernet MLID,NI9210.COM,00M,0FDF
?Driver is self-configuring.
$O00M(NODE ADDRESS)
0
7FFFFFFFFFFF
*O00M(FRAME)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD

