InS_StArT
OCTOK16.COM
1.0
^Olicom Token-Ring MC 16/4 Adapter,OCTOK16.COM,00M
?The driver can communicate across Source Routing bridges. To enable this, load the ROUTE.COM module after OCTOK16.COM
!OIEM(PORT)I/O Port
?If more than one Token-Ring 16/4 adapter is installed, use the PORT parameter to identify the adapter. If no value is entered, the driver will search for an adapter and use the one at the lowest I/O Port address.
A20
A24
A50
A54
$OIEM(NODE ADDRESS)Node Address
400000000000
7FFFFFFFFFFF
$OIEM(MAX FRAME SIZE)Maximum Frame Size
?Maximum frame size accepted by the driver. The default is 4216.
632
17960
*OIEM(FRAME)Frame Type(s)
?Select the frame type(s) used by the protocols in the workstation. If no frame type(s) is specified, TOKEN-RING MSB will be supported. The LSB and MSB attributes are mutually exclusive and should not both be selected for the same frame type.
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
InS_EnD
