InS_StArT
E30ODI.COM
1.0
^Cabletron Systems Ethernet E3010,E30ODI.COM,00M,5606
^Cabletron Systems Ethernet E3010-X,E30ODI.COM,00M,5607
^Cabletron Systems Ethernet E3020,E30ODI.COM,00M,5600
^Cabletron Systems Ethernet E3020-X,E30ODI.COM,00M,5601
^Cabletron Systems Ethernet E3030,E30ODI.COM,00M,5602
^Cabletron Systems Ethernet E3030-X,E30ODI.COM,00M,5603
^Cabletron Systems Ethernet E3040,E30ODI.COM,00M,5604
^Cabletron Systems Ethernet E3040-X,E30ODI.COM,00M,5605
?Select the options you will use.
!R00M(SLOT) Slot Number
?Note: If you don't select a slot number, the first E30 board found will be used.
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS) Node Address
0
FFFFFFFFFFFF
*R00M(FRAME) Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs maybe using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
