InS_StArT
ES3210.COM
1.0
^Racal-Datacom ES3210 ODI MLID,ES3210.COM,0E0,RII0101
?The driver is self-configuring.
$O0E0(NODE ADDRESS)Node Address
0
7FFFFFFFFFFF
*O0E0(FRAME)Frame Type
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD


