InS_StArT
IBMFDDIO.COM
1.0,IBMFDDI.BIN
^IBM FDDI DOS ODI LAN driver for NetWare,IBMFDDIO.COM,00M,8EF4
?The IBM FDDI DOS ODI LAN driver is the terminate-stay-resident (TSR) device driver for the DOS environment.  This driver works with the IBM FDDI FIBER ADAPTER /A or IBM FDDI COPPER ADAPTER /A."
!R00M(SLOT)Slot Number
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS)Node Address
0
7FFFFFFFFFFF
*O00M(FRAME)Media Frame Types
@FDDI_802.2
FDDI_SNAP
!O00M(ATTACHMENTCLASS)FDDI Station Attachment Class
?Attachment Class defines the station as a single attachment (1) station or a dual attachment (2) station.  If Attachment Class is not specified, the driver will determine the setting based on the the IBM FDDI adapters (base and extender) installed.
1
2
!O00M(RXBUFFERS)Number of receive buffers
?The RXBUFFERS keyword specifies the number of receive buffers used by the IBMFDDIO LAN driver.  The value for this keyword must be one of:  1, 2, 4. The default is 2. (NOTE:  Each receive buffer takes 4500 bytes of memory.)
1
2
4
!O00M(TXBUFFERS)Number of transmit buffers
?The TXBUFFERS keyword specifies the number of 4500-byte transmit buffers used by the IBMFDDIO LAN driver.  The value for this keyword must be one of:  1, 2, 4. The default is 2.
1
2
4
InS_EnD
