InS_StArT
INTEL596.COM
1.0
^Intel596,INTEL596.COM,IE0
?This driver is used for systems compatible with the Intel LAN596 specification.  The LAN circuits can be either built directly into the system or onto an adapter board.
!RIE0(NETID)Hardware Configuration in ROM
?0 = No, 1 = Yes.  See your hardware documentation for the correct value.
@0
1
!OIE0(DRIV)Hardware Type
?This is optional.  See your hardware documentation for the correct value.  For the ISA motherboard implementation se
@1
2
$OIE0(GLOB)Global Options
?This is optional.  See your hardware documentation for the correct value.  For the ISA motherboard implementation se
0
FF
@8
$OIE0(ARB)Other Options (ARB)
?This is optional.  See your hardware documentation for the correct value.
0
FF
@0
!OIE0(PORT)Base I/O Port
?This is optional.  See your hardware documentation for the correct value.  For the ISA motherboard implementation th
100 
120
140
160
300
320
340
360
!OIE0(INT)Interrupt Number
?This is optional.  See your hardware documentation for the correct value.  For the ISA motherboard implementation th
5
7
9
10
11
12
15
!OIE0(DMA)DMA Channel
?This is optional.  See your hardware documentation for the correct value.
5
6
7
$OIE0(SLOT)Slot Number
?This is optional.  See your hardware documentation for the correct value.  For the PE596DBM EISA demo board you shou
1
12
$RIE0(FIFO)FIFO Threshold
?This is optional.  See your hardware documentation for the correct value.
0
F
@8
$RIE0(ON)T-ON Value
?This is optional.  See your hardware documentation for the correct value.
0
FFFF
@200
$RIE0(OFF)T-OFF Value
?This is optional.  See your hardware documentation for the correct value.
0
FFFF
@2
*RIE0(FRAME)Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD

