InS_StArT
NI5210.COM
1.0
^Racal-Datacom NI5210 ODI MLID,NI5210.COM,IE0
?Select the options that match your board's jumper settings. Preset settings match default configuration.
!RIE0(INT)Hardware Interrupt
@2
3
4
5
7
!RIE0(MEM)Base Memory Address
?Note: For 16K Memory Card select an address with the sufix "400".
@D0000 200
C0000 200
C4000 200
C8000 200
CC000 200
D4000 400
D8000 400
DC000 400
!RIE0(PORT)Base I/O Port
?Note: Other I/O Port options available.  Check board manual.
@360
300
310
320
340
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*OIE0(FRAME)Frame Type
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD


