InS_StArT
NI9210.COM
1.0
^Racal-Datacom NI9210 ODI MLID,NI9210.COM,00M,0FDF
?Driver is self-configuring.
!RIE0(INT)Hardware Interrupt
@2
3
4
5
7
$O00M(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*O00M(FRAME)Frame Type
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD


