InS_StArT
OSH89XR.COM
1.0,PRORAPM.DWN
^Proteon p189X RapiDriver,OSH89XR.COM,00M,0700
?Set cable type, ring speed and other adapter configurations using the System Reference Diskette.
!R00M(SLOT) Slot Number
?When 0 is selected, the driver scans for the p189X adapter.  It starts at slot 1 and uses the first p189X found.
@0
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS) Node Address
0
7FFFFFFFFFFF
$O00M(MAX FRAME SIZE) Maximum Frame Size
?Allows you to set the maximum frame size.  Default: 4210.
618
4096
$O00M(MAX PACKET SIZE) Maximum Packet Size
?Allows you to set the maximum packet size.  Default: 4210.
618
4202
*O00M(FRAME) Frame Type
@Token-Ring
Token-Ring_SNAP
InS_EnD
