InS_StArT
OSH990R.COM
1.0,PRORAPM.DWN
^Proteon p1990 RapiDriver,OSH990R.COM,0E0,6000
^Proteon p1990 RapiDriver,OSH990R.COM,0E0,6001
?Set cable type, ring speed and other adapter configurations using the System Reference Diskette.
!R0E0(SLOT) Slot Number
?When 0 is selected, the driver scans for the p1990 adapter.  It starts at slot 1 and uses the first p1990 found.
@0
1
2
3
4
5
6
7
8
9
10
11
12
13
14
15
$O0E0(NODE ADDRESS) Node Address
0
7FFFFFFFFFFF
$O0E0(MAX FRAME SIZE) Maximum Frame Size
?Allows you to set the maximum frame size.  Default: 4210.
618
4096
$O0E0(MAX PACKET SIZE) Maximum Packet Size
?Allows you to set the maximum packet size.  Default: 4210.
618
4202
*O0E0(FRAME) Frame Type
@Token-Ring
Token-Ring_SNAP
InS_EnD
