InS_StArT
PCN2L.COM
1.0,ROUTE.COM
^PCN II and PCN Baseband Driver,PCN2L.COM,IE0
^PCN II/A and PCN Baseband/A Driver,PCN2.COM,00M,EFEF
?You can use this driver in an ISA (AT bus), EISA, or microchannel client. You can have a maximum of two PCN II network boards in your machine.
!RIE0(PORT)Base I/O Port
@620
628
$R00M(SLOT)Slot
1
8
$OIEM(NODE ADDRESS)Optional Node Address
?Do not set this address unless you are prepared to administer local addresses according to IBM's specifications and practices for PCN II.
0
7FFFFFFFFFFF
*RIEM(FRAME)Frame Type
?Use the frame types ending in MSB unless you are familiar with the effects and side effects of the LSB suffix.
@IBM_PCN2_802.2 MSB
IBM_PCN2_SNAP MSB
IBM_PCN2_802.2 LSB
IBM_PCN2_SNAP LSB
InS_EnD
